IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "101_W_33rd_St_Balcony.ifc"
Time stamp: "2022-05-04T16:26:21+02:00"
Preprocessor: "IfcOpenShell v0.7.0-1b1fd1e6"
Originating system: "BlenderBIM 0.0.220321"
Authorization: "Nobody"

Units
  AREAUNIT: square inch (conversion based)
  PLANEANGLEUNIT: degree (conversion based)
  VOLUMEUNIT: cubic inch (conversion based)
  LENGTHUNIT: inch (conversion based)
  PLANEANGLEUNIT: degree (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "BASEMENT" | elevation -152.
        IFCSPACE "Steel Connections ALL FLOORS"
          contains 12 elements
            12 x IFCELEMENTASSEMBLY | names: "Connection BEAM-COLUMN TYPE 2", "Connection BEAM-COLUMN TYPE 1", "Connection BEAM-FACADE TYPE 1" | parts: 330 IFCMECHANICALFASTENER, 49 IFCPLATE, 45 IFCFASTENER, 1 IFCELEMENTASSEMBLY
      IFCBUILDINGSTOREY "1ST FLOOR" | elevation 0.
        contains 27 elements
          9 x IFCCOLUMN | type IFCCOLUMNTYPE "Steel Column HHS 6x6x3/8" | names: "Column" | material: profiles "Steel Column HHS 6x6x3/8" ("Steel Column HHS 6x6x3/8": "Steel Column HHS 6x6x3/8") | property sets: EPset_Parametric
          7 x IFCCOLUMN | type IFCCOLUMNTYPE "Steel Column HHS 5.5x5.5x3/8" | names: "Column" | material: profiles "Steel Column HHS 5.5x5.5x3/8" ("Steel Column HHS 5.5x5.5x3/8": "Steel Column HHS 5.5x5.5x3/8") | property sets: EPset_Parametric
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "Steel Column HHS 4x4x3/8" | names: "Column" | material: profiles "Steel Column HHS 4x4x3/8" ("Steel Column HHS 4x4x3/8": "Steel Column HHS 4x4x3/8") | property sets: EPset_Parametric
          4 x IFCELEMENTASSEMBLY | names: "Separation Wall 1", "Separation Wall 2", "Stairs 1ST_FL 1" (+1 more) | parts: 10 IFCMEMBER, 2 IFCPLATE
          6 x IFCBEAM | type IFCBEAMTYPE "Steel Beam C 15x33.9" | names: "Beam" | material: profiles "Steel Beam C 15x33.9" ("Steel Beam C 15x33.9": "Steel Beam C 15x33.9") | property sets: EPset_Parametric
        IFCSPACE "Parapet 1ST FL" | EXTERNAL
          contains 30 elements
            28 x IFCMEMBER | MEMBER | names: "Mesh_Panel", "Post_Rail", "Top_Rail" | material: "2" X 4" 6 GA GALV. MESH PANEL"; "(2) 2X4s LAGGED TOGETHER - EXT STAIN - DARK"; "CONT. TREATED 4X^ WITH ROUNDED EDGES AT TOP"
            2 x IFCELEMENTASSEMBLY | names: "Parapet_Short_Connection.001" | parts: 120 IFCMECHANICALFASTENER
      IFCBUILDINGSTOREY "2ND FLOOR" | elevation 129.625
        contains 34 elements
          27 x IFCBEAM | type IFCBEAMTYPE "Steel Beam C 15x33.9" | names: "Beam" | material: profiles "Steel Beam C 15x33.9" ("Steel Beam C 15x33.9": "Steel Beam C 15x33.9") | property sets: EPset_Parametric
          1 x IFCELEMENTASSEMBLY | SLAB_FIELD | names: "2ND_FL SLAB ASSEMBLY" | parts: 2 IFCBEAM, 1 IFCPLATE
          6 x IFCELEMENTASSEMBLY | names: "Separation Wall 3", "Separation Wall 4", "Separation Wall 5" (+3 more) | parts: 10 IFCMEMBER, 4 IFCPLATE
        IFCSPACE "Parapet 2ND FL" | EXTERNAL
          contains 163 elements
            153 x IFCMEMBER | MEMBER | names: "Mesh_Panel", "Post_Rail", "Top_Rail" | material: "2" X 4" 6 GA GALV. MESH PANEL"; "(2) 2X4s LAGGED TOGETHER - EXT STAIN - DARK"; "CONT. TREATED 4X^ WITH ROUNDED EDGES AT TOP"
            10 x IFCELEMENTASSEMBLY | names: "Parapet_Short_Connection", "Parapet_Short_Connection.001" | parts: 800 IFCMECHANICALFASTENER
      IFCBUILDINGSTOREY "3RD FLOOR" | elevation 257.625
        contains 17 elements
          16 x IFCBEAM | type IFCBEAMTYPE "Steel Beam C 15x33.9" | names: "Beam" | material: profiles "Steel Beam C 15x33.9" ("Steel Beam C 15x33.9": "Steel Beam C 15x33.9") | property sets: EPset_Parametric
          1 x IFCELEMENTASSEMBLY | SLAB_FIELD | names: "3RD_FL SLAB ASSEMBLY" | parts: 2 IFCBEAM, 1 IFCPLATE
        IFCSPACE "Parapet 3RD FL" | EXTERNAL
          contains 128 elements
            115 x IFCMEMBER | MEMBER | names: "Mesh_Panel", "Post_Rail", "Top_Rail" | material: "2" X 4" 6 GA GALV. MESH PANEL"; "(2) 2X4s LAGGED TOGETHER - EXT STAIN - DARK"; "CONT. TREATED 4X^ WITH ROUNDED EDGES AT TOP"
            13 x IFCELEMENTASSEMBLY | names: "Parapet_Short_Connection.001" | parts: 480 IFCMECHANICALFASTENER
      IFCBUILDINGSTOREY "ROOF" | elevation 365.25
        contains 15 elements
          14 x IFCBEAM | type IFCBEAMTYPE "Steel Beam C 15x33.9" | names: "Beam" | material: profiles "Steel Beam C 15x33.9" ("Steel Beam C 15x33.9": "Steel Beam C 15x33.9") | property sets: EPset_Parametric
          1 x IFCELEMENTASSEMBLY | SLAB_FIELD | names: "ROOF ASSEMBLY" | parts: 2 IFCBEAM

Types
  IFCCOLUMNTYPE "Steel Column HHS 6x6x3/8" | COLUMN | 9 occurrences | material: profiles "Steel Column HHS 6x6x3/8" ("Steel Column HHS 6x6x3/8": "Steel Column HHS 6x6x3/8")
  IFCCOLUMNTYPE "Steel Column HHS 5.5x5.5x3/8" | COLUMN | 7 occurrences | material: profiles "Steel Column HHS 5.5x5.5x3/8" ("Steel Column HHS 5.5x5.5x3/8": "Steel Column HHS 5.5x5.5x3/8")
  IFCCOLUMNTYPE "Steel Column HHS 4x4x3/8" | COLUMN | 1 occurrence | material: profiles "Steel Column HHS 4x4x3/8" ("Steel Column HHS 4x4x3/8": "Steel Column HHS 4x4x3/8")
  IFCBEAMTYPE "Steel Beam C 15x33.9" | BEAM | 63 occurrences | material: profiles "Steel Beam C 15x33.9" ("Steel Beam C 15x33.9": "Steel Beam C 15x33.9")

Property sets
  EPset_Parametric | properties | on 80 objects (63 IFCBEAM, 17 IFCCOLUMN)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)