IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Details from CTR.ifc"
Time stamp: "2022-02-15T21:25:40-06:00"
Preprocessor: "IfcOpenShell v0.7.0-4c40fc16"
Originating system: "BlenderBIM 0.0.220210"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "ryan@openingdesign.com" of Organization (no name given)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1644955341 (2022-02-15T20:02:21Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "CANNERY TRAIL RESIDENCES" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 100.
    IFCBUILDING
      IFCBUILDINGSTOREY "BASEMENT" | long name "BASEMENT" | object type "Level:Extremo inicial 8 mm" | elevation -12.6666666666667
        contains 1230 elements
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 56:Generic Models 1" | names: "Generic Models 56:Generic Models 1:1882166" | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 57:Generic Models 65" | names: "Generic Models 57:Generic Models 65:1882175" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel2:Dowel" | names: "Dowel2:Dowel:1882207" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 59:Generic Models 65" | names: "Generic Models 59:Generic Models 65:1882214" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 60:Generic Models 1" | names: "Generic Models 60:Generic Models 1:1882231" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel4:Dowel" | names: "Dowel4:Dowel:1882246" | material: "#4 J's @ 24" O.C. - GROUTED IN PRECAST KEYS AND CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 55:Generic Models 65" | names: "Generic Models 55:Generic Models 65:1882258" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 63:Generic Models 1" | names: "Generic Models 63:Generic Models 1:1882274" | material: "SOLID CMU AS NEEDED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 58:Generic Models 65" | names: "Generic Models 58:Generic Models 65:1882286" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 64:Generic Models 1" | names: "Generic Models 64:Generic Models 1:1882303" | material: "SOLID CMU AS NEEDED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 65:Generic Models 65" | names: "Generic Models 65:Generic Models 65:1882315" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 66:Generic Models 65" | names: "Generic Models 66:Generic Models 65:1882337" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 68:Generic Models 1" | names: "Generic Models 68:Generic Models 1:1882351" | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 69:Generic Models 65" | names: "Generic Models 69:Generic Models 65:1882360" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 70:Generic Models 65" | names: "Generic Models 70:Generic Models 65:1882382" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel3:Dowel" | names: "Dowel3:Dowel:1882405" | material: "#4 REBARS @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 71:Generic Models 65" | names: "Generic Models 71:Generic Models 65:1882412" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 72:Generic Models 65" | names: "Generic Models 72:Generic Models 65:1882434" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 74:Generic Models 1" | names: "Generic Models 74:Generic Models 1:1882446" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 61:Generic Models 65" | names: "Generic Models 61:Generic Models 65:1882468" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 62:Generic Models 65" | names: "Generic Models 62:Generic Models 65:1882490" | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 73:Generic Models 1" | names: "Generic Models 73:Generic Models 1:1882502" | material: "GROUT CORES AT REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 141:Generic Models 1" | names: "Generic Models 141:Generic Models 1:1882569" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 144:Generic Models 1" | names: "Generic Models 144:Generic Models 1:1882574" | material: "#10 6x6 WIRE MESH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 8:Generic Models 1" | names: "Generic Models 8:Generic Models 1:1882646" | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 125:Generic Models 1" | names: "Generic Models 125:Generic Models 1:1883788" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 1:Generic Models 1" | names: "Generic Models 1:Generic Models 1:1883911" | material: "(2) #5's" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 2:Generic Models 1" | names: "Generic Models 2:Generic Models 1:1884041" | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 3:Generic Models 1" | names: "Generic Models 3:Generic Models 1:1884162" | material: "(2) #5's" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel5:Dowel" | names: "Dowel5:Dowel:1884522" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 78:Generic Models 1" | names: "Generic Models 78:Generic Models 1:1884529" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 91:Generic Models 1" | names: "Generic Models 91:Generic Models 1:1884556" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 96:Generic Models 1" | names: "Generic Models 96:Generic Models 1:1884577" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 75:Generic Models 1" | names: "Generic Models 75:Generic Models 1:1884592" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 80:Generic Models 1" | names: "Generic Models 80:Generic Models 1:1884655" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 82:Generic Models 1" | names: "Generic Models 82:Generic Models 1:1884684" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 84:Generic Models 1" | names: "Generic Models 84:Generic Models 1:1884694" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 85:Generic Models 1" | names: "Generic Models 85:Generic Models 1:1884727" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 86:Generic Models 1" | names: "Generic Models 86:Generic Models 1:1884754" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 87:Generic Models 1" | names: "Generic Models 87:Generic Models 1:1884775" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 88:Generic Models 1" | names: "Generic Models 88:Generic Models 1:1884790" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 90:Generic Models 1" | names: "Generic Models 90:Generic Models 1:1884827" | material: "#3 VERTICAL BAR @ 18" O/C" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 95:Generic Models 1" | names: "Generic Models 95:Generic Models 1:1884853" | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 99:Generic Models 1" | names: "Generic Models 99:Generic Models 1:1884868" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 100:Generic Models 1" | names: "Generic Models 100:Generic Models 1:1884878" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 101:Generic Models 1" | names: "Generic Models 101:Generic Models 1:1884899" | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 102:Generic Models 1" | names: "Generic Models 102:Generic Models 1:1884914" | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 103:Generic Models 1" | names: "Generic Models 103:Generic Models 1:1884927" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 104:Generic Models 1" | names: "Generic Models 104:Generic Models 1:1884941" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 105:Generic Models 1" | names: "Generic Models 105:Generic Models 1:1884962" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 113:Generic Models 65" | names: "Generic Models 113:Generic Models 65:1884980" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 114:Generic Models 65" | names: "Generic Models 114:Generic Models 65:1885002" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel13:Dowel" | names: "Dowel13:Dowel:1885023" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 118:Generic Models 65" | names: "Generic Models 118:Generic Models 65:1885030" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 119:Generic Models 65" | names: "Generic Models 119:Generic Models 65:1885052" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 120:Generic Models 1" | names: "Generic Models 120:Generic Models 1:1885064" | material: "REINFORCEMENT GROUTED INTO BROKEN CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 106:Generic Models 65" | names: "Generic Models 106:Generic Models 65:1885091" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 108:Generic Models 65" | names: "Generic Models 108:Generic Models 65:1885103" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 109:Generic Models 65" | names: "Generic Models 109:Generic Models 65:1885125" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 110:Generic Models 65" | names: "Generic Models 110:Generic Models 65:1885137" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 111:Generic Models 65" | names: "Generic Models 111:Generic Models 65:1885159" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 107:Generic Models 65" | names: "Generic Models 107:Generic Models 65:1885177" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 112:Generic Models 65" | names: "Generic Models 112:Generic Models 65:1885189" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 115:Generic Models 65" | names: "Generic Models 115:Generic Models 65:1885211" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 116:Generic Models 65" | names: "Generic Models 116:Generic Models 65:1885223" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 117:Generic Models 1" | names: "Generic Models 117:Generic Models 1:1885240" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 121:Generic Models 1" | names: "Generic Models 121:Generic Models 1:1885274" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 123:Generic Models 1" | names: "Generic Models 123:Generic Models 1:1885287" | material: "#3 J's @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 4:Generic Models 1" | names: "Generic Models 4:Generic Models 1:1885309" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 5:Generic Models 1" | names: "Generic Models 5:Generic Models 1:1885333" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel1:Dowel" | names: "Dowel1:Dowel:1886872" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 6:Generic Models 1" | names: "Generic Models 6:Generic Models 1:1888587" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 7:Generic Models 1" | names: "Generic Models 7:Generic Models 1:1888850" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 13:Generic Models 1" | names: "Generic Models 13:Generic Models 1:1889006" | material: "6" CONCRETE SLAB (2% SLOPE AWAY FROM BUILDING IF NO SLOPE CALLED OUT)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 14:Generic Models 1" | names: "Generic Models 14:Generic Models 1:1889831" | material: "#4 REBARS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 16:Generic Models 1" | names: "Generic Models 16:Generic Models 1:1890075" | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 18:Generic Models 1" | names: "Generic Models 18:Generic Models 1:1890179" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 23:Generic Models 1" | names: "Generic Models 23:Generic Models 1:1890241" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 24:Generic Models 1" | names: "Generic Models 24:Generic Models 1:1890254" | material: "CONCRETE STAIRS - 6 MIN. THICKNESS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 25:Generic Models 1" | names: "Generic Models 25:Generic Models 1:1890271" | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 29:Generic Models 1" | names: "Generic Models 29:Generic Models 1:1890333" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel11:Dowel" | names: "Dowel11:Dowel:1890355" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 30:Generic Models 1" | names: "Generic Models 30:Generic Models 1:1891592" | material: "SEE ARCH. DWG FOR ASSEMBLY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 31:Generic Models 1" | names: "Generic Models 31:Generic Models 1:1891739" | material: "#4 J's @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 27:Generic Models 1" | names: "Generic Models 27:Generic Models 1:1891932" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 32:Generic Models 1" | names: "Generic Models 32:Generic Models 1:1891942" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 33:Generic Models 1" | names: "Generic Models 33:Generic Models 1:1891952" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 34:Generic Models 1" | names: "Generic Models 34:Generic Models 1:1891962" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 26:Generic Models 1" | names: "Generic Models 26:Generic Models 1:1892352" | material: "GALV. PIPE STAIR RAILING SLEEVE OR BOLTED TO SIDE OF CONCRETE STRINGER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 36:Generic Models 1" | names: "Generic Models 36:Generic Models 1:1892706" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 19:Generic Models 1" | names: "Generic Models 19:Generic Models 1:1895067" | material: "(4) #3" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 37:Generic Models 1" | names: "Generic Models 37:Generic Models 1:1895113" | material: "2# @ 8" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 9:Generic Models 1" | names: "Generic Models 9:Generic Models 1:1895448" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 10:Generic Models 1" | names: "Generic Models 10:Generic Models 1:1895632" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 11:Generic Models 1" | names: "Generic Models 11:Generic Models 1:1895741" | material: "CONSTRUCTION JOINT, ROUGHEN, CLEANED AND MOISTENED BEFORE SLAB POUR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 12:Generic Models 1" | names: "Generic Models 12:Generic Models 1:1895853" | material: "CONSTRUCTION JOINT, ROUGHEN, CLEANED AND MOISTENED BEFORE SLAB POUR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel12:Dowel" | names: "Dowel12:Dowel:1935212" | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 15:Generic Models 1" | names: "Generic Models 15:Generic Models 1:1935245" | material: "#3 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 20:Generic Models 1" | names: "Generic Models 20:Generic Models 1:1935631" | material: "#3 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel7:Dowel" | names: "Dowel7:Dowel:1936062" | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 21:Generic Models 1" | names: "Generic Models 21:Generic Models 1:1936090" | material: "#3 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 22:Generic Models 1" | names: "Generic Models 22:Generic Models 1:1936117" | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 38:Generic Models 1" | names: "Generic Models 38:Generic Models 1:1936174" | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 39:Generic Models 1" | names: "Generic Models 39:Generic Models 1:1936184" | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 40:Generic Models 1" | names: "Generic Models 40:Generic Models 1:1938978" | material: "#3 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 41:Generic Models 1" | names: "Generic Models 41:Generic Models 1:1939477" | material: "#3 VERTICAL BAR @ 18" O/C" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 17:Generic Models 1" | names: "Generic Models 17:Generic Models 1:1939912" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 44:Generic Models 1" | names: "Generic Models 44:Generic Models 1:1939925" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 76:Generic Models 1" | names: "Generic Models 76:Generic Models 1:1939935" | material: "6" CONCRETE SLAB (2% SLOPE AWAY FROM BUILDING IF NO SLOPE CALLED OUT)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 77:Generic Models 1" | names: "Generic Models 77:Generic Models 1:1939951" | material: "#4 REBARS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 79:Generic Models 1" | names: "Generic Models 79:Generic Models 1:1939964" | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 81:Generic Models 1" | names: "Generic Models 81:Generic Models 1:1939975" | material: "(4) #3" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 89:Generic Models 1" | names: "Generic Models 89:Generic Models 1:1939989" | material: "2# @ 8" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 92:Generic Models 1" | names: "Generic Models 92:Generic Models 1:1940033" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 124:Generic Models 1" | names: "Generic Models 124:Generic Models 1:1940063" | material: "CONSTRUCTION JOINT, ROUGHEN, CLEANED AND MOISTENED BEFORE SLAB POUR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 126:Generic Models 1" | names: "Generic Models 126:Generic Models 1:1940178" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel6:Dowel" | names: "Dowel6:Dowel:1940224" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 127:Generic Models 1" | names: "Generic Models 127:Generic Models 1:1940231" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 128:Generic Models 1" | names: "Generic Models 128:Generic Models 1:1940244" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 129:Generic Models 1" | names: "Generic Models 129:Generic Models 1:1940307" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel10:Dowel" | names: "Dowel10:Dowel:1940379" | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 130:Generic Models 1" | names: "Generic Models 130:Generic Models 1:1940414" | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 131:Generic Models 1" | names: "Generic Models 131:Generic Models 1:1940445" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 132:Generic Models 1" | names: "Generic Models 132:Generic Models 1:1940797" | material: "GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 133:Generic Models 1" | names: "Generic Models 133:Generic Models 1:1940899" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 134:Generic Models 1" | names: "Generic Models 134:Generic Models 1:1941038" | material: "2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 135:Generic Models 1" | names: "Generic Models 135:Generic Models 1:1941075" | material: "2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 136:Generic Models 1" | names: "Generic Models 136:Generic Models 1:1941131" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 137:Generic Models 1" | names: "Generic Models 137:Generic Models 1:1941416" | material: "FLOOR FINISH T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 138:Generic Models 1" | names: "Generic Models 138:Generic Models 1:1941502" | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 140:Generic Models 1" | names: "Generic Models 140:Generic Models 1:1941860" | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 142:Generic Models 1" | names: "Generic Models 142:Generic Models 1:1943155" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 143:Generic Models 1" | names: "Generic Models 143:Generic Models 1:1943436" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 145:Generic Models 1" | names: "Generic Models 145:Generic Models 1:1944441" | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 146:Generic Models 1" | names: "Generic Models 146:Generic Models 1:1944470" | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 148:Generic Models 1" | names: "Generic Models 148:Generic Models 1:1944597" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 152:Generic Models 1" | names: "Generic Models 152:Generic Models 1:1945498" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 155:Generic Models 1" | names: "Generic Models 155:Generic Models 1:1945713" | material: "MENDING PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 156:Generic Models 1" | names: "Generic Models 156:Generic Models 1:1946023" | material: "MENDING PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 157:Generic Models 1" | names: "Generic Models 157:Generic Models 1:1946086" | material: "MENDING PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 153:Generic Models 1" | names: "Generic Models 153:Generic Models 1:1947642" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 161:Generic Models 1" | names: "Generic Models 161:Generic Models 1:1947695" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel14:Dowel" | names: "Dowel14:Dowel:1947715" | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 163:Generic Models 1" | names: "Generic Models 163:Generic Models 1:1947735" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 164:Generic Models 1" | names: "Generic Models 164:Generic Models 1:1947748" | material: "GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 166:Generic Models 1" | names: "Generic Models 166:Generic Models 1:1947774" | material: "TREATED 2X LEDGER - SIZE T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 169:Generic Models 1" | names: "Generic Models 169:Generic Models 1:1947813" | material: "FLOOR FINISH T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 170:Generic Models 1" | names: "Generic Models 170:Generic Models 1:1947826" | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 171:Generic Models 1" | names: "Generic Models 171:Generic Models 1:1947839" | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 172:Generic Models 1" | names: "Generic Models 172:Generic Models 1:1947861" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 173:Generic Models 1" | names: "Generic Models 173:Generic Models 1:1947878" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 174:Generic Models 1" | names: "Generic Models 174:Generic Models 1:1947901" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 175:Generic Models 1" | names: "Generic Models 175:Generic Models 1:1947923" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel9:Dowel" | names: "Dowel9:Dowel:1948720" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 154:Generic Models 1" | names: "Generic Models 154:Generic Models 1:1948763" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 160:Generic Models 1" | names: "Generic Models 160:Generic Models 1:1948781" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 162:Generic Models 1" | names: "Generic Models 162:Generic Models 1:1948962" | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 167:Generic Models 1" | names: "Generic Models 167:Generic Models 1:1949123" | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 215:Generic Models 1" | names: "Generic Models 215:Generic Models 1:1949294" | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 216:Generic Models 1" | names: "Generic Models 216:Generic Models 1:1949580" | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 217:Generic Models 1" | names: "Generic Models 217:Generic Models 1:1949593" | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 218:Generic Models 1" | names: "Generic Models 218:Generic Models 1:1949610" | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 181:Generic Models 1" | names: "Generic Models 181:Generic Models 1:1949726" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 183:Generic Models 1" | names: "Generic Models 183:Generic Models 1:1949788" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 177:Generic Models 1" | names: "Generic Models 177:Generic Models 1:1949908" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 178:Generic Models 1" | names: "Generic Models 178:Generic Models 1:1949921" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 179:Generic Models 1" | names: "Generic Models 179:Generic Models 1:1949934" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 165:Generic Models 1" | names: "Generic Models 165:Generic Models 1:1950350" | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 168:Generic Models 1" | names: "Generic Models 168:Generic Models 1:1950388" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 180:Generic Models 1" | names: "Generic Models 180:Generic Models 1:1951052" | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 147:Generic Models 1" | names: "Generic Models 147:Generic Models 1:1951830" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 149:Generic Models 1" | names: "Generic Models 149:Generic Models 1:1952230" | material: "NON-BEARING 2X FURRING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 184:Generic Models 1" | names: "Generic Models 184:Generic Models 1:1952243" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 185:Generic Models 1" | names: "Generic Models 185:Generic Models 1:1952256" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 176:Generic Models 1" | names: "Generic Models 176:Generic Models 1:1952821" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 182:Generic Models 1" | names: "Generic Models 182:Generic Models 1:1952834" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 150:Generic Models 1" | names: "Generic Models 150:Generic Models 1:1952855" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 151:Generic Models 1" | names: "Generic Models 151:Generic Models 1:1952868" | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 158:Generic Models 1" | names: "Generic Models 158:Generic Models 1:1953074" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 159:Generic Models 1" | names: "Generic Models 159:Generic Models 1:1953087" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 186:Generic Models 1" | names: "Generic Models 186:Generic Models 1:1953098" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 189:Generic Models 1" | names: "Generic Models 189:Generic Models 1:1953113" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 192:Generic Models 1" | names: "Generic Models 192:Generic Models 1:1953151" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 193:Generic Models 1" | names: "Generic Models 193:Generic Models 1:1953161" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 194:Generic Models 1" | names: "Generic Models 194:Generic Models 1:1953181" | material: "WOOD FRAMING BEARING WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 195:Generic Models 1" | names: "Generic Models 195:Generic Models 1:1953194" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 196:Generic Models 1" | names: "Generic Models 196:Generic Models 1:1953212" | material: "#4 CLOSED STIRRRUPS @ 8" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel15:Dowel" | names: "Dowel15:Dowel:1953242" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel16:Dowel" | names: "Dowel16:Dowel:1953271" | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 201:Generic Models 1" | names: "Generic Models 201:Generic Models 1:1954442" | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 203:Generic Models 1" | names: "Generic Models 203:Generic Models 1:1954645" | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 199:Generic Models 1" | names: "Generic Models 199:Generic Models 1:1954968" | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 200:Generic Models 1" | names: "Generic Models 200:Generic Models 1:1955015" | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 204:Generic Models 1" | names: "Generic Models 204:Generic Models 1:1955035" | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 191:Generic Models 1" | names: "Generic Models 191:Generic Models 1:1955081" | material: "WALL REINFORCEMENT STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 207:Generic Models 1" | names: "Generic Models 207:Generic Models 1:1955840" | material: "WALL REINFORCEMENT STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 190:Generic Models 1" | names: "Generic Models 190:Generic Models 1:1955888" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 208:Generic Models 1" | names: "Generic Models 208:Generic Models 1:1955898" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 209:Generic Models 1" | names: "Generic Models 209:Generic Models 1:1956054" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 210:Generic Models 1" | names: "Generic Models 210:Generic Models 1:1956084" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 212:Generic Models 1" | names: "Generic Models 212:Generic Models 1:1956173" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 213:Generic Models 1" | names: "Generic Models 213:Generic Models 1:1956183" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 214:Generic Models 1" | names: "Generic Models 214:Generic Models 1:1956193" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 219:Generic Models 1" | names: "Generic Models 219:Generic Models 1:1956203" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 220:Generic Models 1" | names: "Generic Models 220:Generic Models 1:1956261" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 221:Generic Models 1" | names: "Generic Models 221:Generic Models 1:1956271" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 198:Generic Models 1" | names: "Generic Models 198:Generic Models 1:1956380" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 197:Generic Models 1" | names: "Generic Models 197:Generic Models 1:1957906" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 202:Generic Models 1" | names: "Generic Models 202:Generic Models 1:1957919" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 206:Generic Models 1" | names: "Generic Models 206:Generic Models 1:1957944" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 223:Generic Models 1" | names: "Generic Models 223:Generic Models 1:1957978" | material: "WOOD FRAMING BEARING WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 224:Generic Models 1" | names: "Generic Models 224:Generic Models 1:1957991" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel17:Dowel" | names: "Dowel17:Dowel:1958030" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel18:Dowel" | names: "Dowel18:Dowel:1958044" | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 232:Generic Models 1" | names: "Generic Models 232:Generic Models 1:1958127" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 237:Generic Models 1" | names: "Generic Models 237:Generic Models 1:1958181" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 238:Generic Models 1" | names: "Generic Models 238:Generic Models 1:1958191" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 239:Generic Models 1" | names: "Generic Models 239:Generic Models 1:1958201" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 240:Generic Models 1" | names: "Generic Models 240:Generic Models 1:1958211" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 241:Generic Models 1" | names: "Generic Models 241:Generic Models 1:1958223" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 242:Generic Models 1" | names: "Generic Models 242:Generic Models 1:1958233" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 243:Generic Models 1" | names: "Generic Models 243:Generic Models 1:1958244" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 244:Generic Models 1" | names: "Generic Models 244:Generic Models 1:1958290" | material: "CONC. FOOTER - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 247:Generic Models 1" | names: "Generic Models 247:Generic Models 1:1958340" | material: "#3@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 248:Generic Models 1" | names: "Generic Models 248:Generic Models 1:1958351" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 249:Generic Models 1" | names: "Generic Models 249:Generic Models 1:1958372" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 250:Generic Models 1" | names: "Generic Models 250:Generic Models 1:1958398" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 251:Generic Models 1" | names: "Generic Models 251:Generic Models 1:1958410" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 252:Generic Models 1" | names: "Generic Models 252:Generic Models 1:1958422" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 253:Generic Models 1" | names: "Generic Models 253:Generic Models 1:1958440" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 254:Generic Models 1" | names: "Generic Models 254:Generic Models 1:1958452" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 255:Generic Models 1" | names: "Generic Models 255:Generic Models 1:1958464" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 256:Generic Models 1" | names: "Generic Models 256:Generic Models 1:1958476" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 257:Generic Models 1" | names: "Generic Models 257:Generic Models 1:1958493" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 258:Generic Models 1" | names: "Generic Models 258:Generic Models 1:1958508" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 259:Generic Models 1" | names: "Generic Models 259:Generic Models 1:1958520" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 263:Generic Models 1" | names: "Generic Models 263:Generic Models 1:1958807" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 205:Generic Models 1" | names: "Generic Models 205:Generic Models 1:1958939" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 233:Generic Models 1" | names: "Generic Models 233:Generic Models 1:1958988" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 234:Generic Models 1" | names: "Generic Models 234:Generic Models 1:1958998" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 235:Generic Models 1" | names: "Generic Models 235:Generic Models 1:1959008" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 236:Generic Models 1" | names: "Generic Models 236:Generic Models 1:1959018" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 264:Generic Models 1" | names: "Generic Models 264:Generic Models 1:1959220" | material: "#4@8"O.C. VERTICAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 265:Generic Models 1" | names: "Generic Models 265:Generic Models 1:1959237" | material: "#4@8"O.C. VERTICAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 228:Generic Models 1" | names: "Generic Models 228:Generic Models 1:1960300" | material: "(2) #4x60" @ 8" O.C. - VERTICAL STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 226:Generic Models 1" | names: "Generic Models 226:Generic Models 1:1960733" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 229:Generic Models 1" | names: "Generic Models 229:Generic Models 1:1960775" | material: "#4@8"O.C. STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 231:Generic Models 1" | names: "Generic Models 231:Generic Models 1:1961064" | material: "#4@8"O.C. STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 246:Generic Models 1" | names: "Generic Models 246:Generic Models 1:1961955" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 260:Generic Models 1" | names: "Generic Models 260:Generic Models 1:1961967" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 261:Generic Models 1" | names: "Generic Models 261:Generic Models 1:1961979" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 305:Generic Models 1" | names: "Generic Models 305:Generic Models 1:1962108" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 262:Generic Models 1" | names: "Generic Models 262:Generic Models 1:1962205" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 266:Generic Models 1" | names: "Generic Models 266:Generic Models 1:1962284" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 270:Generic Models 1" | names: "Generic Models 270:Generic Models 1:1962320" | material: "#5" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 274:Generic Models 1" | names: "Generic Models 274:Generic Models 1:1963612" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 275:Generic Models 1" | names: "Generic Models 275:Generic Models 1:1963623" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 276:Generic Models 1" | names: "Generic Models 276:Generic Models 1:1963637" | material: "WOOD FRAMING BEARING WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 277:Generic Models 1" | names: "Generic Models 277:Generic Models 1:1963650" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 285:Generic Models 1" | names: "Generic Models 285:Generic Models 1:1963766" | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel19:Dowel" | names: "Dowel19:Dowel:1964211" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 299:Generic Models 1" | names: "Generic Models 299:Generic Models 1:1964342" | material: "(2) #4x60" @ 8" O.C. - VERTICAL STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 301:Generic Models 1" | names: "Generic Models 301:Generic Models 1:1964668" | material: "(3)#5" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 302:Generic Models 1" | names: "Generic Models 302:Generic Models 1:1965404" | material: "(2)#4" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 211:Generic Models 1" | names: "Generic Models 211:Generic Models 1:1965515" | material: "#4@8"O.C. HORIZONTAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 303:Generic Models 1" | names: "Generic Models 303:Generic Models 1:1965525" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 273:Generic Models 1" | names: "Generic Models 273:Generic Models 1:1977737" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 278:Generic Models 1" | names: "Generic Models 278:Generic Models 1:1977750" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 279:Generic Models 1" | names: "Generic Models 279:Generic Models 1:1977762" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 280:Generic Models 1" | names: "Generic Models 280:Generic Models 1:1977772" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 281:Generic Models 1" | names: "Generic Models 281:Generic Models 1:1977782" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 282:Generic Models 1" | names: "Generic Models 282:Generic Models 1:1977792" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 283:Generic Models 1" | names: "Generic Models 283:Generic Models 1:1977803" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 284:Generic Models 1" | names: "Generic Models 284:Generic Models 1:1977813" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 286:Generic Models 1" | names: "Generic Models 286:Generic Models 1:1977824" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 287:Generic Models 1" | names: "Generic Models 287:Generic Models 1:1977839" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 288:Generic Models 1" | names: "Generic Models 288:Generic Models 1:1977851" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 289:Generic Models 1" | names: "Generic Models 289:Generic Models 1:1977861" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 290:Generic Models 1" | names: "Generic Models 290:Generic Models 1:1977871" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 291:Generic Models 1" | names: "Generic Models 291:Generic Models 1:1977881" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 292:Generic Models 1" | names: "Generic Models 292:Generic Models 1:1977892" | material: "#4@8"O.C. VERTICAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 293:Generic Models 1" | names: "Generic Models 293:Generic Models 1:1977906" | material: "#4@8"O.C. VERTICAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 295:Generic Models 1" | names: "Generic Models 295:Generic Models 1:1977935" | material: "(2) #4x60" @ 8" O.C. - VERTICAL STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 296:Generic Models 1" | names: "Generic Models 296:Generic Models 1:1977949" | material: "(2) #4x60" @ 8" O.C. - VERTICAL STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 297:Generic Models 1" | names: "Generic Models 297:Generic Models 1:1977972" | material: "(2)#4" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 298:Generic Models 1" | names: "Generic Models 298:Generic Models 1:1977982" | material: "#4@8"O.C. HORIZONTAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 300:Generic Models 1" | names: "Generic Models 300:Generic Models 1:1977992" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel20:Dowel" | names: "Dowel20:Dowel:1978066" | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel21:Dowel" | names: "Dowel21:Dowel:1985673" | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel23:Dowel" | names: "Dowel23:Dowel:1985704" | material: "HSS 5X5X1/2 STEEL COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel24:Dowel" | names: "Dowel24:Dowel:1985718" | material: "1/4" STIFFENER PLATE EACH SIDE @ COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel25:Dowel" | names: "Dowel25:Dowel:1985758" | material: "HSS 5X5X1/2 STEEL COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 308:Generic Models 1" | names: "Generic Models 308:Generic Models 1:1985800" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 310:Generic Models 1" | names: "Generic Models 310:Generic Models 1:1985814" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 311:Generic Models 1" | names: "Generic Models 311:Generic Models 1:1985828" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 336:Generic Models 1" | names: "Generic Models 336:Generic Models 1:1985863" | material: "2" GROUT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "one" | object type "Nut:one" | names: "Nut:one:1985872", "Nut:one:1985877" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1"" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1"" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1":1985875", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1":1985879" | material: "5/8" GALV. ANCHOR BOLT (11" MIN. EMBED)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "one" | object type "Nut:one" | names: "Nut:one:1985882", "Nut:one:1985886" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1"" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1"" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1":1985884", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1":1985888" | material: "5/8" GALV. ANCHOR BOLT (11" MIN. EMBED)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 337:Generic Models 1" | names: "Generic Models 337:Generic Models 1:1985895" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          8 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1" 2" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 2" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 2:1985913", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 2:1985930", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 2:1985932" (+5 more) | material: "ANCHOR BOLT PER ANCHOR TYPE IN HOLD DOWN SCHEDULE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 309:Generic Models 1" | names: "Generic Models 309:Generic Models 1:1985949" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 340:Generic Models 1" | names: "Generic Models 340:Generic Models 1:1985963" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal Fastenings - Base Plate - 11inX11inX3_4in" | object type "050523 - Metal Fastenings - Base Plate - 12inX12inX3_4in:050523 - Metal Fastenings - Base Plate - 11inX11inX3_4in" | names: "050523 - Metal Fastenings - Base Plate - 12inX12inX3_4in:050523 - Metal Fastenings - Base Plate - 11inX11inX3_4in:1991065" | material: "11"X11"X3/4" BASE PLATE W(4) 3/4" DIA. A325 BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal Fastenings - Base Plate - 11inX8inX3_4in 2" | object type "050523 - Metal Fastenings - Base Plate - 12inX12inX3_4in:050523 - Metal Fastenings - Base Plate - 11inX8inX3_4in 2" | names: "050523 - Metal Fastenings - Base Plate - 12inX12inX3_4in:050523 - Metal Fastenings - Base Plate - 11inX8inX3_4in 2:1991530" | material: "3/4"X8"X11" TOP BEARING PLATE W(4) 3/4" DIA. A325 BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel22:Dowel" | names: "Dowel22:Dowel:1993380" | material: "W14X30 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 312:Generic Models 1" | names: "Generic Models 312:Generic Models 1:1993433" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal Fastener - Vertical Plate - 8inX20inX1_2in" | object type "050523 - Metal Fastener - Vertical Plate - 10inX20inX1_2in:050523 - Metal Fastener - Vertical Plate - 8inX20inX1_2in" | names: "050523 - Metal Fastener - Vertical Plate - 10inX20inX1_2in:050523 - Metal Fastener - Vertical Plate - 8inX20inX1_2in:1993471" | material: "1/2"X10"X20" W/(16) 3/4" DIA. X4" H.S." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          7 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable" | object type "051200 - Metal Fastener - Vertical Angle Weld Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable" | names: "051200 - Metal Fastener - Vertical Angle Weld Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable:1996866", "051200 - Metal Fastener - Vertical Angle Weld Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable:1998990", "051200 - Metal Fastener - Vertical Angle Weld Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable:1999024" (+4 more) | material: "3"X3"X1/4" STEEL ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable" | object type "051200 - Metal Fastener - Vertical Angle Weld Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable" | names: "051200 - Metal Fastener - Vertical Angle Weld Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable:1998727", "051200 - Metal Fastener - Vertical Angle Weld Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable:2001427", "051200 - Metal Fastener - Vertical Angle Weld Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable:2006085" | material: "3"X3"X1/4" STEEL ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in" | object type "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in" | names: "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:2000131", "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:2001432", "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:2006090" | material: "1/4"X1/4"X8 1/2" FILLET WELD @ EACH SIDE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in" | object type "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in" | names: "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:2000319", "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:2001435", "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:2003145" (+2 more) | material: "1/4"X1/4"X8 1/2" FILLET WELD @ EACH SIDE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel26:Dowel" | names: "Dowel26:Dowel:2001396" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle - Bolting Plate - 1/2"X3"X8 1/2"" | object type "051200 - Metal Fastener - Vertical Angle - Bolting Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle - Bolting Plate - 1/2"X3"X8 1/2"" | names: "051200 - Metal Fastener - Vertical Angle - Bolting Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle - Bolting Plate - 1/2"X3"X8 1/2":2001428", "051200 - Metal Fastener - Vertical Angle - Bolting Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle - Bolting Plate - 1/2"X3"X8 1/2":2001430", "051200 - Metal Fastener - Vertical Angle - Bolting Plate - LxWxH=Variable:051200 - Metal Fastener - Vertical Angle - Bolting Plate - 1/2"X3"X8 1/2":2004185" (+3 more) | material: "3"X3"X1/4" STEEL ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 313:Generic Models 1" | names: "Generic Models 313:Generic Models 1:2001566" | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel28:Dowel" | names: "Dowel28:Dowel:2002047" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 317:Generic Models 1" | names: "Generic Models 317:Generic Models 1:2002523" | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 315:Generic Models 1" | names: "Generic Models 315:Generic Models 1:2002673" | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 316:Generic Models 1" | names: "Generic Models 316:Generic Models 1:2002794" | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1"" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1"" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1":2004524", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1":2004688", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1":2004708" (+3 more) | material: "5/8" GALV. ANCHOR BOLT (11" MIN. EMBED)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1" 4" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2004854", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005051", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005062" | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1" 4" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005034", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005053", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005064" | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          12 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1" 4" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005271", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005530", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005541" (+9 more) | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1" 4" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005619", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005733", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 4:2005742" (+3 more) | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 318:Generic Models 1" | names: "Generic Models 318:Generic Models 1:2005780" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 319:Generic Models 1" | names: "Generic Models 319:Generic Models 1:2005985" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 320:Generic Models 1" | names: "Generic Models 320:Generic Models 1:2006005" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel27:Dowel" | names: "Dowel27:Dowel:2006081" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 321:Generic Models 1" | names: "Generic Models 321:Generic Models 1:2006099" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel29:Dowel" | names: "Dowel29:Dowel:2006128" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 322:Generic Models 1" | names: "Generic Models 322:Generic Models 1:2006135" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 323:Generic Models 1" | names: "Generic Models 323:Generic Models 1:2006154" | material: "W14X30 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 324:Generic Models 1" | names: "Generic Models 324:Generic Models 1:2006167" | material: "W14X30 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 325:Generic Models 1" | names: "Generic Models 325:Generic Models 1:2006207" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 326:Generic Models 1" | names: "Generic Models 326:Generic Models 1:2006221" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 327:Generic Models 1" | names: "Generic Models 327:Generic Models 1:2006235" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel30:Dowel" | names: "Dowel30:Dowel:2015018" | material: "PRECAST BEAM BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel31:Dowel" | names: "Dowel31:Dowel:2015916" | material: "L3X2X3/8 STEEL ANGLE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel32:Dowel" | names: "Dowel32:Dowel:2016317" | material: "CONT. 3/8"X4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel33:Dowel" | names: "Dowel33:Dowel:2016402" | material: "EMBEDDED STEEL PLATE BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 328:Generic Models 1" | names: "Generic Models 328:Generic Models 1:2016554" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 329:Generic Models 65" | names: "Generic Models 329:Generic Models 65:2016564" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 330:Generic Models 65" | names: "Generic Models 330:Generic Models 65:2016586" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel34:Dowel" | names: "Dowel34:Dowel:2016607" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 331:Generic Models 65" | names: "Generic Models 331:Generic Models 65:2016614" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 333:Generic Models 65" | names: "Generic Models 333:Generic Models 65:2016653" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 334:Generic Models 65" | names: "Generic Models 334:Generic Models 65:2016665" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 335:Generic Models 65" | names: "Generic Models 335:Generic Models 65:2016687" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 342:Generic Models 65" | names: "Generic Models 342:Generic Models 65:2016739" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 343:Generic Models 65" | names: "Generic Models 343:Generic Models 65:2016751" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 344:Generic Models 65" | names: "Generic Models 344:Generic Models 65:2016773" | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 345:Generic Models 65" | names: "Generic Models 345:Generic Models 65:2016785" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 332:Generic Models 1" | names: "Generic Models 332:Generic Models 1:2016877" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 338:Generic Models 1" | names: "Generic Models 338:Generic Models 1:2016896" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 341:Generic Models 1" | names: "Generic Models 341:Generic Models 1:2016915" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 346:Generic Models 1" | names: "Generic Models 346:Generic Models 1:2016934" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX" | object type "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX" | names: "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX:2018066", "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX:2018154", "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX:2038307" | material: "1/4" FILLET WELD EACH SIDE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX" | object type "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX" | names: "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in:051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX:2018133" | material: "1/4" FILLET WELD EACH SIDE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          3 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1" 5" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt without Nut:1" 5" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt without Nut:1" 5:2018223", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt without Nut:1" 5:2018307", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt without Nut:1" 5:2018324" | material: "5/8"@16" O.C. POST INSTALLED ANCHOR - 4 1/2" MIN EMBED" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 347:Generic Models 1" | names: "Generic Models 347:Generic Models 1:2020720" | material: "(2)#4 LONG REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 348:Generic Models 1" | names: "Generic Models 348:Generic Models 1:2020751" | material: "(2)#4 LONG REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 350:Generic Models 1" | names: "Generic Models 350:Generic Models 1:2020882" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 351:Generic Models 1" | names: "Generic Models 351:Generic Models 1:2020896" | material: "#2@8" O.C. CLOSED STIRRUPS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 352:Generic Models 1" | names: "Generic Models 352:Generic Models 1:2021259" | material: "(4)#4 VERTICAL REINFORCEMENT - INSIDE STIRRUPS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 353:Generic Models 1" | names: "Generic Models 353:Generic Models 1:2022156" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 354:Generic Models 1" | names: "Generic Models 354:Generic Models 1:2022954" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 357:Generic Models 1" | names: "Generic Models 357:Generic Models 1:2023602" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 349:Generic Models 1" | names: "Generic Models 349:Generic Models 1:2024697" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 365:Generic Models 1" | names: "Generic Models 365:Generic Models 1:2025048" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 367:Generic Models 1" | names: "Generic Models 367:Generic Models 1:2027860" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 359:Generic Models 1" | names: "Generic Models 359:Generic Models 1:2029638" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 360:Generic Models 1" | names: "Generic Models 360:Generic Models 1:2029912" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 355:Generic Models 1" | names: "Generic Models 355:Generic Models 1:2030025" | material: "POST-INSTALLED REBAR WITH ANCHORING EPOXY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 356:Generic Models 1" | names: "Generic Models 356:Generic Models 1:2030652" | material: "CONC. FOOTER - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 361:Generic Models 1" | names: "Generic Models 361:Generic Models 1:2030748" | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 362:Generic Models 1" | names: "Generic Models 362:Generic Models 1:2030765" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 364:Generic Models 1" | names: "Generic Models 364:Generic Models 1:2030800" | material: "POST-INSTALLED REBAR WITH ANCHORING EPOXY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 358:Generic Models 1" | names: "Generic Models 358:Generic Models 1:2036827" | material: "RC WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel35:Dowel" | names: "Dowel35:Dowel:2037203" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 363:Generic Models 1" | names: "Generic Models 363:Generic Models 1:2037260" | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "3/4" x 1' 3"" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:3/4" x 1' 3"" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:3/4" x 1' 3":2037691" | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel36:Dowel" | names: "Dowel36:Dowel:2038663" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 366:Generic Models 1" | names: "Generic Models 366:Generic Models 1:2039125" | material: "RC WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 370:Generic Models 1" | names: "Generic Models 370:Generic Models 1:2039914" | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 369:Generic Models 1" | names: "Generic Models 369:Generic Models 1:2040070" | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          4 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1" 7" | object type "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 7" | names: "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 7:2040200", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 7:2040424", "050523 - W_P_C - Fastenings - Lag Bolt or Thru Bolt:1" 7:2041466" (+1 more) | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel37:Dowel" | names: "Dowel37:Dowel:2041067" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel38:Dowel" | names: "Dowel38:Dowel:2041420" | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 371:Generic Models 1" | names: "Generic Models 371:Generic Models 1:2041427" | material: "RC WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 372:Generic Models 1" | names: "Generic Models 372:Generic Models 1:2041442" | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 373:Generic Models 1" | names: "Generic Models 373:Generic Models 1:2041456" | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel39:Dowel" | names: "Dowel39:Dowel:2041483" | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel41:Dowel" | names: "Dowel41:Dowel:2041798" | material: "HSS 5X5X1/2 STEEL COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel42:Dowel" | names: "Dowel42:Dowel:2041812" | material: "1/4" STIFFENER PLATE EACH SIDE @ COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 374:Generic Models 1" | names: "Generic Models 374:Generic Models 1:2041857" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 375:Generic Models 1" | names: "Generic Models 375:Generic Models 1:2041871" | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal Fastenings - Base Plate - 11inX8inX3_4in" | object type "050523 - Metal Fastenings - Base Plate - 12inX12inX3_4in:050523 - Metal Fastenings - Base Plate - 11inX8inX3_4in" | names: "050523 - Metal Fastenings - Base Plate - 12inX12inX3_4in:050523 - Metal Fastenings - Base Plate - 11inX8inX3_4in:2041881" | material: "12"X12"X3/4" BASE PLATE W(4) 3/4" DIA. A325 BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 378:Generic Models 1" | names: "Generic Models 378:Generic Models 1:2056250" | material: "RC WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel43:Dowel" | names: "Dowel43:Dowel:2056270" | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "1ST - FLOOR" | long name "1ST - FLOOR" | object type "Level:Extremo inicial 8 mm" | elevation 0.
        contains 15 elements
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 139:Generic Models 1" | names: "Generic Models 139:Generic Models 1:1882559" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 35:Generic Models 1" | names: "Generic Models 35:Generic Models 1:1892541" | material: "GALV. PIPE STAIR RAILING SLEEVE OR BOLTED TO SIDE OF CONCRETE STRINGER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 197:Generic Models 1" | names: "Generic Models 197:Generic Models 1:2271127" | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 157:Generic Models 1" | names: "Generic Models 157:Generic Models 1:2271216" | material: "(S) SOUND BATT. INSULATION (THICKNESS TO MATCH WALL DEPTH)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 979:Generic Models 1" | names: "Generic Models 979:Generic Models 1:2668039" | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "(2) FASTENER AT 1X6 DECKING" | object type "060523 - W_P_C - Fastenings - Generic - Lag Bolt or Thru Bolt:(2) FASTENER AT 1X6 DECKING" | names: "060523 - W_P_C - Fastenings - Generic - Lag Bolt or Thru Bolt:(2) FASTENER AT 1X6 DECKING:2670649", "060523 - W_P_C - Fastenings - Generic - Lag Bolt or Thru Bolt:(2) FASTENER AT 1X6 DECKING:2684559", "060523 - W_P_C - Fastenings - Generic - Lag Bolt or Thru Bolt:(2) FASTENER AT 1X6 DECKING:2685648" (+3 more) | material: "(2) WEATHER RESISTANT SCREWS AT EACH BOARD (MATCH EXISTING)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 1011:Generic Models 1" | names: "Generic Models 1011:Generic Models 1:2684526" | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 1036:Generic Models 1" | names: "Generic Models 1036:Generic Models 1:2685565" | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 1037:Generic Models 1" | names: "Generic Models 1037:Generic Models 1:2685579" | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 1023:Generic Models 1" | names: "Generic Models 1023:Generic Models 1:2752149" | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "2ND FLOOR" | long name "2ND FLOOR" | object type "Level:Extremo inicial 8 mm" | elevation 11.2604166666667
        contains 21 elements
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 42:Generic Models 1" | names: "Generic Models 42:Generic Models 1:1901178" | material: "CONC. FOOTER - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 45:Generic Models 1" | names: "Generic Models 45:Generic Models 1:1901590" | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 48:Generic Models 1" | names: "Generic Models 48:Generic Models 1:1901863" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 46:Generic Models 1" | names: "Generic Models 46:Generic Models 1:1901949" | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 51:Generic Models 1" | names: "Generic Models 51:Generic Models 1:1902893" | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 268:Generic Models 1" | names: "Generic Models 268:Generic Models 1:1904786" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 269:Generic Models 1" | names: "Generic Models 269:Generic Models 1:1905287" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 271:Generic Models 1" | names: "Generic Models 271:Generic Models 1:1905324" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 272:Generic Models 1" | names: "Generic Models 272:Generic Models 1:1905355" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 54:Generic Models 1" | names: "Generic Models 54:Generic Models 1:1906220" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 67:Generic Models 1" | names: "Generic Models 67:Generic Models 1:1906232" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 83:Generic Models 1" | names: "Generic Models 83:Generic Models 1:1906244" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 93:Generic Models 1" | names: "Generic Models 93:Generic Models 1:1906256" | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 222:Generic Models 1" | names: "Generic Models 222:Generic Models 1:1907115" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 225:Generic Models 1" | names: "Generic Models 225:Generic Models 1:1907571" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 304:Generic Models 1" | names: "Generic Models 304:Generic Models 1:1907603" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 43:Generic Models 1" | names: "Generic Models 43:Generic Models 1:1907786" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 98:Generic Models 1" | names: "Generic Models 98:Generic Models 1:1907798" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 122:Generic Models 1" | names: "Generic Models 122:Generic Models 1:1907810" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 230:Generic Models 1" | names: "Generic Models 230:Generic Models 1:1962169" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 245:Generic Models 1" | names: "Generic Models 245:Generic Models 1:1962193" | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Types
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4 J's @ 24" O.C. - GROUTED IN PRECAST KEYS AND CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOLID CMU AS NEEDED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOLID CMU AS NEEDED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4 REBARS @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GROUT CORES AT REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#10 6x6 WIRE MESH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 VERTICAL BAR @ 18" O/C" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "REINFORCEMENT GROUTED INTO BROKEN CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 J's @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6" CONCRETE SLAB (2% SLOPE AWAY FROM BUILDING IF NO SLOPE CALLED OUT)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 REBARS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE STAIRS - 6 MIN. THICKNESS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE ARCH. DWG FOR ASSEMBLY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 J's @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GALV. PIPE STAIR RAILING SLEEVE OR BOLTED TO SIDE OF CONCRETE STRINGER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(4) #3" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2# @ 8" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONSTRUCTION JOINT, ROUGHEN, CLEANED AND MOISTENED BEFORE SLAB POUR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONSTRUCTION JOINT, ROUGHEN, CLEANED AND MOISTENED BEFORE SLAB POUR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 VERTICAL BAR @ 18" O/C" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6" CONCRETE SLAB (2% SLOPE AWAY FROM BUILDING IF NO SLOPE CALLED OUT)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 REBARS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(4) #3" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2# @ 8" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONSTRUCTION JOINT, ROUGHEN, CLEANED AND MOISTENED BEFORE SLAB POUR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLOOR FINISH T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4 BAR HORIZ. REINF" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MENDING PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MENDING PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MENDING PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X LEDGER - SIZE T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLOOR FINISH T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "POST-INSTALLED ANCHORS #3X6" BAR @ 1'-0" O.C. MAX. EMBEDMENT 4" STAGGERED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NON-BEARING 2X FURRING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FRAMING BEARING WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 CLOSED STIRRRUPS @ 8" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(5) # 4 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCEMENT STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCEMENT STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FRAMING BEARING WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOOTER - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C. VERTICAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C. VERTICAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4x60" @ 8" O.C. - VERTICAL STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C. STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C. STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FRAMING BEARING WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X6 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4x60" @ 8" O.C. - VERTICAL STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(3)#5" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2)#4" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C. HORIZONTAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C. VERTICAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C. VERTICAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4x60" @ 8" O.C. - VERTICAL STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #4x60" @ 8" O.C. - VERTICAL STARTER BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2)#4" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C. HORIZONTAL WALL REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4x18" BAR @ 2'-0" O.C. MAX. DRILL THRU HOLLOW CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "HSS 5X5X1/2 STEEL COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "1/4" STIFFENER PLATE EACH SIDE @ COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "HSS 5X5X1/2 STEEL COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2" GROUT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "one" | 2 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "1"" | 2 occurrences | material: "5/8" GALV. ANCHOR BOLT (11" MIN. EMBED)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "one" | 2 occurrences | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "1"" | 2 occurrences | material: "5/8" GALV. ANCHOR BOLT (11" MIN. EMBED)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "1" 2" | 8 occurrences | material: "ANCHOR BOLT PER ANCHOR TYPE IN HOLD DOWN SCHEDULE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal Fastenings - Base Plate - 11inX11inX3_4in" | 1 occurrence | material: "11"X11"X3/4" BASE PLATE W(4) 3/4" DIA. A325 BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal Fastenings - Base Plate - 11inX8inX3_4in 2" | 1 occurrence | material: "3/4"X8"X11" TOP BEARING PLATE W(4) 3/4" DIA. A325 BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X30 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal Fastener - Vertical Plate - 8inX20inX1_2in" | 1 occurrence | material: "1/2"X10"X20" W/(16) 3/4" DIA. X4" H.S." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable" | 7 occurrences | material: "3"X3"X1/4" STEEL ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable" | 3 occurrences | material: "3"X3"X1/4" STEEL ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in" | 3 occurrences | material: "1/4"X1/4"X8 1/2" FILLET WELD @ EACH SIDE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in" | 5 occurrences | material: "1/4"X1/4"X8 1/2" FILLET WELD @ EACH SIDE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle - Bolting Plate - 1/2"X3"X8 1/2"" | 6 occurrences | material: "3"X3"X1/4" STEEL ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "1"" | 6 occurrences | material: "5/8" GALV. ANCHOR BOLT (11" MIN. EMBED)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "1" 4" | 3 occurrences | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "1" 4" | 3 occurrences | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "1" 4" | 12 occurrences | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "1" 4" | 6 occurrences | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "W14X30 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "W14X30 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST BEAM BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "L3X2X3/8 STEEL ANGLE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "CONT. 3/8"X4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "EMBEDDED STEEL PLATE BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX" | 3 occurrences | material: "1/4" FILLET WELD EACH SIDE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX" | 1 occurrence | material: "1/4" FILLET WELD EACH SIDE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "1" 5" | 3 occurrences | material: "5/8"@16" O.C. POST INSTALLED ANCHOR - 4 1/2" MIN EMBED" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2)#4 LONG REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2)#4 LONG REINF." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#2@8" O.C. CLOSED STIRRUPS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(4)#4 VERTICAL REINFORCEMENT - INSIDE STIRRUPS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "POST-INSTALLED REBAR WITH ANCHORING EPOXY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOOTER - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "POST-INSTALLED REBAR WITH ANCHORING EPOXY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RC WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "3/4" x 1' 3"" | 1 occurrence | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RC WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "1" 7" | 4 occurrences | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RC WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X43 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "HSS 5X5X1/2 STEEL COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "1/4" STIFFENER PLATE EACH SIDE @ COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "050523 - Metal Fastenings - Base Plate - 11inX8inX3_4in" | 1 occurrence | material: "12"X12"X3/4" BASE PLATE W(4) 3/4" DIA. A325 BOLTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RC WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W14X53 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "3/4" x 11"" | 1 occurrence | material: "A325-N THRU BOLT 3/4" DIAM." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EMBEDDED STEEL PLATE BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL WASHER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EMBEDDED STEEL PLATE BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EMBEDDED STEEL PLATE BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "8"X9" CONC. CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(4)#3 LONG REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 CLOSED STIRRUPS @ 1'-0" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 - 12" O.C. - DOWEL DRILL & GROUT AFTER PLANK ERECTION - 8" EMBED MIN." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X8 SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK W/ DAPPED TOP - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK W/ DAPPED TOP - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK W/ DAPPED TOP - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "HORZ. REINFORCING - SEE SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "HORZ. REINFORCING - SEE SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILLED WITH GROUT EXTENDING PAST END OF REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILLED WITH GROUT EXTENDING PAST END OF REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6" 25PSI EXTRUDED POLYSTYRENE INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOOTER - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NUMBER OF END WALL STUDS PER HOLD DOWN SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "HOLD DOWN ANCHOR - SEE HOLD DOWN SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "1" 3" | 1 occurrence | material: "ANCHOR BOLT PER ANCHOR TYPE IN HOLD DOWN SCHEDULE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GROUT CORES WITHIN 12" ALL SIDES OF ANCHOR PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE NOTE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8"X4"X4" ANCHOR PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(8) #5" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(8) #5" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOOTING - SEE PLANS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "16"X16" CIP COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "16"X16" CIP COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(8) #5" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 COLUMN TIES @8"O.C. - ENTIRE HEIGHT OF COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FOOTING REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE SCHEDULE FOR SIZE AND REINFORCING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DISCONTINUE EVERY OTHER REBAR AT JOINT (TOP AND BOTTOM REBAR TO BE CONT.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" DEEP NOTCH AT EACH SIDE OF WALL (SPACE 25FT APART MIN.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PRECAST BEAM BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6"X8" MASONRY LINTEL SUPPORTED BY 6" CMU WALL NEXT TO CONCRETE COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6"X8" KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GROUT FILLED CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4" CLADDING - TO MATCH CMU FINISH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(1) #3 @ 16" O.C. HOOK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "10 X 8 X 16 CMU BLOCKS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(1) #5 REINFORCEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL REINF. (1) #5 @ 32" O.C. (FULLY GROUTED)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/2" LEVELING MORTAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4" CLADDING - TO MATCH CMU FINISH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GROUT FILLED CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "10 X 8 X 16 CMU BLOCKS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6"X8" KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6"X8" KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6"X8" KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6"X8" KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ALL 6" CMU TO BE FILLED WITH GROUT FOR 2 HR FIRE RATING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ALL 6" CMU TO BE FILLED WITH GROUT FOR 2 HR FIRE RATING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 404" | 1 occurrence | material: "LINTEL CMU 10W X 16D" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 404" | 1 occurrence | material: "(1) #5 LINTEL BOTTOM REINFORCEMENT" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 404" | 1 occurrence | material: "(1) #5 REINFORCEMENT @ CORNER TOP LENGHT = 25" + 25"" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 404" | 1 occurrence | material: materials ("FILLED WITH GROUT EXTENDING PAST END OF REBAR", "LINTEL CMU 10W X 16D") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 404" | 1 occurrence | material: "FILLED WITH GROUT EXTENDING PAST END OF REBAR" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "10 X 8 X 16 CMU BLOCKS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "10 X 8 X 16 CMU BLOCKS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ADJUSTABLE UNIT TIE @ 32"O.C. (AT CONCRETE BEAM & COLUMN)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ADJUSTABLE UNIT TIE @ 32"O.C. (AT CONCRETE BEAM & COLUMN)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONT. 2X TOP PLATE - STAGGER SEAMS - SEE STRUCT. SCHEDULES FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH SILL PLATE TO RIM BOARD W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO RIM BOARD W/10D @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RIM BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOE NAIL FLOOR TRUSS 2X TOP PLATE w/ (4) 16D EACH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD HEADER - SEE SCHEDULE - HEIGHT WILL VARY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONT. 2X TOP PLATE - STAGGER SEAMS - SEE STRUCT. SCHEDULES FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH SILL PLATE TO RIM BOARD W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO RIM BOARD W/10D @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 1/8” OSB RIM BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH WALL SEATHING TO END OF EACH FLOOR TRUSS W/ 10D AT 6" O/C" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOE NAIL FLOOR TRUSS 2X TOP PLATE w/ (4) 16D EACH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD HEADER - SEE SCHEDULE - HEIGHT WILL VARY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO RIM BOARD W/10D @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "JACK STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 EXTERIOR BEARING WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH SILL PLATE TO RIM BOARD W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO RIM BOARD W/10D @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RIM BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH RIM BOARD TO FLOOR TRUSS W/ (5) 16D NAILS (ATTACHEMENTS AT BLIND FASCIA T.B.D.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOE NAIL EACH TRUSS TO TOP PLATE W/(4) 16D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS 1 1/8" OSB RIM BOARD OR 1 3/4" LVL BLIND FASCIA" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LADDER TRUSS W/10D X 1 1/2" NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FULL DEPTH BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BLOCKING AS REQUIRED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "KNOCK OUT BOND BEAM - SEE ELEVATOR ELEVATIONS FOR SIZE AND REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BOTTOM SILL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LEDGER AND FLOOR TRUSSES W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X8 LEDGER ATTACHED W/ (2) STAGGERED 1/2" X 6 SIMPSON TITEN HD ANCHORS @ 24" O/C (3 5/8" MIN, EMBED)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X4 STUD WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE FOR FIRE PROTECTION - SEAL ALL PENETRATIONS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LADDER TRUSS W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 SHEAR WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RIM BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LADDER TRUSS W/10D X 1 1/2" NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONT. 2X TOP PLATE STAGGER SEAMS - SEE STRUCT. SCHEDULES FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOE NAIL FLOOR TRUSS 2X TOP PLATE w/ (4) 16D EACH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD HEADER - SEE SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO RIM BOARD W/10D @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH SILL PLATE TO DOUBLE TOP PLATE W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X4 LEDGER ATTACHED W/60D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/2" BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 16 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH SILL PLATE TO DOUBLE TOP PLATE W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH SILL PLATE TO DOUBLE TOP PLATE W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 16 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LEDGER AND DOUBLE PLATE W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE - PAINT DARK GRAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH SILL PLATE TO DOUBLE TOP PLATE W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 16 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X6 SOUTHERN PINE - NO. 1 - 32" O.C. - PAINTED DARK GRAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LEDGER AND DOUBLE PLATE W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/2" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "19/32" OSB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X6 SOUTHERN PINE - NO. 1 - 32" O.C. - PAINTED DARK GRAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO 4X6 JOIST AND LEDGER W/10D NAILS @ 6" O.C. (TAKE CARE TO NOT EXPOSE FASTENERS TO FINISH SPACE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X6 SOUTHERN PINE - NO. 1 - 32" O.C. - PAINTED DARK GRAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 RIM BOARD W/ (3) 16D NAILS AT EACH JOIST" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOE NAIL RIM BOARD TO DOUBLE TOP PLATE W/ 10D AT 7" O/C UNLESS NOTED OTHERWISE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LEDGER AND DOUBLE PLATE W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X6 SOUTHERN PINE - NO. 1 - 32" O.C. - PAINTED DARK GRAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE ARCH DWGS FOR INSULATION/MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH SILL PLATE TO DOUBLE TOP PLATE W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - NO WOOD STAMPS VISIBLE FROM UNDERSIDE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 16 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X6 SOUTHERN PINE - NO. 1 - 32" O.C. - PAINTED DARK GRAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X6 SOUTHERN PINE - NO. 1 - 32" O.C. - PAINTED DARK GRAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE ARCH DWGS FOR INSULATION/MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LEDGER AND DOUBLE PLATE W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LEDGER AND DOUBLE PLATE W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4 PLYWOOD GUSSET GLUED AND NAILED TO TOP AND BOTTOM CHORDS W/ 10D @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 EXTERIOR BEARING WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH SILL PLATE TO RIM BOARD W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO RIM BOARD W/10D @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RIM BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH RIM BOARD TO FLOOR TRUSS W/ (5) 16D NAILS (ATTACHEMENTS AT BLIND FASCIA T.B.D.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS 1 1/8" OSB RIM BOARD OR 1 3/4" LVL BLIND FASCIA" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LADDER TRUSS W/10D X 1 1/2" NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FULL DEPTH BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "W12X87 STEEL BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X PLATE ATTACHED TO STEEL W/ (T.B.D.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOE NAIL EACH TRUSS TO TOP PLATE W/(4) 16D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "3/4" | 1 occurrence | material: "3/4" DIAMETER x 8" EMBEDMENT EPOXY ANCHORS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "3/4" | 1 occurrence | material: "3/4" DIAMETER x 8" EMBEDMENT EPOXY ANCHORS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/4 X 3 TITEN ANCHOR MODEL THDB25300H @ 4FT O.C. (WITHIN 8" OF EVERY CORNER)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/4 X 3 TITEN ANCHOR MODEL THDB25300H @ 4FT O.C. (WITHIN 8" OF EVERY CORNER)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 16 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD ROOF TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TPO MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE ARCH DWGS FOR INSULATION/MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE/SPACING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATING TO DOUBLE TOP PLATE W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 LEDGER W/ (2) 1/4" DIA. X 6" SIMPSON SDS SCREWS AT EACH STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/2" BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 16 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "KNOCK OUT BOND BEAM - SEE ELEVATOR ELEVATIONS FOR SIZE AND REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH TRUSS TO DOUBLE TOP PLATE W/ 16D FASTENERS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X4 LEDGER ATTACHED W/60D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 16 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X4 LEDGER ATTACHED W/60D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/2" BLOCKING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X4 LEDGER ATTACHED W/60D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LEDGER AND FLOOR TRUSSES W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATING TO DOUBLE TOP PLATE W/10D NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL PER BALC. MANU" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "BALC FASTENER" | 1 occurrence | material: "ATTACHMENTS PER BALC. MANU." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "BALC FASTENER" | 1 occurrence | material: "ATTACHMENTS PER BALC. MANU." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) 1 1/8" RIM BOARDS - (1ST) - ATTACH WITH W/(5) 16D AT EACH TRUSS - (2ND) - BLOCKING BETWEEN TRUSSES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 16 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1X VERY TOP PLATE (VTP)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SLOTTED CLIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 16 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DS DRYWALL STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DS DRYWALL STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SHIM UNDER DRYWALL STOP AS NECESSARY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" OSB - SEE FLOOR SHEATHING IN WOOD FRAMING SCHEDULE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 SHEAR WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD. (PAINTED) AT CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/8" THICK SOUND ATTENUATION MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. INSTALLED PERPENDICULAR TO TRUSSES - SPACED 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 1/8" OSB RIM BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FASTENER/SPACING T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO LADDER TRUSS W/10D X 1 1/2" NAILS @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONT. 2X TOP PLATE STAGGER SEAMS - SEE STRUCT. SCHEDULES FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOE NAIL FLOOR TRUSS 2X TOP PLATE w/ (4) 16D EACH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO RIM BOARD W/10D @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PLUMBING VENTS/WASTE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GUSSET PLATES BY TRUSS MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD FLOOR TRUSSES - SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONT. 2X TOP PLATE STAGGER SEAMS - SEE STRUCT. SCHEDULES FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO RIM BOARD W/10D @ 6" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PROVIDE HALF THE NUMBER OF VERTICAL REINFORCING CALLED OUT IN THE SCHEDULE (BOTH FACES)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) # 6 x5'- 0" ONE EACH FACE OF CORNER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PROVIDE HALF THE NUMBER OF HORZ. REINFORCING (TOP AND BOTTOM) CALLED OUT IN THE SCHEDULE (BOTH FACES)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "FOR EVERY LAYER OF REBAR INDICATED IN THE SCHEDULE, PROVIDE (1) LAYER OF (4) #5 DIAGONAL BARS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "ADJUST OR SHIFT REINFORCING TO SLIDE AROUND WALL PENETRATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PIPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOOTER - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE SCHEDULE FOR SIZE AND REINFORCING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ALL PIPING TO CLEAR SLEEVE BY 1/2'' ALL AROUND. TYPICAL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PIPE - COORDINATE LOCATOIN W/ PIPING CONTRACTOR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL ANNUAL SPACE WITH BELOW GRADE FLEXIBLE SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PIPE SLEEVE - COORDINATE W/ PIPING CONTRACTOR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL ANNUAL SPACE WITH BELOW GRADE FLEXIBLE SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PIPE SLEEVE - COORDINATE W/ PIPING CONTRACTOR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE SCHEDULE FOR SIZE AND REINFORCING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE SCHEDULE FOR SIZE AND REINFORCING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DISCONTINUE EVERY OTHER REBAR AT JOINT (TOP AND BOTTOM REBAR TO BE CONT.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" DEEP NOTCH AT EACH SIDE OF WALL (SPACE 25FT APART MIN.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DISCONTINUE EVERY OTHER REBAR AT JOINT (TOP AND BOTTOM REBAR TO BE CONT.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Walls" | 1 occurrence | material: "2" x 4" CONTINUOUS VERTICAL KEYWALL FULL HEIGHT" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 435" | 1 occurrence | material: "LAP HORIZONTAL REINFORCING" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOOTING - SEE PLANS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE SCHEDULE FOR SIZE AND REINFORCING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE SCHEDULE FOR SIZE AND REINFORCING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12" EACH WAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE SLAB ON GRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE SLAB ON GRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12" EACH WAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 DOWEL @ 18"O.C. TYPICAL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#8@12" O.C. EACH WAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#8@12" O.C. EACH WAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 DOWEL @ 18"O.C. TYPICAL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12" O.C. HORIZONTAL AND VERTICAL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ROUGHENED SURFACE OR 2X4 KEYWAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #5 x CONTINUOUS LAP 30" MINIMUM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6" SERRATED TYPE PVC WATERSTOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6" SERRATED TYPE PVC WATERSTOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXPANSION JOINT MATERIAL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PROVIDE STANDARD 90º HOOK INTO FOOTING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2x4 KEYWAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2x4 KEYWAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE ARCH. DWGS FOR WATERPROOFING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "24" U SHAPED #3 STIRRUP - WRAP AROUND ANCHOR BOLTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NON SHRINK LEVELING GROUT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "5/8" (at 8" base plate)" | 3 occurrences | material: "(4) 5/8" DIA F1554 GR36 ANCHRO BOLTS (W/ DOUBLE NUT) - POST INSTALLED W/ HILTI EPOXY" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "HSS 8X8X3/16 STEEL COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "14"X13"X3/4" BASE PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "5/8" (at 8" base plate)" | 1 occurrence | material: "(4) 5/8" DIA F1554 GR36 ANCHRO BOLTS (W/ DOUBLE NUT) - POST INSTALLED W/ HILTI EPOXY" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GROUT CORES WITHIN 12" ALL SIDES OF ANCHOR PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NON SHRINK LEVELING GROUT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "HSS 8X8X3/16 STEEL COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "14"X11"X3/4" BASE PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "5/8" (at 8" base plate)" | 2 occurrences | material: "(4) 5/8" DIA F1554 GR36 ANCHRO BOLTS (W/ DOUBLE NUT) - POST INSTALLED W/ HILTI EPOXY" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PRECAST BEAM BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NON SHRINK LEVELING GROUT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "HSS 8X8X3/16 STEEL COLUMN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "14"X14"X3/4" BASE PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PRECAST BEAM BY PRECAST MANU." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/4" SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLOOR FINISH T.B.D (3/8" ZONE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "25/32" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE - PAINT DARK GRAY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "19/32" OSB PLYWOOD BONDED W/ EXT. GLUE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "19/32" OSB PLYWOOD BONDED W/ EXT. GLUE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 TREATED BLOCKING BETWEEN JOISTS - 5/8" TITEN HD SCREWS 16" O.C. (4"MIN. EMBED) - GROUT CORE SOLID AT ANCHORS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "5/8"" | 1 occurrence | material: "3/4" DIAMETER x 8" EMBEDMENT EPOXY ANCHORS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH FLOOR SHEATHING TO 4X6 JOIST AND LEDGER W/10D NAILS @ 6" O.C. (TAKE CARE TO NOT EXPOSE FASTENERS TO FINISH SPACE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BALC. STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONT. 2X TOP PLATE - STAGGER SEAMS - SEE STRUCT. SCHEDULES FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" RIGID INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BALC. STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" FURRING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FIBER CEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "3/8" | 36 occurrences | material: "3/8"X5" GALV. LAG BOLT" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BALC. STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONT. 2X TOP PLATE - STAGGER SEAMS - SEE STRUCT. SCHEDULES FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" RIGID INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BALC. STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" FURRING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FIBER CEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL SHEATHING (IF SHEAR WALL) - SEE SCHEDULE FOR SIZE/FASTENERS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BALC. STEEL PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CRIPPLE STUD BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "19/32" OSB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "25 PSI RIGID INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOUNDATION - (SEE 'WALL TAG' FOR SIZE/REBAR) - LIQUID MEMB. IF BELOW GRADE (WRAP FOOTING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "LEVELING GROUT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLUID APPLIED MEMBRANE (2 APPLICATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLUID APPLIED WATERPROOFING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RUBBER MEMBRANE COMPATIABLE WITH FLUID APPLIED MEMBRANE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "25 PSI RIGID INSULATION 'CURB'" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DRAINAGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" XPS INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DRAINAGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DRAINAGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X4 TREATED POSTED 24" O.C. - EXTERIOR STAIN TO MATCH DECKING COLOR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GALV. BRAKE METAL FLASHING - WITH BACK LEG END DAM - CAST INTO CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "5/8" | 4 occurrences | material: materials ("5/8"X10" GALV. ANCHORS (COUNTERSUNK)", "GALV. WASHERS AS NECESSARY") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXTEIOR CEMENT BOARD MEETING ASTM C 1325" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EIFS BASE AND FINISH COAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLUID APPLIED MEMBRANE (2 APPLICATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "FASTENER AT 1X6 DECKING" | 4 occurrences | material: "(0.220 X 3) SDWS TIMBER SCREW W/ DOUBLE-BARRIER COATING - FLAT HEAD" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X4 TREATED POSTED 24" O.C. - EXTERIOR STAIN TO MATCH DECKING COLOR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "(2) FASTENER AT 1X6 DECKING" | 58 occurrences | material: "(2) WEATHER RESISTANT SCREWS AT EACH BOARD (MATCH EXISTING)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RIPPED 1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X4 TREATED POSTED 24" O.C. - EXTERIOR STAIN TO MATCH DECKING COLOR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X4 TREATED POSTED 24" O.C. - EXTERIOR STAIN TO MATCH DECKING COLOR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 TREATED BLOCKING TOENAILED AT POSTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X6 TREATED BLOCKING TOENAILED AT POSTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE SLAB WITH #10 6X6 WIRE MESH - SLOPED TOWARD DRAINS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "25 PSI RIGID INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DRAINAGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLUID APPLIED MEMBRANE (2 APPLICATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLUID APPLIED MEMBRANE (2 APPLICATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLUID APPLIED MEMBRANE (2 APPLICATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE SLAB WITH #10 6X6 WIRE MESH - SLOPED TOWARD DRAINS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EIFS BASE AND FINISH COAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X4 TREATED POSTED 24" O.C. - EXTERIOR STAIN TO MATCH DECKING COLOR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X6 BLOCKING (OR 2 SISTERED 2X6'S) BETWEEN JOISTS - PAINT TO MATCH JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "25 PSI RIGID INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLUID APPLIED MEMBRANE (2 APPLICATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DRAINAGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4X4 TREATED POSTED 24" O.C. - EXTERIOR STAIN TO MATCH DECKING COLOR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE SLAB WITH #10 6X6 WIRE MESH - SLOPED TOWARD DRAINS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "SIMPSON - ABA66Z W/ 5/8"X8" ANCHOR BOLT W/ NON-SHRINK GROUT AT BASE" | 1 occurrence | material: materials ("5/8" X 3.5" ANCHOR BOLT", "SIMPSON APVB44 AT EACH 4X4 POST") | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "C_APVB44_3d_Cad_MULT_Prod" | 1 occurrence | material: "Galvanized" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "F70_1" | 1 occurrence | material: "ROTHOBLAAS F7080 - GALV. CONCEALED BLADE BASE" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "3/8 AT DIVIDER SHAFT" | 2 occurrences | material: "3/8"X4" GALV. THRU BOLT W/ GALV. WASHERS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "3/8 AT DIVIDER SHAFT" | 2 occurrences | material: "3/8"X4" GALV. THRU BOLT W/ GALV. WASHERS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "1/4 anchors at divider posts" | 2 occurrences | material: "(4) 1/4" x 3.5" GALV. EXPANSION ANCHORS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "1/4 anchors at divider posts" | 2 occurrences | material: "(4) 1/4" x 3.5" GALV. EXPANSION ANCHORS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GALV. OR SS SHIMS AS NECESSARY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEYOND - 1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GALV. PIPE STAIR RAILING SLEEVE OR BOLTED TO SIDE OF CONCRETE STRINGER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(S) SOUND BATT. INSULATION (THICKNESS TO MATCH WALL DEPTH)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1 X 6 (.94 IN X 5.5 IN) SQUARE-EDGE BOARD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONC. FOOTER - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#5@12"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4@8"O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon

Property sets
  Pset_ProductRequirements | properties | on 1167 objects (1047 IFCWALL, 120 IFCOPENINGELEMENT) | on 1047 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 176 objects (172 IFCBUILDINGELEMENTPROXY, 4 IFCOPENINGELEMENT) | on 30 type objects
    Category = "Structural Connections" (IFCLABEL)
  Pset_ProductRequirements | properties | on 47 objects (47 IFCBUILDINGELEMENTPROXY) | on 22 type objects
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "FOUNDATION" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "1ST - FLOOR" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "2ND FLOOR" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 956 objects (913 IFCWALL, 43 IFCOPENINGELEMENT) | on 913 type objects
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 147 objects (74 IFCOPENINGELEMENT, 73 IFCWALL) | on 73 type objects
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 64 objects (61 IFCWALL, 3 IFCOPENINGELEMENT) | on 61 type objects
    Reference = "Dowel" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 58 objects (58 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "(2) FASTENER AT 1X6 DECKING" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 36 objects (36 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "3/8" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 24 objects (24 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Reference = "1" 4" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Reference = "1"" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 28 more contents on 85 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 913 objects (913 IFCWALL) | on 913 type objects
    Reference = "Generic Models 1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 73 objects (73 IFCWALL) | on 73 type objects
    Reference = "Generic Models 65" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 61 objects (61 IFCWALL) | on 61 type objects
    Reference = "Dowel" (IFCLABEL)
  Pset_WallCommon | properties | on 913 objects (913 IFCWALL) | on 913 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 73 objects (73 IFCWALL) | on 73 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 61 objects (61 IFCWALL) | on 61 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Dowel" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 74 objects (74 IFCOPENINGELEMENT)
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 43 objects (43 IFCOPENINGELEMENT)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 4 objects (4 IFCOPENINGELEMENT)
    Reference = "F70_1" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 3 objects (3 IFCOPENINGELEMENT)
    Reference = "Dowel" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 58 objects (58 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "(2) FASTENER AT 1X6 DECKING" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 36 objects (36 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "3/8" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 24 objects (24 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Reference = "1" 4" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Reference = "1"" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "051200 - Metal Fastener - Vertical Angle Weld Plate - 8.5inX3inxH=Variable" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY) | on 2 type objects
    Reference = "051200 - Metal Fastener - Vertical Angle Weld - 1_4inX1_4inX8 1_2in" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "1" 2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Reference = "5/8" (at 8" base plate)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 25 more contents on 59 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 5 objects (4 IFCOPENINGELEMENT, 1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Rotho Blaas srl" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Manufacturer = "Simpson Strong-Tie Company Inc." (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "FOUNDATION" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "1ST - FLOOR" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "2ND FLOOR" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)

Other addresses and roles
  2 x postal address: "1750 N OXFORD AVE. - EAU CLAIRE, WI", "<Default>"