IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Details from OD Template.ifc"
Time stamp: "2022-02-15T21:26:37-06:00"
Preprocessor: "IfcOpenShell v0.7.0-4c40fc16"
Originating system: "BlenderBIM 0.0.220210"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "ryan@openingdesign.com" of Organization (no name given)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1644959437 (2022-02-15T21:10:37Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "**NAME OF PROJECT**" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 100.
    IFCBUILDING
      IFCBUILDINGSTOREY "BASEMENT (RENAME, BUT DON'T DELETE THIS LEVEL)" | long name "BASEMENT (RENAME, BUT DON'T DELETE THIS LEVEL)" | object type "Level:Project Base Point" | elevation -8.
        contains 183 elements
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 129:Generic Models 1" | names: "Generic Models 129:Generic Models 1:609995" | material: "EXISTING SLAB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 8:Generic Models 1" | names: "Generic Models 8:Generic Models 1:826903" | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 141:Generic Models 1" | names: "Generic Models 141:Generic Models 1:830973" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 144:Generic Models 1" | names: "Generic Models 144:Generic Models 1:830994" | material: "#10 6x6 WIRE MESH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 145:Generic Models 1" | names: "Generic Models 145:Generic Models 1:831218" | material: "6 MIL VAPOR BARRIER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 150:Generic Models 1" | names: "Generic Models 150:Generic Models 1:831484" | material: "6" COMPACTED CRUSHED STONE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 151:Generic Models 1" | names: "Generic Models 151:Generic Models 1:832637" | material: "GRADE (SLOPE 2% MIN AWAY FROM BUILDING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 183:Generic Models 1" | names: "Generic Models 183:Generic Models 1:854474" | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 177:Generic Models 1" | names: "Generic Models 177:Generic Models 1:856630" | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 155" | object type "Generic Models 178:Generic Models 155" | names: "Generic Models 178:Generic Models 155:856646" | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 184" | object type "Generic Models 184:Generic Models 184" | names: "Generic Models 184:Generic Models 184:858653" | material: "GRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 269:Generic Models 263" | names: "Generic Models 269:Generic Models 263:1381148" | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 270:Generic Models 263" | names: "Generic Models 270:Generic Models 263:1381912" | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 271:Generic Models 263" | names: "Generic Models 271:Generic Models 263:1382304" | material: "EXISTING PAVEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 274:Generic Models 263" | names: "Generic Models 274:Generic Models 263:1384626" | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 275:Generic Models 263" | names: "Generic Models 275:Generic Models 263:1384752" | material: "COMPACTED SUBGRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 277:Generic Models 263" | names: "Generic Models 277:Generic Models 263:1385057" | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 278:Generic Models 263" | names: "Generic Models 278:Generic Models 263:1385167" | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 279:Generic Models 263" | names: "Generic Models 279:Generic Models 263:1385327" | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 280:Generic Models 263" | names: "Generic Models 280:Generic Models 263:1385413" | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 281:Generic Models 263" | names: "Generic Models 281:Generic Models 263:1385588" | material: "3" TO 6" WASHED OR CLEAR STONE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 286:Generic Models 263" | names: "Generic Models 286:Generic Models 263:1386677" | material: "6" CRUSHED AGGREGATE BASE COURSE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 292:Generic Models 263" | names: "Generic Models 292:Generic Models 263:1388713" | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 294:Generic Models 263" | names: "Generic Models 294:Generic Models 263:1388734" | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 295:Generic Models 263" | names: "Generic Models 295:Generic Models 263:1388746" | material: "CRUSHED AGGREGATE BASE COURSE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 289:Generic Models 263" | names: "Generic Models 289:Generic Models 263:1394121" | material: "7" CONC. DRIVE APPROACH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 297:Generic Models 263" | names: "Generic Models 297:Generic Models 263:1394272" | material: "SLOPED - 7" CONC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 298:Generic Models 263" | names: "Generic Models 298:Generic Models 263:1394399" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 299:Generic Models 263" | names: "Generic Models 299:Generic Models 263:1395691" | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 300:Generic Models 263" | names: "Generic Models 300:Generic Models 263:1395728" | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 282:Generic Models 263" | names: "Generic Models 282:Generic Models 263:1398156" | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 301:Generic Models 263" | names: "Generic Models 301:Generic Models 263:1398203" | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 290:Generic Models 263" | names: "Generic Models 290:Generic Models 263:1399522" | material: "GRADED BACKFILL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 291:Generic Models 263" | names: "Generic Models 291:Generic Models 263:1399720" | material: "GRADED BACKFILL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 306:Generic Models 263" | names: "Generic Models 306:Generic Models 263:1399821" | material: "EXISTING GRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 307:Generic Models 263" | names: "Generic Models 307:Generic Models 263:1400379" | material: "CONCRETE PAVEMENT HEAVY DUTY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 310:Generic Models 263" | names: "Generic Models 310:Generic Models 263:1400408" | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 311:Generic Models 263" | names: "Generic Models 311:Generic Models 263:1400420" | material: "COMPACTED SUBGRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 309:Generic Models 263" | names: "Generic Models 309:Generic Models 263:1400637" | material: "EPOXY COATED 6 X 6 X W2.9 X W2.9, PLACED 3" ABOVE SLAB BASE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 283:Generic Models 263" | names: "Generic Models 283:Generic Models 263:1403684" | material: "SLOPED - 7" CONC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 284:Generic Models 263" | names: "Generic Models 284:Generic Models 263:1403706" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 276:Generic Models 263" | names: "Generic Models 276:Generic Models 263:1405189" | material: "1" EXPANSION JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 263" | object type "Generic Models 299:Generic Models 263" | names: "Generic Models 299:Generic Models 263:1451698" | material: "CONCRETE CURB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 263" | object type "Generic Models 299:Generic Models 263" | names: "Generic Models 299:Generic Models 263:1451928" | material: "CONCRETE CURB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 349:Generic Models 1" | names: "Generic Models 349:Generic Models 1:1464038" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 414:Generic Models 1" | names: "Generic Models 414:Generic Models 1:1506002" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 423:Generic Models 1" | names: "Generic Models 423:Generic Models 1:1507139" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 424:Generic Models 1" | names: "Generic Models 424:Generic Models 1:1507163" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 425:Generic Models 1" | names: "Generic Models 425:Generic Models 1:1507183" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 428:Generic Models 1" | names: "Generic Models 428:Generic Models 1:1507428" | material: "R-19 BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Ground Rod" | object type "Ground Rod:Ground Rod" | names: "Ground Rod:Ground Rod:1515191" | material: "5/8" x 8' GROUND ROD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate" | object type "Light Pole Base Plate1:Light Pole Base Plate" | names: "Light Pole Base Plate1:Light Pole Base Plate:1515308" | material: "(4) VERTICAL #6 REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate" | object type "Light Pole Base Plate2:Light Pole Base Plate" | names: "Light Pole Base Plate2:Light Pole Base Plate:1516878" | material: "STEEL BASE PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 126" | object type "Walls 126:Walls 126" | names: "Walls 126:Walls 126:1518668" | material: "24" DIA. CONCRETE POLE BASE WITH THOROSEAL FINISH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Walls 126" | object type "Walls 127:Walls 126" | names: "Walls 127:Walls 126:1519197" | material: "Earth" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 500:Generic Models 1" | names: "Generic Models 500:Generic Models 1:1577429" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 11:Generic Models 1" | names: "Generic Models 11:Generic Models 1:1577503" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 28:Generic Models 1" | names: "Generic Models 28:Generic Models 1:1577522" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 238:Generic Models 1" | names: "Generic Models 238:Generic Models 1:1577541" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 446:Generic Models 1" | names: "Generic Models 446:Generic Models 1:1577560" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 26:Generic Models 1" | names: "Generic Models 26:Generic Models 1:1577677" | material: "OTHER WALL TYPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 514:Generic Models 1" | names: "Generic Models 514:Generic Models 1:1578074" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 537:Generic Models 1" | names: "Generic Models 537:Generic Models 1:1579530" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate" | object type "Light Pole Base Plate3:Light Pole Base Plate" | names: "Light Pole Base Plate3:Light Pole Base Plate:1586248" | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate" | object type "Light Pole Base Plate4:Light Pole Base Plate" | names: "Light Pole Base Plate4:Light Pole Base Plate:1586650" | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCBUILDINGELEMENTPROXY | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1595839", "Model Text:OD_Very Large:1595840", "Model Text:OD_Very Large:1595841" (+3 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 44:Generic Models 1" | names: "Generic Models 44:Generic Models 1:1601268" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 40:Generic Models 1" | names: "Generic Models 40:Generic Models 1:1601430" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 45:Generic Models 1" | names: "Generic Models 45:Generic Models 1:1601478" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 50:Generic Models 1" | names: "Generic Models 50:Generic Models 1:1601574" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 54:Generic Models 1" | names: "Generic Models 54:Generic Models 1:1601706" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 8:Generic Models 1" | names: "Generic Models 8:Generic Models 1:1622703" | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 141:Generic Models 1" | names: "Generic Models 141:Generic Models 1:1622735" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 144:Generic Models 1" | names: "Generic Models 144:Generic Models 1:1622740" | material: "#10 6x6 WIRE MESH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 213:Generic Models 1" | names: "Generic Models 213:Generic Models 1:1633830" | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 216:Generic Models 1" | names: "Generic Models 216:Generic Models 1:1633848" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 217:Generic Models 1" | names: "Generic Models 217:Generic Models 1:1633858" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 218:Generic Models 1" | names: "Generic Models 218:Generic Models 1:1633868" | material: "7/8" FURRING CHANNELS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 221:Generic Models 1" | names: "Generic Models 221:Generic Models 1:1633899" | material: "R-19 BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 223:Generic Models 1" | names: "Generic Models 223:Generic Models 1:1633925" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 224:Generic Models 1" | names: "Generic Models 224:Generic Models 1:1633938" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 225:Generic Models 1" | names: "Generic Models 225:Generic Models 1:1633951" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 226:Generic Models 1" | names: "Generic Models 226:Generic Models 1:1633964" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 229:Generic Models 1" | names: "Generic Models 229:Generic Models 1:1633990" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 230:Generic Models 1" | names: "Generic Models 230:Generic Models 1:1634117" | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 231:Generic Models 1" | names: "Generic Models 231:Generic Models 1:1634198" | material: "5/8" GYP. BD @ CEILING (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 430:Generic Models 1" | names: "Generic Models 430:Generic Models 1:1651556" | material: "NOMINAL 3/4" THICK, 48" WIDE GYPSUM BOARD - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 797:Generic Models 1" | names: "Generic Models 797:Generic Models 1:1651582" | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 431:Generic Models 1" | names: "Generic Models 431:Generic Models 1:1651595" | material: "RESILIENT CHANNEL - FORMED FROM MIN. 25 MSG GALV. STEEL SPACED MAX 24" O.C. PERPENDICULAR TO JOISTS - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 433:Generic Models 1" | names: "Generic Models 433:Generic Models 1:1651607" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 796:Generic Models 1" | names: "Generic Models 796:Generic Models 1:1651622" | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 421:Generic Models 1" | names: "Generic Models 421:Generic Models 1:1651662" | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 422:Generic Models 1" | names: "Generic Models 422:Generic Models 1:1651685" | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 233:Generic Models 1" | names: "Generic Models 233:Generic Models 1:1651709" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 234:Generic Models 1" | names: "Generic Models 234:Generic Models 1:1651722" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 235:Generic Models 1" | names: "Generic Models 235:Generic Models 1:1651751" | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 237:Generic Models 1" | names: "Generic Models 237:Generic Models 1:1651777" | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 239:Generic Models 1" | names: "Generic Models 239:Generic Models 1:1651794" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 240:Generic Models 1" | names: "Generic Models 240:Generic Models 1:1651807" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 241:Generic Models 1" | names: "Generic Models 241:Generic Models 1:1651820" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 244:Generic Models 1" | names: "Generic Models 244:Generic Models 1:1651835" | material: "GALV. STEEL WITH TOTAL AREA OF DUCT OPENING NOT TO EXCEED 113 SQ. IN. PER 100 SQ. FT. OF CEILING AREA, AREA OF INDIVIDUAL DUCT OPENING NOT TO EXCEED 113 SQ. IN. MAX. DIMENSION OF OPENING 12" - SEE UL ..." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 249:Generic Models 1" | names: "Generic Models 249:Generic Models 1:1651856" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 253:Generic Models 1" | names: "Generic Models 253:Generic Models 1:1651877" | material: "20" X 48"/60" OR 24" X 48" - MAX OF 16 SQ FT PER 100 SQ FT OF CEILING AREA - OR - INCANDESCENT LAMP TYPE 6.5" DIA. X 7-1/2" HIGH - (4) FIXTURES PER 100 SQ FT OF CEILING AREA (USE FIXTURE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 254:Generic Models 1" | names: "Generic Models 254:Generic Models 1:1651918" | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 255:Generic Models 1" | names: "Generic Models 255:Generic Models 1:1651932" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 256:Generic Models 1" | names: "Generic Models 256:Generic Models 1:1651956" | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 257:Generic Models 1" | names: "Generic Models 257:Generic Models 1:1651969" | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 258:Generic Models 1" | names: "Generic Models 258:Generic Models 1:1651985" | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 259:Generic Models 1" | names: "Generic Models 259:Generic Models 1:1651998" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 260:Generic Models 1" | names: "Generic Models 260:Generic Models 1:1652050" | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 261:Generic Models 1" | names: "Generic Models 261:Generic Models 1:1652062" | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 262:Generic Models 1" | names: "Generic Models 262:Generic Models 1:1652080" | material: "GYPSUM BOARD — 5/8" X 4 FT WIDE GYPSUM BOARD, INSTALLED WITH LONG DIMENSION PERPENDICULAR TO CROSS TEES WITH SIDE JOINTS CENTERED ALONG MAIN RUNNERS." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 265:Generic Models 1" | names: "Generic Models 265:Generic Models 1:1652106" | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 266:Generic Models 1" | names: "Generic Models 266:Generic Models 1:1652123" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 267:Generic Models 1" | names: "Generic Models 267:Generic Models 1:1652136" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 268:Generic Models 1" | names: "Generic Models 268:Generic Models 1:1652149" | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 296:Generic Models 1" | names: "Generic Models 296:Generic Models 1:1652164" | material: "AIR DUCT — MIN 0.029 IN. THICK (22 GAUGE) GALV STEEL AIR DUCT. TOTAL AREA OF DUCT OPENINGS NOT TO EXCEED 114 SQ IN. PER EACH 100 SQ FT OF CEILING AREA." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 302:Generic Models 1" | names: "Generic Models 302:Generic Models 1:1652185" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 303:Generic Models 1" | names: "Generic Models 303:Generic Models 1:1652206" | material: "2' x 4' RECESSED LIGHT FIXTURE WITH STEEL HOUSING AND 'FIXTURE PROTECTION' - SPACED TO NOT EXCEED 24 SQ FT PER 100 SQ FT OF CEILING AREA - SEE UL LISTING FOR MORE INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 305:Generic Models 1" | names: "Generic Models 305:Generic Models 1:1652247" | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 313:Generic Models 1" | names: "Generic Models 313:Generic Models 1:1652261" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 314:Generic Models 1" | names: "Generic Models 314:Generic Models 1:1652285" | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 315:Generic Models 1" | names: "Generic Models 315:Generic Models 1:1652301" | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 316:Generic Models 1" | names: "Generic Models 316:Generic Models 1:1652314" | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 317:Generic Models 1" | names: "Generic Models 317:Generic Models 1:1652367" | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 318:Generic Models 1" | names: "Generic Models 318:Generic Models 1:1652390" | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 404:Generic Models 1" | names: "Generic Models 404:Generic Models 1:1659546" | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 321:Generic Models 1" | names: "Generic Models 321:Generic Models 1:1659594" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 322:Generic Models 1" | names: "Generic Models 322:Generic Models 1:1659680" | material: "BREAK EVERY OTHER REBAR AT JOINT (TOP AND BOTTOM REBAR TO BE CONT.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 319:Generic Models 1" | names: "Generic Models 319:Generic Models 1:1660588" | material: "3/4" DEEP NOTCH AT EACH SIDE OF WALL (SPACE APART - 25FT MIN.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 555:Generic Models 1" | names: "Generic Models 555:Generic Models 1:1713008" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 204:Generic Models 1" | names: "Generic Models 204:Generic Models 1:1773316" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 206:Generic Models 1" | names: "Generic Models 206:Generic Models 1:1773499" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 208:Generic Models 1" | names: "Generic Models 208:Generic Models 1:1773613" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 210:Generic Models 1" | names: "Generic Models 210:Generic Models 1:1773717" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 596:Generic Models 1" | names: "Generic Models 596:Generic Models 1:1818276" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 57:Generic Models 1" | names: "Generic Models 57:Generic Models 1:1824687" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 58:Generic Models 1" | names: "Generic Models 58:Generic Models 1:1824706" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 61:Generic Models 1" | names: "Generic Models 61:Generic Models 1:1848231" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 63:Generic Models 1" | names: "Generic Models 63:Generic Models 1:1848259" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 68:Generic Models 1" | names: "Generic Models 68:Generic Models 1:1848300" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 70:Generic Models 1" | names: "Generic Models 70:Generic Models 1:1848326" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 71:Generic Models 1" | names: "Generic Models 71:Generic Models 1:1848339" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 72:Generic Models 1" | names: "Generic Models 72:Generic Models 1:1848352" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 73:Generic Models 1" | names: "Generic Models 73:Generic Models 1:1848365" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 211:Generic Models 1" | names: "Generic Models 211:Generic Models 1:1848391" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 212:Generic Models 1" | names: "Generic Models 212:Generic Models 1:1848411" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 214:Generic Models 1" | names: "Generic Models 214:Generic Models 1:1848424" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 215:Generic Models 1" | names: "Generic Models 215:Generic Models 1:1848437" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 345:Generic Models 1" | names: "Generic Models 345:Generic Models 1:1848797" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 342:Generic Models 1" | names: "Generic Models 342:Generic Models 1:1848940" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 64:Generic Models 1" | names: "Generic Models 64:Generic Models 1:1849353" | material: "CONDUIT/PIPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 344:Generic Models 1" | names: "Generic Models 344:Generic Models 1:1849507" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 348:Generic Models 1" | names: "Generic Models 348:Generic Models 1:1849566" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 351:Generic Models 1" | names: "Generic Models 351:Generic Models 1:1849596" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 353:Generic Models 1" | names: "Generic Models 353:Generic Models 1:1849609" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 354:Generic Models 1" | names: "Generic Models 354:Generic Models 1:1850205" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 387:Generic Models 1" | names: "Generic Models 387:Generic Models 1:1850257" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 388:Generic Models 1" | names: "Generic Models 388:Generic Models 1:1850301" | material: "UL RATED FIRE STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 389:Generic Models 1" | names: "Generic Models 389:Generic Models 1:1850411" | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 390:Generic Models 1" | names: "Generic Models 390:Generic Models 1:1850535" | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 391:Generic Models 1" | names: "Generic Models 391:Generic Models 1:1850568" | material: "2X WOOD STUDS BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 392:Generic Models 1" | names: "Generic Models 392:Generic Models 1:1850653" | material: "2X WOOD STUDS BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 399:Generic Models 1" | names: "Generic Models 399:Generic Models 1:1850846" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 62:Generic Models 1" | names: "Generic Models 62:Generic Models 1:1850876" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 400:Generic Models 1" | names: "Generic Models 400:Generic Models 1:1850894" | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 401:Generic Models 1" | names: "Generic Models 401:Generic Models 1:1850912" | material: "CONDUIT/PIPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 405:Generic Models 1" | names: "Generic Models 405:Generic Models 1:1851094" | material: "UL RATED FIRE STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 406:Generic Models 1" | names: "Generic Models 406:Generic Models 1:1851126" | material: "CONDUIT/PIPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 407:Generic Models 1" | names: "Generic Models 407:Generic Models 1:1851151" | material: "UL RATED FIRE STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 409:Generic Models 1" | names: "Generic Models 409:Generic Models 1:1851602" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 352:Generic Models 1" | names: "Generic Models 352:Generic Models 1:1851677" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 410:Generic Models 1" | names: "Generic Models 410:Generic Models 1:1851747" | material: "HATCHED AREA" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 411:Generic Models 1" | names: "Generic Models 411:Generic Models 1:1852408" | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 561:Generic Models 1" | names: "Generic Models 561:Generic Models 1:2355825" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 453:Generic Models 1" | names: "Generic Models 453:Generic Models 1:2360995" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 502:Generic Models 1" | names: "Generic Models 502:Generic Models 1:2361008" | material: "OTHER WALL TYPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 530:Generic Models 1" | names: "Generic Models 530:Generic Models 1:2713353" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
      IFCBUILDINGSTOREY "1ST FLOOR (RENAME, BUT DON'T DELETE THIS LEVEL)" | long name "1ST FLOOR (RENAME, BUT DON'T DELETE THIS LEVEL)" | object type "Level:Project Base Point" | elevation 0.
        contains 556 elements
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 15:Generic Models 1" | names: "Generic Models 15:Generic Models 1:426780" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 17:Generic Models 1" | names: "Generic Models 17:Generic Models 1:426800" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 20:Generic Models 1" | names: "Generic Models 20:Generic Models 1:426834" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 23:Generic Models 1" | names: "Generic Models 23:Generic Models 1:426865" | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 24:Generic Models 1" | names: "Generic Models 24:Generic Models 1:426875" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 1:Generic Models 1" | names: "Generic Models 1:Generic Models 1:582123" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 2:Generic Models 1" | names: "Generic Models 2:Generic Models 1:582133" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 3:Generic Models 1" | names: "Generic Models 3:Generic Models 1:582143" | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 5:Generic Models 1" | names: "Generic Models 5:Generic Models 1:582163" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 14:Generic Models 1" | names: "Generic Models 14:Generic Models 1:582243" | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 41:Generic Models 1" | names: "Generic Models 41:Generic Models 1:582283" | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 42:Generic Models 1" | names: "Generic Models 42:Generic Models 1:582293" | material: "MATCH EXISTING BASE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 49:Generic Models 1" | names: "Generic Models 49:Generic Models 1:582363" | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 52:Generic Models 65" | names: "Generic Models 52:Generic Models 65:587734" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 19:Generic Models 65" | names: "Generic Models 19:Generic Models 65:588926" | material: "METAL STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 122:Generic Models 1" | names: "Generic Models 122:Generic Models 1:609975" | material: "TOP METAL STUD TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 128:Generic Models 1" | names: "Generic Models 128:Generic Models 1:609985" | material: "STRUCTURAL DECK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 132:Generic Models 1" | names: "Generic Models 132:Generic Models 1:610005" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 134:Generic Models 1" | names: "Generic Models 134:Generic Models 1:610015" | material: "CEILING TRACK TO MATCH EXISTING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 136:Generic Models 1" | names: "Generic Models 136:Generic Models 1:610020" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 142:Generic Models 1" | names: "Generic Models 142:Generic Models 1:610035" | material: "CEILING TRACK TO MATCH EXISTING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 143:Generic Models 1" | names: "Generic Models 143:Generic Models 1:610045" | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 146:Generic Models 1" | names: "Generic Models 146:Generic Models 1:610055" | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 147:Generic Models 65" | names: "Generic Models 147:Generic Models 65:610068" | material: "METAL STUD (16" O.C.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 149:Generic Models 1" | names: "Generic Models 149:Generic Models 1:610088" | material: "ALUM. STOREFRONT W/ TEMPERED SINGLE GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 83:Generic Models 1" | names: "Generic Models 83:Generic Models 1:610098" | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 94:Generic Models 65" | names: "Generic Models 94:Generic Models 65:610108" | material: "DIAGONAL BRACING AS NECESSARY - ATTACH TO STRUCTURAL DECK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 46" | object type "Generic Models 97:Generic Models 46" | names: "Generic Models 97:Generic Models 46:610121" | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 98:Generic Models 1" | names: "Generic Models 98:Generic Models 1:610131" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 124:Generic Models 1" | names: "Generic Models 124:Generic Models 1:610141" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 46" | object type "Generic Models 126:Generic Models 46" | names: "Generic Models 126:Generic Models 46:610159" | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 135:Generic Models 1" | names: "Generic Models 135:Generic Models 1:610170" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 137:Generic Models 1" | names: "Generic Models 137:Generic Models 1:610180" | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 138:Generic Models 1" | names: "Generic Models 138:Generic Models 1:637141" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 16:Generic Models 1" | names: "Generic Models 16:Generic Models 1:637269" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 34:Generic Models 1" | names: "Generic Models 34:Generic Models 1:828799" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "1/2"" | object type "Anchor Bolt:1/2"" | names: "Anchor Bolt:1/2":829037" | material: "1/2" ANCHOR BOLTS (7" MIN. EMBED) AT 72" MIN O.C. SPACING (18" MAX. FROM CORNERS)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 43:Generic Models 65" | names: "Generic Models 43:Generic Models 65:829101" | material: "2X6s WOOD JOISTS - 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 46:Generic Models 1" | names: "Generic Models 46:Generic Models 1:829188" | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 51:Generic Models 1" | names: "Generic Models 51:Generic Models 1:829284" | material: "VINYL SIDING OVER AIR & MOISTURE BARRIER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 140:Generic Models 1" | names: "Generic Models 140:Generic Models 1:829357" | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 139:Generic Models 1" | names: "Generic Models 139:Generic Models 1:829521" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 152:Generic Models 1" | names: "Generic Models 152:Generic Models 1:833476" | material: "1/2" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 153:Generic Models 1" | names: "Generic Models 153:Generic Models 1:852181" | material: "SILL PLATE GASKET" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 181:Generic Models 65" | names: "Generic Models 181:Generic Models 65:854445" | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 154:Generic Models 1" | names: "Generic Models 154:Generic Models 1:855166" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 158:Generic Models 1" | names: "Generic Models 158:Generic Models 1:855467" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 159:Generic Models 1" | names: "Generic Models 159:Generic Models 1:855498" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 160:Generic Models 1" | names: "Generic Models 160:Generic Models 1:855513" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 161:Generic Models 1" | names: "Generic Models 161:Generic Models 1:855528" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 162:Generic Models 1" | names: "Generic Models 162:Generic Models 1:855543" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 163:Generic Models 1" | names: "Generic Models 163:Generic Models 1:855558" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 164:Generic Models 1" | names: "Generic Models 164:Generic Models 1:855573" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 165:Generic Models 1" | names: "Generic Models 165:Generic Models 1:855588" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 166:Generic Models 1" | names: "Generic Models 166:Generic Models 1:855603" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 167:Generic Models 1" | names: "Generic Models 167:Generic Models 1:855618" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 168:Generic Models 1" | names: "Generic Models 168:Generic Models 1:855633" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 169:Generic Models 1" | names: "Generic Models 169:Generic Models 1:855648" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 170:Generic Models 1" | names: "Generic Models 170:Generic Models 1:855663" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 171:Generic Models 1" | names: "Generic Models 171:Generic Models 1:855678" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 172:Generic Models 1" | names: "Generic Models 172:Generic Models 1:855693" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 173:Generic Models 1" | names: "Generic Models 173:Generic Models 1:855708" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 174:Generic Models 1" | names: "Generic Models 174:Generic Models 1:855723" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 175:Generic Models 1" | names: "Generic Models 175:Generic Models 1:855738" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 176:Generic Models 1" | names: "Generic Models 176:Generic Models 1:855753" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 179:Generic Models 1" | names: "Generic Models 179:Generic Models 1:855824" | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 180:Generic Models 65" | names: "Generic Models 180:Generic Models 65:856122" | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 197:Generic Models 1" | names: "Generic Models 197:Generic Models 1:1181065" | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 272:Generic Models 263" | names: "Generic Models 272:Generic Models 263:1384116" | material: "1.50" ASPHALT SURFACE COURSE (E-0.3)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 273:Generic Models 263" | names: "Generic Models 273:Generic Models 263:1384314" | material: "INSTALL TACK COAT PER WDOT SPECIFICATIONS IF LAYERS ARE NOT INSTALLED AT THE SAME TIME" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 263:Generic Models 263" | names: "Generic Models 263:Generic Models 263:1384500" | material: "1.50" ASPHALT BINDER COURSE (E-0.3)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 288:Generic Models 263" | names: "Generic Models 288:Generic Models 263:1387393" | material: "7" CONC. SIDE WALK, IF PRESENT (SEE SITE PLAN)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 304:Generic Models 263" | names: "Generic Models 304:Generic Models 263:1396625" | material: "1" EXPANSION JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 308:Generic Models 263" | names: "Generic Models 308:Generic Models 263:1400384" | material: "MEDIUM BROOM FINISH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 312:Generic Models 263" | names: "Generic Models 312:Generic Models 263:1402220" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 263" | object type "Generic Models 285:Generic Models 263" | names: "Generic Models 285:Generic Models 263:1403728" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 263" | object type "Generic Models 285:Generic Models 263" | names: "Generic Models 285:Generic Models 263:1451950" | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 356:Generic Models 65" | names: "Generic Models 356:Generic Models 65:1460408" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 360:Generic Models 65" | names: "Generic Models 360:Generic Models 65:1460526" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 366:Generic Models 65" | names: "Generic Models 366:Generic Models 65:1460740" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 384:Generic Models 1" | names: "Generic Models 384:Generic Models 1:1461889" | material: "STRUCTURAL DECK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Continuous Angle" | object type "Continuous Angle1:Continuous Angle" | names: "Continuous Angle1:Continuous Angle:1463390" | material: "L6X4X1/2 W/ 4" SLOT IN VERT. LOG FOR KWIK BOLT CENTER IN BLOCK (1/2" DIA. KWIK BOLT EXPANSION ANCHOR 2.25" EMBEDMENT AT 4FT O.C.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel:Dowel" | names: "Dowel:Dowel:1463972" | material: "6" CMU WALL W/#4 VERT. BARS AT 32" O.C. (TYP.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel1:Dowel" | names: "Dowel1:Dowel:1464093" | material: "6" CMU WALL W/#4 VERT. BARS AT 32" O.C. (TYP.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 426:Generic Models 1" | names: "Generic Models 426:Generic Models 1:1507267" | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 427:Generic Models 1" | names: "Generic Models 427:Generic Models 1:1507317" | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 429:Generic Models 1" | names: "Generic Models 429:Generic Models 1:1507517" | material: "3/4" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Pole" | object type "Pole:Pole" | names: "Pole:Pole:1510851" | material: "STEEL LIGHT POLE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Base Plate" | object type "Light Pole Base Plate:Light Pole Base Plate" | names: "Light Pole Base Plate:Light Pole Base Plate:1510904" | material: "STEEL BASE PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_1" Light Pole Anchor Bolt" | object type "060523 - W_P_C - Fastenings - Generic:_1" Light Pole Anchor Bolt" | names: "060523 - W_P_C - Fastenings - Generic:_1" Light Pole Anchor Bolt:1512772" | material: "5/8" GALV. ANCHOR BOLT @ 24" O.C. (6" MIN. EMBEDMENT)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_1" Light Pole Anchor Bolt" | object type "060523 - W_P_C - Fastenings - Generic:_1" Light Pole Anchor Bolt" | names: "060523 - W_P_C - Fastenings - Generic:_1" Light Pole Anchor Bolt:1512896" | material: "5/8" GALV. ANCHOR BOLT @ 24" O.C. (6" MIN. EMBEDMENT)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 32:Generic Models 1" | names: "Generic Models 32:Generic Models 1:1563609" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 287:Generic Models 65" | names: "Generic Models 287:Generic Models 65:1564528" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 293:Generic Models 65" | names: "Generic Models 293:Generic Models 65:1565394" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 346:Generic Models 65" | names: "Generic Models 346:Generic Models 65:1565428" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 350:Generic Models 65" | names: "Generic Models 350:Generic Models 65:1565497" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 355:Generic Models 65" | names: "Generic Models 355:Generic Models 65:1565531" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 358:Generic Models 1" | names: "Generic Models 358:Generic Models 1:1566354" | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 155:Generic Models 1" | names: "Generic Models 155:Generic Models 1:1566670" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 157:Generic Models 1" | names: "Generic Models 157:Generic Models 1:1566688" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 18:Generic Models 1" | names: "Generic Models 18:Generic Models 1:1566854" | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 6:Generic Models 1" | names: "Generic Models 6:Generic Models 1:1566942" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 10:Generic Models 1" | names: "Generic Models 10:Generic Models 1:1567002" | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 12:Generic Models 1" | names: "Generic Models 12:Generic Models 1:1567081" | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 9:Generic Models 1" | names: "Generic Models 9:Generic Models 1:1567282" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 13:Generic Models 1" | names: "Generic Models 13:Generic Models 1:1567312" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 25:Generic Models 1" | names: "Generic Models 25:Generic Models 1:1567317" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 228:Generic Models 1" | names: "Generic Models 228:Generic Models 1:1567337" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 245:Generic Models 1" | names: "Generic Models 245:Generic Models 1:1567372" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 246:Generic Models 1" | names: "Generic Models 246:Generic Models 1:1567387" | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 247:Generic Models 1" | names: "Generic Models 247:Generic Models 1:1567397" | material: "MATCH EXISTING BASE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 359:Generic Models 1" | names: "Generic Models 359:Generic Models 1:1567464" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 361:Generic Models 1" | names: "Generic Models 361:Generic Models 1:1567469" | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 364:Generic Models 1" | names: "Generic Models 364:Generic Models 1:1567501" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 368:Generic Models 1" | names: "Generic Models 368:Generic Models 1:1567528" | material: "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 370:Generic Models 1" | names: "Generic Models 370:Generic Models 1:1567562" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 371:Generic Models 1" | names: "Generic Models 371:Generic Models 1:1567595" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 375:Generic Models 1" | names: "Generic Models 375:Generic Models 1:1567753" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 376:Generic Models 1" | names: "Generic Models 376:Generic Models 1:1567763" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 377:Generic Models 1" | names: "Generic Models 377:Generic Models 1:1567773" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 378:Generic Models 1" | names: "Generic Models 378:Generic Models 1:1567783" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 29:Generic Models 1" | names: "Generic Models 29:Generic Models 1:1567832" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 362:Generic Models 1" | names: "Generic Models 362:Generic Models 1:1568068" | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 380:Generic Models 1" | names: "Generic Models 380:Generic Models 1:1568122" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 252:Generic Models 1" | names: "Generic Models 252:Generic Models 1:1568456" | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 434:Generic Models 1" | names: "Generic Models 434:Generic Models 1:1568846" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 436:Generic Models 1" | names: "Generic Models 436:Generic Models 1:1568967" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 437:Generic Models 1" | names: "Generic Models 437:Generic Models 1:1568984" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 438:Generic Models 1" | names: "Generic Models 438:Generic Models 1:1569050" | material: "2X NAILER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 439:Generic Models 1" | names: "Generic Models 439:Generic Models 1:1569101" | material: "2X NAILER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 442:Generic Models 1" | names: "Generic Models 442:Generic Models 1:1569205" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 443:Generic Models 1" | names: "Generic Models 443:Generic Models 1:1569271" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 372:Generic Models 1" | names: "Generic Models 372:Generic Models 1:1569322" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 435:Generic Models 1" | names: "Generic Models 435:Generic Models 1:1569461" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 444:Generic Models 1" | names: "Generic Models 444:Generic Models 1:1569466" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 445:Generic Models 1" | names: "Generic Models 445:Generic Models 1:1569476" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 449:Generic Models 1" | names: "Generic Models 449:Generic Models 1:1569511" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 450:Generic Models 1" | names: "Generic Models 450:Generic Models 1:1569526" | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 451:Generic Models 1" | names: "Generic Models 451:Generic Models 1:1569536" | material: "MATCH EXISTING BASE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 456:Generic Models 1" | names: "Generic Models 456:Generic Models 1:1569594" | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 457:Generic Models 1" | names: "Generic Models 457:Generic Models 1:1569615" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 460:Generic Models 1" | names: "Generic Models 460:Generic Models 1:1569645" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 461:Generic Models 1" | names: "Generic Models 461:Generic Models 1:1569658" | material: "1/2" GYP. BD. OR FINISH PLYWOOD (SEE INTERIOR ELEVATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 465:Generic Models 1" | names: "Generic Models 465:Generic Models 1:1569706" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 466:Generic Models 1" | names: "Generic Models 466:Generic Models 1:1569716" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 467:Generic Models 1" | names: "Generic Models 467:Generic Models 1:1569726" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 468:Generic Models 1" | names: "Generic Models 468:Generic Models 1:1569736" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 469:Generic Models 1" | names: "Generic Models 469:Generic Models 1:1569746" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 471:Generic Models 1" | names: "Generic Models 471:Generic Models 1:1569762" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 486:Generic Models 1" | names: "Generic Models 486:Generic Models 1:1569950" | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 487:Generic Models 1" | names: "Generic Models 487:Generic Models 1:1569974" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 488:Generic Models 1" | names: "Generic Models 488:Generic Models 1:1569981" | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 459:Generic Models 1" | names: "Generic Models 459:Generic Models 1:1570040" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 489:Generic Models 1" | names: "Generic Models 489:Generic Models 1:1571359" | material: "3.5" X 6" LVLs - 32" O.C. - EXPOSED - NO WOOD STAMPS - SEE STRUCT FOR DEPTH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 490:Generic Models 1" | names: "Generic Models 490:Generic Models 1:1571399" | material: "3.5" X 6" LVLs BLOCKING BETWEEN LVL JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 470:Generic Models 1" | names: "Generic Models 470:Generic Models 1:1571758" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 493:Generic Models 1" | names: "Generic Models 493:Generic Models 1:1571806" | material: "LVL RIM BOARD - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 472:Generic Models 1" | names: "Generic Models 472:Generic Models 1:1571883" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 455:Generic Models 1" | names: "Generic Models 455:Generic Models 1:1572450" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 479:Generic Models 1" | names: "Generic Models 479:Generic Models 1:1572503" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 484:Generic Models 1" | names: "Generic Models 484:Generic Models 1:1572705" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 485:Generic Models 1" | names: "Generic Models 485:Generic Models 1:1572715" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_3/4" x 4"" | object type "060523 - W_P_C - Fastenings - Generic:_3/4" x 4"" | names: "060523 - W_P_C - Fastenings - Generic:_3/4" x 4":1572967" | material: "EXPOSED LAG BOLTS - SEE STRUCT." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 21:Generic Models 1" | names: "Generic Models 21:Generic Models 1:1575228" | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 35:Generic Models 1" | names: "Generic Models 35:Generic Models 1:1575271" | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 36:Generic Models 1" | names: "Generic Models 36:Generic Models 1:1576960" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 67:Generic Models 1" | names: "Generic Models 67:Generic Models 1:1576965" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 242:Generic Models 1" | names: "Generic Models 242:Generic Models 1:1576975" | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 251:Generic Models 1" | names: "Generic Models 251:Generic Models 1:1576985" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 454:Generic Models 1" | names: "Generic Models 454:Generic Models 1:1577005" | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 503:Generic Models 1" | names: "Generic Models 503:Generic Models 1:1577075" | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 504:Generic Models 65" | names: "Generic Models 504:Generic Models 65:1577086" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 505:Generic Models 1" | names: "Generic Models 505:Generic Models 1:1577112" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 506:Generic Models 1" | names: "Generic Models 506:Generic Models 1:1577117" | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 508:Generic Models 1" | names: "Generic Models 508:Generic Models 1:1577149" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 509:Generic Models 1" | names: "Generic Models 509:Generic Models 1:1577160" | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 499:Generic Models 1" | names: "Generic Models 499:Generic Models 1:1577281" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 7:Generic Models 1" | names: "Generic Models 7:Generic Models 1:1577398" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 447:Generic Models 1" | names: "Generic Models 447:Generic Models 1:1577634" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 501:Generic Models 65" | names: "Generic Models 501:Generic Models 65:1577857" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 507:Generic Models 65" | names: "Generic Models 507:Generic Models 65:1577891" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 511:Generic Models 65" | names: "Generic Models 511:Generic Models 65:1577960" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 512:Generic Models 65" | names: "Generic Models 512:Generic Models 65:1577994" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 513:Generic Models 1" | names: "Generic Models 513:Generic Models 1:1578028" | material: "STRUCTURAL DECK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Continuous Angle" | object type "Continuous Angle2:Continuous Angle" | names: "Continuous Angle2:Continuous Angle:1578039" | material: "3" X 3" X 8" L. CLIP ANGLES @ 4'-0" O.C. MECH. FASTENED TO UNDERSIDE OF STRUCTURE OR SLAB - BOTH SIDES OF WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Continuous Angle" | object type "Continuous Angle3:Continuous Angle" | names: "Continuous Angle3:Continuous Angle:1578050" | material: "3" X 3" X 8" L. CLIP ANGLES @ 4'-0" O.C. MECH. FASTENED TO UNDERSIDE OF STRUCTURE OR SLAB - BOTH SIDES OF WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 515:Generic Models 65" | names: "Generic Models 515:Generic Models 65:1578102" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 516:Generic Models 65" | names: "Generic Models 516:Generic Models 65:1578139" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 517:Generic Models 65" | names: "Generic Models 517:Generic Models 65:1578173" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 519:Generic Models 65" | names: "Generic Models 519:Generic Models 65:1578242" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 520:Generic Models 65" | names: "Generic Models 520:Generic Models 65:1578276" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 521:Generic Models 1" | names: "Generic Models 521:Generic Models 1:1578306" | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 347:Generic Models 65" | names: "Generic Models 347:Generic Models 65:1578448" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 363:Generic Models 65" | names: "Generic Models 363:Generic Models 65:1578492" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 510:Generic Models 65" | names: "Generic Models 510:Generic Models 65:1578542" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 518:Generic Models 65" | names: "Generic Models 518:Generic Models 65:1578630" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 33:Generic Models 1" | names: "Generic Models 33:Generic Models 1:1579126" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 31:Generic Models 1" | names: "Generic Models 31:Generic Models 1:1579142" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 522:Generic Models 1" | names: "Generic Models 522:Generic Models 1:1579361" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 523:Generic Models 1" | names: "Generic Models 523:Generic Models 1:1579371" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 524:Generic Models 1" | names: "Generic Models 524:Generic Models 1:1579381" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 525:Generic Models 1" | names: "Generic Models 525:Generic Models 1:1579391" | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 526:Generic Models 1" | names: "Generic Models 526:Generic Models 1:1579401" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 531:Generic Models 65" | names: "Generic Models 531:Generic Models 65:1579452" | material: "METAL STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 532:Generic Models 1" | names: "Generic Models 532:Generic Models 1:1579457" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 533:Generic Models 1" | names: "Generic Models 533:Generic Models 1:1579462" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 534:Generic Models 1" | names: "Generic Models 534:Generic Models 1:1579472" | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 535:Generic Models 1" | names: "Generic Models 535:Generic Models 1:1579509" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 536:Generic Models 1" | names: "Generic Models 536:Generic Models 1:1579514" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 538:Generic Models 1" | names: "Generic Models 538:Generic Models 1:1579544" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 539:Generic Models 1" | names: "Generic Models 539:Generic Models 1:1579563" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 540:Generic Models 1" | names: "Generic Models 540:Generic Models 1:1579573" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 541:Generic Models 1" | names: "Generic Models 541:Generic Models 1:1579600" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 542:Generic Models 1" | names: "Generic Models 542:Generic Models 1:1579655" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 543:Generic Models 1" | names: "Generic Models 543:Generic Models 1:1579695" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 544:Generic Models 1" | names: "Generic Models 544:Generic Models 1:1579725" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 545:Generic Models 1" | names: "Generic Models 545:Generic Models 1:1579771" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 546:Generic Models 1" | names: "Generic Models 546:Generic Models 1:1579861" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 547:Generic Models 1" | names: "Generic Models 547:Generic Models 1:1579890" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 548:Generic Models 1" | names: "Generic Models 548:Generic Models 1:1579970" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 549:Generic Models 1" | names: "Generic Models 549:Generic Models 1:1582866" | material: "BOND BEAM W/ (1) CONT. #5 BAR CONT." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 369:Generic Models 1" | names: "Generic Models 369:Generic Models 1:1583302" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_1/2" x 3"" | object type "060523 - W_P_C - Fastenings - Generic:_1/2" x 3"" | names: "060523 - W_P_C - Fastenings - Generic:_1/2" x 3":1583615", "060523 - W_P_C - Fastenings - Generic:_1/2" x 3":1583627" | material: "1/2" DIA. A325 BOLT AT EACH PURLIN" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "_GROUND LUG" | object type "060523 - W_P_C - Fastenings - Generic:_GROUND LUG" | names: "060523 - W_P_C - Fastenings - Generic:_GROUND LUG:1587577" | material: "GROUND WIRE BOLTED TO POLE'S GROUND LUG" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 53:Generic Models 1" | names: "Generic Models 53:Generic Models 1:1601636" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel5:Dowel" | names: "Dowel5:Dowel:1614630" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 78:Generic Models 1" | names: "Generic Models 78:Generic Models 1:1614654" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel7:Dowel" | names: "Dowel7:Dowel:1614828" | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 91:Generic Models 1" | names: "Generic Models 91:Generic Models 1:1614869" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 96:Generic Models 1" | names: "Generic Models 96:Generic Models 1:1614983" | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 75:Generic Models 1" | names: "Generic Models 75:Generic Models 1:1615730" | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 76:Generic Models 1" | names: "Generic Models 76:Generic Models 1:1615830" | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel6:Dowel" | names: "Dowel6:Dowel:1615883" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 77:Generic Models 1" | names: "Generic Models 77:Generic Models 1:1616055" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 79:Generic Models 1" | names: "Generic Models 79:Generic Models 1:1616415" | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 80:Generic Models 1" | names: "Generic Models 80:Generic Models 1:1616542" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 81:Generic Models 1" | names: "Generic Models 81:Generic Models 1:1616646" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 82:Generic Models 1" | names: "Generic Models 82:Generic Models 1:1616792" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 84:Generic Models 1" | names: "Generic Models 84:Generic Models 1:1616808" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "5/8"" | object type "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8"" | names: "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8":1617861", "050523 - W_P_C - Fastenings - Bent Anchor Bolt:5/8":1618148" | material: "5/8” GALV. BENT ANCHOR BOLT @ 4’ O.C. (WITHIN 8” OF EVERY CORNER) 7” MIN. EMBEDMENT" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel8:Dowel" | names: "Dowel8:Dowel:1617962" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 85:Generic Models 1" | names: "Generic Models 85:Generic Models 1:1617969" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel9:Dowel" | names: "Dowel9:Dowel:1617989" | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 86:Generic Models 1" | names: "Generic Models 86:Generic Models 1:1617996" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 87:Generic Models 1" | names: "Generic Models 87:Generic Models 1:1618017" | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 88:Generic Models 1" | names: "Generic Models 88:Generic Models 1:1618032" | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 89:Generic Models 1" | names: "Generic Models 89:Generic Models 1:1618045" | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel10:Dowel" | names: "Dowel10:Dowel:1618061" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 90:Generic Models 1" | names: "Generic Models 90:Generic Models 1:1618070" | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 92:Generic Models 1" | names: "Generic Models 92:Generic Models 1:1618083" | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 95:Generic Models 1" | names: "Generic Models 95:Generic Models 1:1618109" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 99:Generic Models 1" | names: "Generic Models 99:Generic Models 1:1618126" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 100:Generic Models 1" | names: "Generic Models 100:Generic Models 1:1618136" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 101:Generic Models 1" | names: "Generic Models 101:Generic Models 1:1618681" | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 102:Generic Models 1" | names: "Generic Models 102:Generic Models 1:1618883" | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 103:Generic Models 1" | names: "Generic Models 103:Generic Models 1:1619141" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 104:Generic Models 1" | names: "Generic Models 104:Generic Models 1:1619290" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 105:Generic Models 1" | names: "Generic Models 105:Generic Models 1:1619338" | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 113:Generic Models 65" | names: "Generic Models 113:Generic Models 65:1619487" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 114:Generic Models 65" | names: "Generic Models 114:Generic Models 65:1619509" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel13:Dowel" | names: "Dowel13:Dowel:1619577" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 118:Generic Models 65" | names: "Generic Models 118:Generic Models 65:1619584" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 119:Generic Models 65" | names: "Generic Models 119:Generic Models 65:1619606" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 120:Generic Models 1" | names: "Generic Models 120:Generic Models 1:1619618" | material: "REINFORCEMENT GROUTED INTO BROKEN CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 106:Generic Models 65" | names: "Generic Models 106:Generic Models 65:1619787" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 108:Generic Models 65" | names: "Generic Models 108:Generic Models 65:1619799" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 109:Generic Models 65" | names: "Generic Models 109:Generic Models 65:1619830" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 110:Generic Models 65" | names: "Generic Models 110:Generic Models 65:1619842" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 111:Generic Models 65" | names: "Generic Models 111:Generic Models 65:1619877" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 107:Generic Models 65" | names: "Generic Models 107:Generic Models 65:1620157" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 112:Generic Models 65" | names: "Generic Models 112:Generic Models 65:1620169" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 115:Generic Models 65" | names: "Generic Models 115:Generic Models 65:1620201" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 116:Generic Models 65" | names: "Generic Models 116:Generic Models 65:1620213" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 117:Generic Models 1" | names: "Generic Models 117:Generic Models 1:1620261" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 121:Generic Models 1" | names: "Generic Models 121:Generic Models 1:1621614" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 123:Generic Models 1" | names: "Generic Models 123:Generic Models 1:1621813" | material: "#3 J's @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 127:Generic Models 1" | names: "Generic Models 127:Generic Models 1:1622300" | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 130:Generic Models 65" | names: "Generic Models 130:Generic Models 65:1622309" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel11:Dowel" | names: "Dowel11:Dowel:1622333" | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 131:Generic Models 65" | names: "Generic Models 131:Generic Models 65:1622340" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 133:Generic Models 1" | names: "Generic Models 133:Generic Models 1:1622357" | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel12:Dowel" | names: "Dowel12:Dowel:1622372" | material: "#4 J's @ 24" O.C. - GROUTED IN PRECAST KEYS AND CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 182:Generic Models 65" | names: "Generic Models 182:Generic Models 65:1622384" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 185:Generic Models 1" | names: "Generic Models 185:Generic Models 1:1622400" | material: "SOLID CMU AS NEEDED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 186:Generic Models 65" | names: "Generic Models 186:Generic Models 65:1622412" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 187:Generic Models 1" | names: "Generic Models 187:Generic Models 1:1622429" | material: "SOLID CMU AS NEEDED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 188:Generic Models 65" | names: "Generic Models 188:Generic Models 65:1622441" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 189:Generic Models 65" | names: "Generic Models 189:Generic Models 65:1622463" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 190:Generic Models 1" | names: "Generic Models 190:Generic Models 1:1622477" | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 191:Generic Models 65" | names: "Generic Models 191:Generic Models 65:1622486" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 192:Generic Models 65" | names: "Generic Models 192:Generic Models 65:1622508" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Dowel" | object type "Dowel14:Dowel" | names: "Dowel14:Dowel:1622531" | material: "#4 REBARS @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 193:Generic Models 65" | names: "Generic Models 193:Generic Models 65:1622538" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 194:Generic Models 65" | names: "Generic Models 194:Generic Models 65:1622560" | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 195:Generic Models 1" | names: "Generic Models 195:Generic Models 1:1622572" | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 196:Generic Models 65" | names: "Generic Models 196:Generic Models 65:1622594" | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 198:Generic Models 65" | names: "Generic Models 198:Generic Models 65:1622616" | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 199:Generic Models 1" | names: "Generic Models 199:Generic Models 1:1622628" | material: "GROUT CORES AT REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 200:Generic Models 1" | names: "Generic Models 200:Generic Models 1:1622654" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 201:Generic Models 1" | names: "Generic Models 201:Generic Models 1:1622672" | material: "(2) #5's" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 202:Generic Models 1" | names: "Generic Models 202:Generic Models 1:1622682" | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 203:Generic Models 1" | names: "Generic Models 203:Generic Models 1:1622696" | material: "(2) #5's" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 139:Generic Models 1" | names: "Generic Models 139:Generic Models 1:1622725" | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 55:Generic Models 1" | names: "Generic Models 55:Generic Models 1:1622967" | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 56:Generic Models 1" | names: "Generic Models 56:Generic Models 1:1623516" | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 219:Generic Models 1" | names: "Generic Models 219:Generic Models 1:1633873" | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 220:Generic Models 1" | names: "Generic Models 220:Generic Models 1:1633886" | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 222:Generic Models 1" | names: "Generic Models 222:Generic Models 1:1633912" | material: "3/4" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 227:Generic Models 1" | names: "Generic Models 227:Generic Models 1:1633977" | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 232:Generic Models 1" | names: "Generic Models 232:Generic Models 1:1651569" | material: "EXISTING FLOOR SUBSTRATE - MIN 19/32 THICK WOOD STRUCTURAL PANELS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 236:Generic Models 1" | names: "Generic Models 236:Generic Models 1:1651764" | material: "EXISTING FLOOR SUBSTRATE - 1 X 4 T&G LAID PERPENDICULAR TO JOISTS, OR 19/32" PLYWOOD WOOD STRUCTURAL PANELS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 264:Generic Models 1" | names: "Generic Models 264:Generic Models 1:1652093" | material: "EXISTING FLOOR SUBSTRATE - 15/32" THICK PLYWOOD OR 7/16" THICK ORIENTATED STRAND BOARD (OSB) WOOD STRUCTURAL PANELS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 320:Generic Models 1" | names: "Generic Models 320:Generic Models 1:1712872" | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 323:Generic Models 1" | names: "Generic Models 323:Generic Models 1:1712877" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 324:Generic Models 1" | names: "Generic Models 324:Generic Models 1:1712887" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 325:Generic Models 1" | names: "Generic Models 325:Generic Models 1:1712897" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 327:Generic Models 1" | names: "Generic Models 327:Generic Models 1:1712912" | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 65" | object type "Generic Models 328:Generic Models 65" | names: "Generic Models 328:Generic Models 65:1712927" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 329:Generic Models 1" | names: "Generic Models 329:Generic Models 1:1712951" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 330:Generic Models 1" | names: "Generic Models 330:Generic Models 1:1712956" | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 331:Generic Models 1" | names: "Generic Models 331:Generic Models 1:1712977" | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 332:Generic Models 1" | names: "Generic Models 332:Generic Models 1:1712988" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 333:Generic Models 1" | names: "Generic Models 333:Generic Models 1:1712994" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 334:Generic Models 1" | names: "Generic Models 334:Generic Models 1:1713023" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 335:Generic Models 1" | names: "Generic Models 335:Generic Models 1:1713033" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 336:Generic Models 1" | names: "Generic Models 336:Generic Models 1:1713051" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 337:Generic Models 1" | names: "Generic Models 337:Generic Models 1:1713061" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 338:Generic Models 1" | names: "Generic Models 338:Generic Models 1:1713077" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 339:Generic Models 1" | names: "Generic Models 339:Generic Models 1:1713083" | material: "IF SHEAR WALL - WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 340:Generic Models 1" | names: "Generic Models 340:Generic Models 1:1713096" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 341:Generic Models 1" | names: "Generic Models 341:Generic Models 1:1713106" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 556:Generic Models 1" | names: "Generic Models 556:Generic Models 1:1713116" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 567:Generic Models 1" | names: "Generic Models 567:Generic Models 1:1713134" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 571:Generic Models 1" | names: "Generic Models 571:Generic Models 1:1713139" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 577:Generic Models 1" | names: "Generic Models 577:Generic Models 1:1713149" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 590:Generic Models 1" | names: "Generic Models 590:Generic Models 1:1713167" | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 558:Generic Models 1" | names: "Generic Models 558:Generic Models 1:1713172" | material: "IF SHEAR WALL - WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 81:Structural Framing 1" | names: "Structural Framing 81:Structural Framing 1:1773330" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 82:Structural Framing 1" | names: "Structural Framing 82:Structural Framing 1:1773340" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 108:Structural Framing 1" | names: "Structural Framing 108:Structural Framing 1:1773350" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 109:Structural Framing 1" | names: "Structural Framing 109:Structural Framing 1:1773360" | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 110:Structural Framing 1" | names: "Structural Framing 110:Structural Framing 1:1773370" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 111:Structural Framing 1" | names: "Structural Framing 111:Structural Framing 1:1773380" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 112:Structural Framing 2" | names: "Structural Framing 112:Structural Framing 2:1773393" | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 114:Structural Framing 1" | names: "Structural Framing 114:Structural Framing 1:1773410" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 115:Structural Framing 1" | names: "Structural Framing 115:Structural Framing 1:1773421" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 116:Structural Framing 1" | names: "Structural Framing 116:Structural Framing 1:1773432" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 117:Structural Framing 1" | names: "Structural Framing 117:Structural Framing 1:1773443" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 118:Structural Framing 1" | names: "Structural Framing 118:Structural Framing 1:1773454" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 119:Structural Framing 1" | names: "Structural Framing 119:Structural Framing 1:1773465" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 120:Structural Framing 1" | names: "Structural Framing 120:Structural Framing 1:1773476" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 121:Structural Framing 2" | names: "Structural Framing 121:Structural Framing 2:1773516" | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 123:Structural Framing 1" | names: "Structural Framing 123:Structural Framing 1:1773531" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 124:Structural Framing 1" | names: "Structural Framing 124:Structural Framing 1:1773541" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 125:Structural Framing 1" | names: "Structural Framing 125:Structural Framing 1:1773551" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 126:Structural Framing 1" | names: "Structural Framing 126:Structural Framing 1:1773561" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 127:Structural Framing 1" | names: "Structural Framing 127:Structural Framing 1:1773571" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 128:Structural Framing 1" | names: "Structural Framing 128:Structural Framing 1:1773581" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 129:Structural Framing 1" | names: "Structural Framing 129:Structural Framing 1:1773591" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 130:Structural Framing 2" | names: "Structural Framing 130:Structural Framing 2:1773630" | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 132:Structural Framing 1" | names: "Structural Framing 132:Structural Framing 1:1773645" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 133:Structural Framing 1" | names: "Structural Framing 133:Structural Framing 1:1773655" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 134:Structural Framing 1" | names: "Structural Framing 134:Structural Framing 1:1773665" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 135:Structural Framing 1" | names: "Structural Framing 135:Structural Framing 1:1773675" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 136:Structural Framing 1" | names: "Structural Framing 136:Structural Framing 1:1773685" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 137:Structural Framing 1" | names: "Structural Framing 137:Structural Framing 1:1773695" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 139:Structural Framing 1" | names: "Structural Framing 139:Structural Framing 1:1773740" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 140:Structural Framing 7" | names: "Structural Framing 140:Structural Framing 7:1773754" | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 37:Structural Framing 7" | names: "Structural Framing 37:Structural Framing 7:1773764" | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 141:Structural Framing 7" | names: "Structural Framing 141:Structural Framing 7:1773775" | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 142:Structural Framing 7" | names: "Structural Framing 142:Structural Framing 7:1773785" | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 143:Structural Framing 2" | names: "Structural Framing 143:Structural Framing 2:1773795" | material: "SILL STUD" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 144:Structural Framing 2" | names: "Structural Framing 144:Structural Framing 2:1773804" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 145:Structural Framing 1" | names: "Structural Framing 145:Structural Framing 1:1773810" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 146:Structural Framing 1" | names: "Structural Framing 146:Structural Framing 1:1773820" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 147:Structural Framing 1" | names: "Structural Framing 147:Structural Framing 1:1773830" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 148:Structural Framing 1" | names: "Structural Framing 148:Structural Framing 1:1773840" | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 149:Structural Framing 1" | names: "Structural Framing 149:Structural Framing 1:1773850" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 150:Structural Framing 1" | names: "Structural Framing 150:Structural Framing 1:1773860" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 151:Structural Framing 1" | names: "Structural Framing 151:Structural Framing 1:1773870" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 152:Structural Framing 1" | names: "Structural Framing 152:Structural Framing 1:1773880" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 153:Structural Framing 1" | names: "Structural Framing 153:Structural Framing 1:1773890" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 154:Structural Framing 1" | names: "Structural Framing 154:Structural Framing 1:1773900" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 155:Structural Framing 2" | names: "Structural Framing 155:Structural Framing 2:1773913" | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 156:Structural Framing 1" | names: "Structural Framing 156:Structural Framing 1:1773919" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 157:Structural Framing 1" | names: "Structural Framing 157:Structural Framing 1:1773929" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 158:Structural Framing 1" | names: "Structural Framing 158:Structural Framing 1:1773939" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 159:Structural Framing 1" | names: "Structural Framing 159:Structural Framing 1:1773949" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 160:Structural Framing 7" | names: "Structural Framing 160:Structural Framing 7:1773962" | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 161:Structural Framing 7" | names: "Structural Framing 161:Structural Framing 7:1773971" | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 162:Structural Framing 7" | names: "Structural Framing 162:Structural Framing 7:1773980" | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 163:Structural Framing 7" | names: "Structural Framing 163:Structural Framing 7:1773989" | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 164:Structural Framing 7" | names: "Structural Framing 164:Structural Framing 7:1773998" | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 165:Structural Framing 7" | names: "Structural Framing 165:Structural Framing 7:1774007" | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 166:Structural Framing 2" | names: "Structural Framing 166:Structural Framing 2:1774016" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 167:Structural Framing 1" | names: "Structural Framing 167:Structural Framing 1:1774022" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 168:Structural Framing 7" | names: "Structural Framing 168:Structural Framing 7:1774035" | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 169:Structural Framing 7" | names: "Structural Framing 169:Structural Framing 7:1774044" | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | object type "Structural Framing 170:Structural Framing 7" | names: "Structural Framing 170:Structural Framing 7:1774053" | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 171:Structural Framing 1" | names: "Structural Framing 171:Structural Framing 1:1774059" | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
      IFCBUILDINGSTOREY "2ND FLOOR" | long name "2ND FLOOR" | object type "Level:Project Base Point" | elevation 10.0000000000002
        contains 61 elements
          1 x IFCWALL | type IFCWALLTYPE "Light Pole Luminaire" | object type "Light Pole Luminaire:Light Pole Luminaire" | names: "Light Pole Luminaire:Light Pole Luminaire:1513850" | material: "LUMINAIRE HOUSING AS SPECIFIED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 243:Generic Models 1" | names: "Generic Models 243:Generic Models 1:1567367" | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 248:Generic Models 1" | names: "Generic Models 248:Generic Models 1:1567407" | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 365:Generic Models 1" | names: "Generic Models 365:Generic Models 1:1567512" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 373:Generic Models 1" | names: "Generic Models 373:Generic Models 1:1567700" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 367:Generic Models 1" | names: "Generic Models 367:Generic Models 1:1567716" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 374:Generic Models 1" | names: "Generic Models 374:Generic Models 1:1567726" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 379:Generic Models 1" | names: "Generic Models 379:Generic Models 1:1568544" | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 382:Generic Models 1" | names: "Generic Models 382:Generic Models 1:1568585" | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 381:Generic Models 1" | names: "Generic Models 381:Generic Models 1:1568658" | material: "2X WOOD SILL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 383:Generic Models 1" | names: "Generic Models 383:Generic Models 1:1568679" | material: "1" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 385:Generic Models 1" | names: "Generic Models 385:Generic Models 1:1568750" | material: "1" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 440:Generic Models 1" | names: "Generic Models 440:Generic Models 1:1569136" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 441:Generic Models 1" | names: "Generic Models 441:Generic Models 1:1569178" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 475:Generic Models 1" | names: "Generic Models 475:Generic Models 1:1569824" | material: "2X WOOD SILL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 476:Generic Models 1" | names: "Generic Models 476:Generic Models 1:1569829" | material: "19"/32" FINISH GRADE PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 477:Generic Models 1" | names: "Generic Models 477:Generic Models 1:1569842" | material: "1" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 478:Generic Models 1" | names: "Generic Models 478:Generic Models 1:1569855" | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 491:Generic Models 1" | names: "Generic Models 491:Generic Models 1:1571538" | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 492:Generic Models 1" | names: "Generic Models 492:Generic Models 1:1571583" | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 474:Generic Models 1" | names: "Generic Models 474:Generic Models 1:1571647" | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE - NO STAMPS - EXPOSED TO FINISH SPACE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 473:Generic Models 1" | names: "Generic Models 473:Generic Models 1:1571933" | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 448:Generic Models 1" | names: "Generic Models 448:Generic Models 1:1572049" | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 452:Generic Models 1" | names: "Generic Models 452:Generic Models 1:1572213" | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 458:Generic Models 1" | names: "Generic Models 458:Generic Models 1:1572226" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 462:Generic Models 1" | names: "Generic Models 462:Generic Models 1:1572298" | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 463:Generic Models 1" | names: "Generic Models 463:Generic Models 1:1572311" | material: "1/2" GYP. BD. OR FINISH PLYWOOD (SEE INTERIOR ELEVATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 464:Generic Models 1" | names: "Generic Models 464:Generic Models 1:1572359" | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 480:Generic Models 1" | names: "Generic Models 480:Generic Models 1:1572521" | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 481:Generic Models 1" | names: "Generic Models 481:Generic Models 1:1572564" | material: "FLOOR FINISH T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 482:Generic Models 1" | names: "Generic Models 482:Generic Models 1:1572617" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 483:Generic Models 1" | names: "Generic Models 483:Generic Models 1:1572641" | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 494:Generic Models 1" | names: "Generic Models 494:Generic Models 1:1572795" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 495:Generic Models 1" | names: "Generic Models 495:Generic Models 1:1572805" | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 496:Generic Models 1" | names: "Generic Models 496:Generic Models 1:1574821" | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          6 x IFCBUILDINGELEMENTPROXY | object type "Model Text:OD_Very Large" | names: "Model Text:OD_Very Large:1594948", "Model Text:OD_Very Large:1594962", "Model Text:OD_Very Large:1594972" (+3 more) | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 125:Generic Models 1" | names: "Generic Models 125:Generic Models 1:1773303" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 113:Structural Framing 2" | names: "Structural Framing 113:Structural Framing 2:1773402" | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 205:Generic Models 1" | names: "Generic Models 205:Generic Models 1:1773486" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 122:Structural Framing 2" | names: "Structural Framing 122:Structural Framing 2:1773525" | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 207:Generic Models 1" | names: "Generic Models 207:Generic Models 1:1773600" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 131:Structural Framing 2" | names: "Structural Framing 131:Structural Framing 2:1773639" | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 209:Generic Models 1" | names: "Generic Models 209:Generic Models 1:1773704" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 138:Structural Framing 2" | names: "Structural Framing 138:Structural Framing 2:1773734" | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 74:Generic Models 1" | names: "Generic Models 74:Generic Models 1:1775660" | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCWALL | type IFCWALLTYPE "Generic Models 1" | object type "Generic Models 93:Generic Models 1" | names: "Generic Models 93:Generic Models 1:1775673" | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 12:Structural Framing 1" | names: "Structural Framing 12:Structural Framing 1:1775694" | material: "BEND DOWN FLANGE OF METAL TRACK - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 13:Structural Framing 2" | names: "Structural Framing 13:Structural Framing 2:1775703" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 14:Structural Framing 2" | names: "Structural Framing 14:Structural Framing 2:1775712" | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 15:Structural Framing 2" | names: "Structural Framing 15:Structural Framing 2:1775721" | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 16:Structural Framing 2" | names: "Structural Framing 16:Structural Framing 2:1775730" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 17:Structural Framing 2" | names: "Structural Framing 17:Structural Framing 2:1775739" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | object type "Structural Framing 18:Structural Framing 2" | names: "Structural Framing 18:Structural Framing 2:1775748" | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 19:Structural Framing 1" | names: "Structural Framing 19:Structural Framing 1:1775754" | material: "VERTICAL METAL CRIPPLE STUD BEYOND" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 21:Structural Framing 1" | names: "Structural Framing 21:Structural Framing 1:1775764" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | object type "Structural Framing 22:Structural Framing 1" | names: "Structural Framing 22:Structural Framing 1:1775774" | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff

Types
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING SLAB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#10 6x6 WIRE MESH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6 MIL VAPOR BARRIER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "6" COMPACTED CRUSHED STONE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GRADE (SLOPE 2% MIN AWAY FROM BUILDING)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL WOOD COLUMN - SIZE TBD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 155" | 1 occurrence | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 184" | 1 occurrence | material: "GRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "EXISTING PAVEMENT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "COMPACTED SUBGRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "5" MIN. COMPACTED BASE AGGREGATE UNDER CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "3" TO 6" WASHED OR CLEAR STONE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "6" CRUSHED AGGREGATE BASE COURSE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "PAVING SURFACE (TYP.) SEE PLANS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "CRUSHED AGGREGATE BASE COURSE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "7" CONC. DRIVE APPROACH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "SLOPED - 7" CONC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "GRADED BACKFILL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "GRADED BACKFILL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "EXISTING GRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE PAVEMENT HEAVY DUTY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "8" CRUSHED 1.25" AGGREGATE BASE COURSE (COMPACTED)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "COMPACTED SUBGRADE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "EPOXY COATED 6 X 6 X W2.9 X W2.9, PLACED 3" ABOVE SLAB BASE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "SLOPED - 7" CONC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "1" EXPANSION JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 263" | 1 occurrence | material: "CONCRETE CURB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "R-19 BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Ground Rod" | 1 occurrence | material: "5/8" x 8' GROUND ROD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate" | 1 occurrence | material: "(4) VERTICAL #6 REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate" | 1 occurrence | material: "STEEL BASE PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Walls 126" | 1 occurrence | material: "24" DIA. CONCRETE POLE BASE WITH THOROSEAL FINISH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Walls 126" | 1 occurrence | material: "Earth" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OTHER WALL TYPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate" | 1 occurrence | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate" | 1 occurrence | material: "1 1/2" GAVL. STEEL (RGS) CONDUIT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE (3000 PSI CONCRETE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#10 6x6 WIRE MESH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 12" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "R-19 BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING (SHALL BEAR THE UL CERTIFICATION MARK)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NOMINAL 3/4" THICK, 48" WIDE GYPSUM BOARD - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - FORMED FROM MIN. 25 MSG GALV. STEEL SPACED MAX 24" O.C. PERPENDICULAR TO JOISTS - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT SOUND ISOLATION ACCESSORY SHALL BE USED AT EACH ATTACHMENT POINT OF THE RESILIENT CHANNELS AND SPACED MAX 16" O.C. - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GALV. STEEL WITH TOTAL AREA OF DUCT OPENING NOT TO EXCEED 113 SQ. IN. PER 100 SQ. FT. OF CEILING AREA, AREA OF INDIVIDUAL DUCT OPENING NOT TO EXCEED 113 SQ. IN. MAX. DIMENSION OF OPENING 12" - SEE UL ..." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "20" X 48"/60" OR 24" X 48" - MAX OF 16 SQ FT PER 100 SQ FT OF CEILING AREA - OR - INCANDESCENT LAMP TYPE 6.5" DIA. X 7-1/2" HIGH - (4) FIXTURES PER 100 SQ FT OF CEILING AREA (USE FIXTURE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL MATERIAL - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GYPSUM BOARD — 5/8" X 4 FT WIDE GYPSUM BOARD, INSTALLED WITH LONG DIMENSION PERPENDICULAR TO CROSS TEES WITH SIDE JOINTS CENTERED ALONG MAIN RUNNERS." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GLASS FIBER OR MINERAL WOOL INSULATION BEARING THE UL CLASSIFICATION MARKING AS TO SURFACE BURNING CHARACTERISTICS AND/OR FIRE RESISTANCE - SEE UL LISTING FOR ADDITIONAL INFORMATION - FILL CAVITY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - 2X WOOD JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "AIR DUCT — MIN 0.029 IN. THICK (22 GAUGE) GALV STEEL AIR DUCT. TOTAL AREA OF DUCT OPENINGS NOT TO EXCEED 114 SQ IN. PER EACH 100 SQ FT OF CEILING AREA." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2' x 4' RECESSED LIGHT FIXTURE WITH STEEL HOUSING AND 'FIXTURE PROTECTION' - SPACED TO NOT EXCEED 24 SQ FT PER 100 SQ FT OF CEILING AREA - SEE UL LISTING FOR MORE INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING - FLOOR BRIDGING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NOM 2 BY 4 IN. INSTALLED BETWEEN AND PERPENDICULAR TO WOOD JOISTS, AND CENTERED 5 IN. BELOW SUBFLOORING." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "NO. 12 SWG GALV. STEEL WIRE, SUPPORTED FROM 16D NAILS DRIVEN THROUGH WOOD JOISTS 5" FROM BOTTOM OF JOISTS AND BENT UPWARD AT BOTH ENDS FOR POSITIVE SUPPORT - SEE UL LISTING FOR ADDITIONAL INFORMATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FIXTURE PROTECTION (IF NON-RATED FIXTURE) - SEE UL LISTING FOR SPECIFICS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STEEL FRAMING MEMBERS - SEE UL LISTING FOR RANGE OF OPTIONS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE & REBAR)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BREAK EVERY OTHER REBAR AT JOINT (TOP AND BOTTOM REBAR TO BE CONT.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" DEEP NOTCH AT EACH SIDE OF WALL (SPACE APART - 25FT MIN.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONDUIT/PIPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "7/8" FURRING CHANNELS @ 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONDUIT/PIPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONDUIT/PIPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "HATCHED AREA" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CAVITY WITH BATT INSULATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OTHER WALL TYPE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MATCH EXISTING BASE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "METAL STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOP METAL STUD TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL DECK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK TO MATCH EXISTING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK TO MATCH EXISTING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "METAL STUD (16" O.C.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED SINGLE GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "DIAGONAL BRACING AS NECESSARY - ATTACH TO STRUCTURAL DECK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 46" | 1 occurrence | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 46" | 1 occurrence | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEALANT (W/ BACKER ROD IF NECESSARY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "1/2"" | 1 occurrence | material: "1/2" ANCHOR BOLTS (7" MIN. EMBED) AT 72" MIN O.C. SPACING (18" MAX. FROM CORNERS)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "2X6s WOOD JOISTS - 16" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/2" CDX PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VINYL SIDING OVER AIR & MOISTURE BARRIER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/2" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SILL PLATE GASKET" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "VERTICAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "HORIZONTAL 1X6 CEDAR PLANKS W/ CLEAR WOOD SEALER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "1.50" ASPHALT SURFACE COURSE (E-0.3)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "INSTALL TACK COAT PER WDOT SPECIFICATIONS IF LAYERS ARE NOT INSTALLED AT THE SAME TIME" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "1.50" ASPHALT BINDER COURSE (E-0.3)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "7" CONC. SIDE WALK, IF PRESENT (SEE SITE PLAN)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "1" EXPANSION JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "MEDIUM BROOM FINISH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 263" | 1 occurrence | material: "SEE SITE PLAN FOR LANDSCAPING" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL DECK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Continuous Angle" | 1 occurrence | material: "L6X4X1/2 W/ 4" SLOT IN VERT. LOG FOR KWIK BOLT CENTER IN BLOCK (1/2" DIA. KWIK BOLT EXPANSION ANCHOR 2.25" EMBEDMENT AT 4FT O.C.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "6" CMU WALL W/#4 VERT. BARS AT 32" O.C. (TYP.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "6" CMU WALL W/#4 VERT. BARS AT 32" O.C. (TYP.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Pole" | 1 occurrence | material: "STEEL LIGHT POLE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Light Pole Base Plate" | 1 occurrence | material: "STEEL BASE PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "_1" Light Pole Anchor Bolt" | 1 occurrence | material: "5/8" GALV. ANCHOR BOLT @ 24" O.C. (6" MIN. EMBEDMENT)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_1" Light Pole Anchor Bolt" | 1 occurrence | material: "5/8" GALV. ANCHOR BOLT @ 24" O.C. (6" MIN. EMBEDMENT)" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MATCH EXISTING BASE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X NAILER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X NAILER" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "MATCH EXISTING BASE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/2" GYP. BD. OR FINISH PLYWOOD (SEE INTERIOR ELEVATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3.5" X 6" LVLs - 32" O.C. - EXPOSED - NO WOOD STAMPS - SEE STRUCT FOR DEPTH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3.5" X 6" LVLs BLOCKING BETWEEN LVL JOISTS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "LVL RIM BOARD - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "_3/4" x 4"" | 1 occurrence | material: "EXPOSED LAG BOLTS - SEE STRUCT." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD TRUSS FLOOR ASSEMBLY - FILL CAVITY WITH BATT. INSULATION - (UL - L521 FLOOR ASSEMBLY)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL DECK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Continuous Angle" | 1 occurrence | material: "3" X 3" X 8" L. CLIP ANGLES @ 4'-0" O.C. MECH. FASTENED TO UNDERSIDE OF STRUCTURE OR SLAB - BOTH SIDES OF WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Continuous Angle" | 1 occurrence | material: "3" X 3" X 8" L. CLIP ANGLES @ 4'-0" O.C. MECH. FASTENED TO UNDERSIDE OF STRUCTURE OR SLAB - BOTH SIDES OF WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "METAL STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BOND BEAM W/ (1) CONT. #5 BAR CONT." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "_1/2" x 3"" | 2 occurrences | material: "1/2" DIA. A325 BOLT AT EACH PURLIN" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_GROUND LUG" | 1 occurrence | material: "GROUND WIRE BOLTED TO POLE'S GROUND LUG" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "5/8"" | 2 occurrences | material: "5/8” GALV. BENT ANCHOR BOLT @ 4’ O.C. (WITHIN 8” OF EVERY CORNER) 7” MIN. EMBEDMENT" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4 x 16" BAR @ 2-0" O.C. MAX. DRILL THRU HOLLOWCORE OR KEYWAY & INTO CIP WALL W/ 4" MIN. EMBED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONCRETE FOUNDATION - (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TREATED 2X SILL PLATE - SEE STRUCT. SCHEDULES FOR SIZE - ATTACH WITH" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR IN TOPPING SLAB" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 VERTICAL U-SHAPED HAIRPINS AT 18" O.C. - 36" LONG" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 HORZ. U-SHAPED HAIRPINS - 36" LONG - LOOP AROUND VERT. HAIRPIN" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS - SEE STRUCT SCHEDULE FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FILL CORE IF APPLICABLE - SEE STRUCTURAL DWGS FOR DETAILS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "REINFORCEMENT GROUTED INTO BROKEN CORE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#3 J's @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "PRECAST PLANK - SEE PRECAST SHOPS FOR SIZE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BEARING STRIP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4 J's @ 24" O.C. - GROUTED IN PRECAST KEYS AND CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOLID CMU AS NEEDED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOLID CMU AS NEEDED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SEE SCHEDULE FOR FILLED CORES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Dowel" | 1 occurrence | material: "#4 REBARS @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CMU (SEE 'WALL TAG' FOR SIZE)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3" CONCRETE TOPPING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "GROUT CORES AT REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONT. KNOCK OUT BOND BEAM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "(2) #5's" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "#4 CONT. STEEL REBAR" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "4x4 - W4.0xW4.0 WWM - OVERLAP 8" AT SPLICES" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL REINFORCING - SEE PLAN SCHEDULES FOR SIZE/LOCATION" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING FLOOR SUBSTRATE - MIN 19/32 THICK WOOD STRUCTURAL PANELS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING FLOOR SUBSTRATE - 1 X 4 T&G LAID PERPENDICULAR TO JOISTS, OR 19/32" PLYWOOD WOOD STRUCTURAL PANELS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING FLOOR SUBSTRATE - 15/32" THICK PLYWOOD OR 7/16" THICK ORIENTATED STRAND BOARD (OSB) WOOD STRUCTURAL PANELS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "IF SHEAR WALL - WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "IF SHEAR WALL - WOOD STRUCTURAL PANEL (WSP) - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING TO BRIDGE AT LEAST (3) VERTICAL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "SILL STUD" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "CRIPPLE STUD OR CLIP ANGLE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 7" | 1 occurrence | material: "BLOCKING @ DOOR HINGE LOCATIONS - EXTEND TO AT LEAST (3) VERT. STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL SILL CHANNEL - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "TYP. VERTICAL METAL STUD - SEE WALL TAG FOR SPACING AND GUAGE" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "TOP METAL STUD TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "METAL STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "METAL STUD BRACE TO DECK AS NECESSARY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL CEILING TRACK/TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL CEILING TRACK/TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FIRE TREATED BLOCKING - SIZE AS NECESSARY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "_METAL STUD - HEAD - GENERIC" | 1 occurrence | material: "AT HEAD FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_METAL STUD - HEAD - GENERIC" | 1 occurrence | material: "AT HEAD FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ALUM. STOREFRONT W/ TEMPERED SINGLE GLAZING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "MORTAR JOINT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "OPEN WEB WOOD TRUSS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD @ CEILING" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SINGLE 2X WOOD SILL - TREATED IF CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUDS BEYOND" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UL RATED FIRE STOP" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL CEILING TRACK/TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL CEILING TRACK/TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "BLOCKING - SIZE AS NEC." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "EXISTING ACOUSTICAL TILE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "J BEAD DRYWALL TRIM" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "_WOOD STUD - SILL - GENERIC" | 6 occurrences | material: "AT SILL - FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "WOOD STUD BRACE TO DECK AS NECESSARY" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "_Genric Fastener" | 1 occurrence | material: "AT SILL - FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_Genric Fastener" | 1 occurrence | material: "AT SILL - FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DEEP LEG OF DEFLECTION TRACK (2" MIN. DEFLECTION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "METAL STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X BLOCKING - LOCATED AT GRAB BARS, WALL HUNG CABINETS, ETC.)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "_METAL STUD - SILL - GENERIC" | 4 occurrences | material: "AT SILL - FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_WOOD STUD - DRYWALL - GENERIC" | 2 occurrences | material: "DRYWALL SCREW" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_WOOD STUD - DRYWALL - GENERIC" | 3 occurrences | material: "DRYWALL SCREW" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_WOOD STUD - DRYWALL - GENERIC" | 2 occurrences | material: "DRYWALL SCREW" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_WOOD STUD - DRYWALL - GENERIC" | 2 occurrences | material: "DRYWALL SCREW" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_METAL STUD - DRYWALL - GENERIC" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_METAL STUD - DRYWALL - GENERIC" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_METAL STUD - DRYWALL - GENERIC" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_METAL STUD - DRYWALL - GENERIC" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "_METAL STUD - HEAD - GENERIC" | 3 occurrences | material: "AT HEAD FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL - TREATED IF ON CONCRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL RUNNER CHANNEL; FASTEN @ 24" O.C." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 65" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "DOUBLE 2X WOOD TOP PLATE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ACOUSTICAL SEALANT OR FIRE SEALANT, IF RATED WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING TRACK AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CEILING AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Light Pole Luminaire" | 1 occurrence | material: "LUMINAIRE HOUSING AS SPECIFIED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "ATTACH GYPSUM BOARD TO STUDS AND NOT TO TOP TRACK" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "LADDER TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD SILL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "19"/32" FINISH GRADE PLYWOOD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1" GYP. CRETE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "2X WOOD STUD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "19"/32" OSB PLYWOOD BONDED W/ EXT. GLUE - NO STAMPS - EXPOSED TO FINISH SPACE" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WOOD TRUSS - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "5/8" GYP. BD" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "1/2" GYP. BD. OR FINISH PLYWOOD (SEE INTERIOR ELEVATIONS)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "RESILIENT CHANNEL - 25 GA. FURRING CHANNELS INSTALLED HORIZONTALLY SPACED 24 IN. OC" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "SOUND MAT" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "FLOOR FINISH T.B.D" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "WALL BASE AS SCHEDULED" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "CONTINUOUS FIRE RATED SEALANT EACH SIDE." | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL TRACK CHANNEL @ HEAD - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "UNDERSIDE OF FLOOR ASSEMBLY - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCWALLTYPE "Generic Models 1" | 1 occurrence | material: "STRUCTURAL FLOOR - SEE STRUCT. DWGS" | property sets: Pset_ProductRequirements, Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "BEND DOWN FLANGE OF METAL TRACK - FASTENER PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "(2) BOXED STUDS - SAME SIZE AS WALL STUDS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2" | 1 occurrence | material: "METAL STUD TRACK WELDED OR SCREWED PER MANU. REQUIREMENTS" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "VERTICAL METAL CRIPPLE STUD BEYOND" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 1" | 1 occurrence | material: "DOUBLE UP METAL STUDS @ JAMB" | property sets: Pset_BuildingElementProxyCommon, Pset_ProductRequirements, Pset_QuantityTakeOff

Property sets
  Pset_ProductRequirements | properties | on 679 objects (654 IFCWALL, 25 IFCOPENINGELEMENT) | on 654 type objects
    Category = "Walls" (IFCLABEL)
  Pset_ProductRequirements | properties | on 92 objects (92 IFCBUILDINGELEMENTPROXY) | on 92 type objects
    Category = "Structural Framing" (IFCLABEL)
  Pset_ProductRequirements | properties | on 37 objects (37 IFCBUILDINGELEMENTPROXY) | on 21 type objects
    Category = "Structural Connections" (IFCLABEL)
  Pset_ProductRequirements | properties | on 17 objects (17 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Category = "Generic Models" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "BASEMENT (RENAME, BUT DON'T DELETE THIS LEVEL)" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "1ST FLOOR (RENAME, BUT DON'T DELETE THIS LEVEL)" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "2ND FLOOR" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 523 objects (523 IFCWALL) | on 523 type objects
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 87 objects (63 IFCWALL, 24 IFCOPENINGELEMENT) | on 63 type objects
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 51 objects (51 IFCBUILDINGELEMENTPROXY) | on 51 type objects
    Reference = "Structural Framing 1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 42 objects (39 IFCWALL, 3 IFCBUILDINGELEMENTPROXY) | on 42 type objects
    Reference = "Generic Models 263" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 28 objects (28 IFCBUILDINGELEMENTPROXY) | on 28 type objects
    Reference = "Structural Framing 2" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY) | on 13 type objects
    Reference = "Structural Framing 7" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCWALL) | on 12 type objects
    Reference = "Dowel" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Reference = "OD_Very Large" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 21 more contents on 57 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 523 objects (523 IFCWALL) | on 523 type objects
    Reference = "Generic Models 1" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 63 objects (63 IFCWALL) | on 63 type objects
    Reference = "Generic Models 65" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 39 objects (39 IFCWALL) | on 39 type objects
    Reference = "Generic Models 263" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 12 objects (12 IFCWALL) | on 12 type objects
    Reference = "Dowel" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 5 objects (5 IFCWALL) | on 5 type objects
    Reference = "Light Pole Base Plate" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 3 objects (3 IFCWALL) | on 3 type objects
    Reference = "Continuous Angle" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALL) | on 2 type objects
    Reference = "Generic Models 46" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALL) | on 2 type objects
    Reference = "Walls 126" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall: 5 more contents on 5 objects not shown
  Pset_WallCommon | properties | on 523 objects (523 IFCWALL) | on 523 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 1" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 63 objects (63 IFCWALL) | on 63 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 39 objects (39 IFCWALL) | on 39 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 263" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 12 objects (12 IFCWALL) | on 12 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Dowel" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 5 objects (5 IFCWALL) | on 5 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Light Pole Base Plate" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 3 objects (3 IFCWALL) | on 3 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Continuous Angle" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL) | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Generic Models 46" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL) | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Walls 126" (IFCIDENTIFIER)
  Pset_WallCommon: 5 more contents on 5 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 51 objects (51 IFCBUILDINGELEMENTPROXY) | on 51 type objects
    Reference = "Structural Framing 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 28 objects (28 IFCBUILDINGELEMENTPROXY) | on 28 type objects
    Reference = "Structural Framing 2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 13 objects (13 IFCBUILDINGELEMENTPROXY) | on 13 type objects
    Reference = "Structural Framing 7" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY)
    Reference = "OD_Very Large" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Reference = "_WOOD STUD - DRYWALL - GENERIC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "_WOOD STUD - SILL - GENERIC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 5 objects (5 IFCBUILDINGELEMENTPROXY) | on 3 type objects
    Reference = "_METAL STUD - HEAD - GENERIC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY) | on 4 type objects
    Reference = "_METAL STUD - DRYWALL - GENERIC" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 9 more contents on 18 objects not shown
  Pset_OpeningElementCommon | properties | on 24 objects (24 IFCOPENINGELEMENT)
    Reference = "Generic Models 65" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 1 object (1 IFCOPENINGELEMENT)
    Reference = "Ground Rod" (IFCIDENTIFIER)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "BASEMENT (RENAME, BUT DON'T DELETE THIS LEVEL)" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "1ST FLOOR (RENAME, BUT DON'T DELETE THIS LEVEL)" (IFCLABEL)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "2ND FLOOR" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 3 objects (3 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 3 (IFCINTEGER)

Other addresses and roles
  2 x postal address: "**ADDRESS OF PROJECT**", "<Default>"