IFC building model
Schema: "IFC4"
Description: "ViewDefinition [DesignTransferView_V1.0]"
File name: "Project Number"
Time stamp: "2022-11-08T17:53:39"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.3.3.0 - Alternate UI 20.3.3.0"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "ryan@openingdesign.com" of Organization (no name given)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1667949735 (2022-11-08T23:22:15Z)

Units
  LENGTHUNIT: FOOT (conversion based)
  AREAUNIT: SQUARE FOOT (conversion based)
  VOLUMEUNIT: CUBIC FOOT (conversion based)
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "MARCO POLO" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 100.
    IFCBUILDING | postal address: "101 W 33RD STREET - CITY OF BRYAN TOWNSITE, BLOCK 96, LOT 3-5 & PT OF 6 & PT OF ALLEY - BRYAN, TX 77803", "<Default>"
      IFCBUILDINGSTOREY "BASEMENT" | long name "BASEMENT" | object type "Level:Project Base Point" | elevation -12.6666666666667
        contains 4 elements
          1 x IFCFOOTING | type IFCFOOTINGTYPE "Wall Foundation:UNDER LANDSCAPE WALLS" | object type "Wall Foundation:UNDER LANDSCAPE WALLS" | STRIP_FOOTING | names: "Wall Foundation:UNDER LANDSCAPE WALLS:4315419" | material: "CONCRETE FOOTING - SEE SCHEDULE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FootingCommon, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCFOOTINGTYPE "Wall Foundation:UNDER LANDSCAPE WALLS" | object type "Wall Foundation:UNDER LANDSCAPE WALLS" | STRIP_FOOTING | names: "Wall Foundation:UNDER LANDSCAPE WALLS:4315435" | material: "CONCRETE FOOTING - SEE SCHEDULE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FootingCommon, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCFOOTINGTYPE "Wall Foundation:UNDER LANDSCAPE WALLS" | object type "Wall Foundation:UNDER LANDSCAPE WALLS" | STRIP_FOOTING | names: "Wall Foundation:UNDER LANDSCAPE WALLS:4315451" | material: "CONCRETE FOOTING - SEE SCHEDULE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FootingCommon, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
          1 x IFCFOOTING | type IFCFOOTINGTYPE "Wall Foundation:UNDER LANDSCAPE WALLS" | object type "Wall Foundation:UNDER LANDSCAPE WALLS" | STRIP_FOOTING | names: "Wall Foundation:UNDER LANDSCAPE WALLS:4586578" | material: "CONCRETE FOOTING - SEE SCHEDULE" | property sets: Pset_EnvironmentalImpactIndicators, Pset_FootingCommon, Pset_ReinforcementBarCountOfIndependentFooting, Pset_ReinforcementBarPitchOfContinuousFooting
      IFCBUILDINGSTOREY "1ST FLOOR" | long name "1ST FLOOR" | object type "Level:Project Base Point" | elevation 0.
        contains 352 elements
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:3651721" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:3654220" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 6X6X3/8" | object type "HSS-Hollow Structural Section-Column:HSS 6X6X3/8" | COLUMN | names: "HSS-Hollow Structural Section-Column:HSS 6X6X3/8:3654361" | material: profiles "HSS 6X6X3/8" ("HSS 6X6X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:3981294" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4003615" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4003624" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4003626" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4003828" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4003837" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4003839" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4003951" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4003960" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4003962" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8" | object type "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8" | COLUMN | names: "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8:4009173", "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8:4410107", "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8:4410282" (+3 more) | material: profiles "HSS 5.5X5.5X3/8" ("HSS 5.5X5.5X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 9:Structural Framing 9" | object type "Structural Framing 9:Structural Framing 9" | names: "Structural Framing 9:Structural Framing 9:4058362" | material: "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8" | object type "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8" | COLUMN | names: "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8:4121300" | material: profiles "HSS 5.5X5.5X3/8" ("HSS 5.5X5.5X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4122313" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4122413" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4177760" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4228511" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4238194" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4245135" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4309330" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 6X6X3/8" | object type "HSS-Hollow Structural Section-Column:HSS 6X6X3/8" | COLUMN | names: "HSS-Hollow Structural Section-Column:HSS 6X6X3/8:4369599" | material: profiles "HSS 6X6X3/8" ("HSS 6X6X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4370944" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4371225" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4371599", "061100 - Wood Framing:(3)-2X8:4371630" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4371615" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4371645" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4371660" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4371732" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4371751" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4371768" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4371785" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4371804" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4372891" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4372910" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4372925" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4372946" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4372961" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4372976" | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4374082" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4374096" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4374113" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4374132" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4374149" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4374164" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          3 x IFCBEAM | type IFCBEAMTYPE "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4"" | object type "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4"" | BEAM | names: "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4":4375456", "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4":4375469", "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4":4375540" | material: profiles "GL - 3 1/2" X 11 1/4"" ("GL - 3 1/2" X 11 1/4"": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4376406", "061100 - Wood Framing:(3)-2X8:4376771" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4376486" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4376787" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4376802" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4376817", "061100 - Wood Framing:(3)-2X8:4377091" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4377735" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4377750" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4377771" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4377792" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4377807" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378598" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378621" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378636" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378649" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378662" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378675" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378733", "061100 - Wood Framing:(3)2X6:4378802" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378746" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378761" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378774" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4378787" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          4 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | object type "061100 - Wood Framing:(3)-2X12" | BEAM | names: "061100 - Wood Framing:(3)-2X12:4380877", "061100 - Wood Framing:(3)-2X12:4380892", "061100 - Wood Framing:(3)-2X12:4380986" (+1 more) | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4385346", "061100 - Wood Framing:(3)2X6:4385942" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4385502" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4385515" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          3 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4385910", "061100 - Wood Framing:(3)2X6:4385993", "061100 - Wood Framing:(3)2X6:4386010" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4385927" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4385978" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4386027" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4387452" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4387467" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4387895" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4387910" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4387927" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4387942" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4387961" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4387978" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4387993" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4388008" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4388023" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4388040" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4389653" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4390150" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4390535" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | object type "061100 - Wood Framing:(3)-2X8" | BEAM | names: "061100 - Wood Framing:(3)-2X8:4390584" | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4400046", "C-Channel:C15x33.9, TYP.:4400236" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4407171" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X8 - JOIST" | object type "061100 - Wood Framing:2X8 - JOIST" | BEAM | names: "061100 - Wood Framing:2X8 - JOIST:4408534" | material: profiles "2X8 - JOIST" ("2X8 - JOIST": "BOTTOM CHORD OF FIELD FRAMED OVERHANG") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4423975" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 29:Structural Framing 9" | object type "Structural Framing 29:Structural Framing 9" | names: "Structural Framing 29:Structural Framing 9:4431102" | material: "TREATED 2X LEDGER - EXT. STAIN" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X8 - JOIST" | object type "061100 - Wood Framing:2X8 - JOIST" | BEAM | names: "061100 - Wood Framing:2X8 - JOIST:4442757" | material: profiles "2X8 - JOIST" ("2X8 - JOIST": "BOTTOM CHORD OF FIELD FRAMED OVERHANG") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X8 - JOIST" | object type "061100 - Wood Framing:2X8 - JOIST" | BEAM | names: "061100 - Wood Framing:2X8 - JOIST:4442863" | material: profiles "2X8 - JOIST" ("2X8 - JOIST": "BOTTOM CHORD OF FIELD FRAMED OVERHANG") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6":4451701" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6":4452591" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4468435" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4468437" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4468440" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4468443" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4468446" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4468448" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4468779" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4468794" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4468894" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4468910" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4469311" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4469384" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4469608" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4470358" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | object type "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | names: "061100 - Wood Framing:2X4 - BLOCKING:4470462" | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x50, TYP." | object type "C-Channel:C15x50, TYP." | BEAM | names: "C-Channel:C15x50, TYP.:4485396" | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x50, TYP." | object type "C-Channel:C15x50, TYP." | BEAM | names: "C-Channel:C15x50, TYP.:4485865" | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "Dimension Lumber - Truncated:(2) 2X8 @ ROOF EDGE" | object type "Dimension Lumber - Truncated:(2) 2X8 @ ROOF EDGE" | BEAM | names: "Dimension Lumber - Truncated:(2) 2X8 @ ROOF EDGE:4486653", "Dimension Lumber - Truncated:(2) 2X8 @ ROOF EDGE:4491245" | material: profiles "(2) 2X8 @ ROOF EDGE" ("(2) 2X8 @ ROOF EDGE": "TREATED 2X JOISTS - EXT. STAIN") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4"" | object type "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4"" | BEAM | names: "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4":4491078" | material: profiles "GL - 3 1/2" X 11 1/4"" ("GL - 3 1/2" X 11 1/4"": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | object type "061100 - Wood Framing:(3)2X6" | BEAM | names: "061100 - Wood Framing:(3)2X6:4492336", "061100 - Wood Framing:(3)2X6:4492703" | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X8 - OUTRIGGER" | object type "061100 - Wood Framing:2X8 - OUTRIGGER" | BEAM | names: "061100 - Wood Framing:2X8 - OUTRIGGER:4494729" | material: profiles "2X8 - OUTRIGGER" ("2X8 - OUTRIGGER": "2X8 OUTRIGGER - SISTER TO ROOF TRUSSES") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2X8 - OUTRIGGER" | object type "061100 - Wood Framing:2X8 - OUTRIGGER" | BEAM | names: "061100 - Wood Framing:2X8 - OUTRIGGER:4496076" | material: profiles "2X8 - OUTRIGGER" ("2X8 - OUTRIGGER": "2X8 OUTRIGGER - SISTER TO ROOF TRUSSES") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Timber-Column:(4) 2X6 - BUILT-UP COLUMN" | object type "Timber-Column:(4) 2X6 - BUILT-UP COLUMN" | COLUMN | names: "Timber-Column:(4) 2X6 - BUILT-UP COLUMN:4497989", "Timber-Column:(4) 2X6 - BUILT-UP COLUMN:4498133", "Timber-Column:(4) 2X6 - BUILT-UP COLUMN:4498182" (+1 more) | material: profiles "(4) 2X6 - BUILT-UP COLUMN" ("(4) 2X6 - BUILT-UP COLUMN": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6":4503448" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6":4503622" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5':4503784" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6":4503915" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5':4504039" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6":4504223" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5':4504320" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6":4504438" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5':4504574" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6":4504778" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5':4504859" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6":4505023" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5':4505204" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | object type "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | names: "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5':4505334" | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfSlab, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 8X8X3/8" | object type "HSS-Hollow Structural Section-Column:HSS 8X8X3/8" | COLUMN | names: "HSS-Hollow Structural Section-Column:HSS 8X8X3/8:4510977" | material: profiles "HSS 8X8X3/8" ("HSS 8X8X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          6 x IFCCOLUMN | type IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 8X8X3/8" | object type "HSS-Hollow Structural Section-Column:HSS 8X8X3/8" | COLUMN | names: "HSS-Hollow Structural Section-Column:HSS 8X8X3/8:4511074", "HSS-Hollow Structural Section-Column:HSS 8X8X3/8:4511210", "HSS-Hollow Structural Section-Column:HSS 8X8X3/8:4511218" (+3 more) | material: profiles "HSS 8X8X3/8" ("HSS 8X8X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4515443" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | object type "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | BEAM | names: "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE):4555461" | material: profiles "2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" ("2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4563352" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2X8" | object type "061100 - Wood Framing:(2) 2X8" | BEAM | names: "061100 - Wood Framing:(2) 2X8:4601764", "061100 - Wood Framing:(2) 2X8:4602105" | material: profiles "(2) 2X8" ("(2) 2X8": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2X8" | object type "061100 - Wood Framing:(2) 2X8" | BEAM | names: "061100 - Wood Framing:(2) 2X8:4611927" | material: profiles "(2) 2X8" ("(2) 2X8": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2X8" | object type "061100 - Wood Framing:(2) 2X8" | BEAM | names: "061100 - Wood Framing:(2) 2X8:4612402" | material: profiles "(2) 2X8" ("(2) 2X8": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8" | object type "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8" | COLUMN | names: "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8:4630404" | material: profiles "HSS 5.5X5.5X3/8" ("HSS 5.5X5.5X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4630971" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4630973" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4630975" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4634376" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4634383" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x50, TYP." | object type "C-Channel:C15x50, TYP." | BEAM | names: "C-Channel:C15x50, TYP.:4641845" | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x50, TYP." | object type "C-Channel:C15x50, TYP." | BEAM | names: "C-Channel:C15x50, TYP.:4641854" | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x50, TYP." | object type "C-Channel:C15x50, TYP." | BEAM | names: "C-Channel:C15x50, TYP.:4642037" | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x50, TYP." | object type "C-Channel:C15x50, TYP." | BEAM | names: "C-Channel:C15x50, TYP.:4642044" | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4642187" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x50, TYP." | object type "C-Channel:C15x50, TYP." | BEAM | names: "C-Channel:C15x50, TYP.:4642263" | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x50, TYP." | object type "C-Channel:C15x50, TYP." | BEAM | names: "C-Channel:C15x50, TYP.:4642270" | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4642801" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4642834" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4642850" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4642857" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647131" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647146" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647354" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647358" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647368" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647372" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647382" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647386" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647396" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4647400" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4651751" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4651830" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4651836" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4651842" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4651848" | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | object type "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | BEAM | names: "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE):4653147" | material: profiles "2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" ("2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | object type "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | BEAM | names: "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE):4653213" | material: profiles "2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" ("2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | object type "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | BEAM | names: "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE):4653240" | material: profiles "2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" ("2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4666545" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4666664" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4668628" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4668663" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4669573" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4669575" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4669899" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4669901" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4676451" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4676453" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4677176" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4677184" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4677186" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4679001" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4679004" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4679007" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4679009" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4679333" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4679335" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4679337" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4679339" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4961862" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:4961898" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 985:Generic Models 629" | object type "Generic Models 985:Generic Models 629" | names: "Generic Models 985:Generic Models 629:5008280" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 986:Generic Models 629" | object type "Generic Models 986:Generic Models 629" | names: "Generic Models 986:Generic Models 629:5009664" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 987:Generic Models 629" | object type "Generic Models 987:Generic Models 629" | names: "Generic Models 987:Generic Models 629:5009745" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 988:Generic Models 629" | object type "Generic Models 988:Generic Models 629" | names: "Generic Models 988:Generic Models 629:5009798" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 989:Generic Models 629" | object type "Generic Models 989:Generic Models 629" | names: "Generic Models 989:Generic Models 629:5009851" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 990:Generic Models 629" | object type "Generic Models 990:Generic Models 629" | names: "Generic Models 990:Generic Models 629:5009904" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 991:Generic Models 629" | object type "Generic Models 991:Generic Models 629" | names: "Generic Models 991:Generic Models 629:5009957" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 992:Generic Models 629" | object type "Generic Models 992:Generic Models 629" | names: "Generic Models 992:Generic Models 629:5010010" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 993:Generic Models 629" | object type "Generic Models 993:Generic Models 629" | names: "Generic Models 993:Generic Models 629:5010063" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 994:Generic Models 629" | object type "Generic Models 994:Generic Models 629" | names: "Generic Models 994:Generic Models 629:5010116" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 995:Generic Models 629" | object type "Generic Models 995:Generic Models 629" | names: "Generic Models 995:Generic Models 629:5010169" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 996:Generic Models 629" | object type "Generic Models 996:Generic Models 629" | names: "Generic Models 996:Generic Models 629:5010222" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 997:Generic Models 629" | object type "Generic Models 997:Generic Models 629" | names: "Generic Models 997:Generic Models 629:5010275" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 998:Generic Models 629" | object type "Generic Models 998:Generic Models 629" | names: "Generic Models 998:Generic Models 629:5010328" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 734:Generic Models 629" | object type "Generic Models 734:Generic Models 629" | names: "Generic Models 734:Generic Models 629:5010381" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 999:Generic Models 629" | object type "Generic Models 999:Generic Models 629" | names: "Generic Models 999:Generic Models 629:5010434" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1000:Generic Models 629" | object type "Generic Models 1000:Generic Models 629" | names: "Generic Models 1000:Generic Models 629:5010487" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1001:Generic Models 629" | object type "Generic Models 1001:Generic Models 629" | names: "Generic Models 1001:Generic Models 629:5010540" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5017545" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5017589" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5027996" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5028036" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5029936" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5029980" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5030128" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5030172" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5171784" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | object type "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | names: "061100 - Wood Framing:(2) 2x12 - RIM JOIST:5171862" | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 925:Generic Models 629" | object type "Generic Models 925:Generic Models 629" | names: "Generic Models 925:Generic Models 629:5217417" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 927:Generic Models 629" | object type "Generic Models 927:Generic Models 629" | names: "Generic Models 927:Generic Models 629:5217435" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 928:Generic Models 629" | object type "Generic Models 928:Generic Models 629" | names: "Generic Models 928:Generic Models 629:5217454" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 929:Generic Models 629" | object type "Generic Models 929:Generic Models 629" | names: "Generic Models 929:Generic Models 629:5217472" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 930:Generic Models 629" | object type "Generic Models 930:Generic Models 629" | names: "Generic Models 930:Generic Models 629:5217491" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 931:Generic Models 629" | object type "Generic Models 931:Generic Models 629" | names: "Generic Models 931:Generic Models 629:5217509" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 932:Generic Models 629" | object type "Generic Models 932:Generic Models 629" | names: "Generic Models 932:Generic Models 629:5217528" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 933:Generic Models 629" | object type "Generic Models 933:Generic Models 629" | names: "Generic Models 933:Generic Models 629:5217546" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 934:Generic Models 629" | object type "Generic Models 934:Generic Models 629" | names: "Generic Models 934:Generic Models 629:5217565" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 935:Generic Models 629" | object type "Generic Models 935:Generic Models 629" | names: "Generic Models 935:Generic Models 629:5217583" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 936:Generic Models 629" | object type "Generic Models 936:Generic Models 629" | names: "Generic Models 936:Generic Models 629:5217602" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 937:Generic Models 629" | object type "Generic Models 937:Generic Models 629" | names: "Generic Models 937:Generic Models 629:5217620" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 938:Generic Models 629" | object type "Generic Models 938:Generic Models 629" | names: "Generic Models 938:Generic Models 629:5217639" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 939:Generic Models 629" | object type "Generic Models 939:Generic Models 629" | names: "Generic Models 939:Generic Models 629:5217657" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 940:Generic Models 629" | object type "Generic Models 940:Generic Models 629" | names: "Generic Models 940:Generic Models 629:5217676" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 941:Generic Models 629" | object type "Generic Models 941:Generic Models 629" | names: "Generic Models 941:Generic Models 629:5217694" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 942:Generic Models 629" | object type "Generic Models 942:Generic Models 629" | names: "Generic Models 942:Generic Models 629:5217713" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 943:Generic Models 629" | object type "Generic Models 943:Generic Models 629" | names: "Generic Models 943:Generic Models 629:5217731" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 944:Generic Models 629" | object type "Generic Models 944:Generic Models 629" | names: "Generic Models 944:Generic Models 629:5217750" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 945:Generic Models 629" | object type "Generic Models 945:Generic Models 629" | names: "Generic Models 945:Generic Models 629:5217768" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 947:Generic Models 629" | object type "Generic Models 947:Generic Models 629" | names: "Generic Models 947:Generic Models 629:5217787" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 948:Generic Models 629" | object type "Generic Models 948:Generic Models 629" | names: "Generic Models 948:Generic Models 629:5217805" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 949:Generic Models 629" | object type "Generic Models 949:Generic Models 629" | names: "Generic Models 949:Generic Models 629:5217824" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 952:Generic Models 629" | object type "Generic Models 952:Generic Models 629" | names: "Generic Models 952:Generic Models 629:5217842" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 953:Generic Models 629" | object type "Generic Models 953:Generic Models 629" | names: "Generic Models 953:Generic Models 629:5217861" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 954:Generic Models 629" | object type "Generic Models 954:Generic Models 629" | names: "Generic Models 954:Generic Models 629:5217879" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 955:Generic Models 629" | object type "Generic Models 955:Generic Models 629" | names: "Generic Models 955:Generic Models 629:5217898" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 956:Generic Models 629" | object type "Generic Models 956:Generic Models 629" | names: "Generic Models 956:Generic Models 629:5217916" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 957:Generic Models 629" | object type "Generic Models 957:Generic Models 629" | names: "Generic Models 957:Generic Models 629:5217935" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 958:Generic Models 629" | object type "Generic Models 958:Generic Models 629" | names: "Generic Models 958:Generic Models 629:5217953" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 959:Generic Models 629" | object type "Generic Models 959:Generic Models 629" | names: "Generic Models 959:Generic Models 629:5217972" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 960:Generic Models 629" | object type "Generic Models 960:Generic Models 629" | names: "Generic Models 960:Generic Models 629:5217990" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 961:Generic Models 629" | object type "Generic Models 961:Generic Models 629" | names: "Generic Models 961:Generic Models 629:5218009" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 962:Generic Models 629" | object type "Generic Models 962:Generic Models 629" | names: "Generic Models 962:Generic Models 629:5218027" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 963:Generic Models 629" | object type "Generic Models 963:Generic Models 629" | names: "Generic Models 963:Generic Models 629:5218046" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 964:Generic Models 629" | object type "Generic Models 964:Generic Models 629" | names: "Generic Models 964:Generic Models 629:5218064" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 782:Generic Models 629" | object type "Generic Models 782:Generic Models 629" | names: "Generic Models 782:Generic Models 629:5294244" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 783:Generic Models 629" | object type "Generic Models 783:Generic Models 629" | names: "Generic Models 783:Generic Models 629:5294262" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 784:Generic Models 629" | object type "Generic Models 784:Generic Models 629" | names: "Generic Models 784:Generic Models 629:5294284" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 785:Generic Models 629" | object type "Generic Models 785:Generic Models 629" | names: "Generic Models 785:Generic Models 629:5294302" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 786:Generic Models 629" | object type "Generic Models 786:Generic Models 629" | names: "Generic Models 786:Generic Models 629:5294320" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 787:Generic Models 629" | object type "Generic Models 787:Generic Models 629" | names: "Generic Models 787:Generic Models 629:5294338" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 788:Generic Models 629" | object type "Generic Models 788:Generic Models 629" | names: "Generic Models 788:Generic Models 629:5294356" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 789:Generic Models 629" | object type "Generic Models 789:Generic Models 629" | names: "Generic Models 789:Generic Models 629:5294374" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 790:Generic Models 629" | object type "Generic Models 790:Generic Models 629" | names: "Generic Models 790:Generic Models 629:5294392" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 791:Generic Models 629" | object type "Generic Models 791:Generic Models 629" | names: "Generic Models 791:Generic Models 629:5294410" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 792:Generic Models 629" | object type "Generic Models 792:Generic Models 629" | names: "Generic Models 792:Generic Models 629:5294428" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 793:Generic Models 629" | object type "Generic Models 793:Generic Models 629" | names: "Generic Models 793:Generic Models 629:5294446" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 794:Generic Models 629" | object type "Generic Models 794:Generic Models 629" | names: "Generic Models 794:Generic Models 629:5294464" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 795:Generic Models 629" | object type "Generic Models 795:Generic Models 629" | names: "Generic Models 795:Generic Models 629:5294482" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 798:Generic Models 629" | object type "Generic Models 798:Generic Models 629" | names: "Generic Models 798:Generic Models 629:5294500" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 799:Generic Models 629" | object type "Generic Models 799:Generic Models 629" | names: "Generic Models 799:Generic Models 629:5294518" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 800:Generic Models 629" | object type "Generic Models 800:Generic Models 629" | names: "Generic Models 800:Generic Models 629:5294536" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 801:Generic Models 629" | object type "Generic Models 801:Generic Models 629" | names: "Generic Models 801:Generic Models 629:5294554" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 840:Generic Models 629" | object type "Generic Models 840:Generic Models 629" | names: "Generic Models 840:Generic Models 629:5295496" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 841:Generic Models 629" | object type "Generic Models 841:Generic Models 629" | names: "Generic Models 841:Generic Models 629:5295514" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 842:Generic Models 629" | object type "Generic Models 842:Generic Models 629" | names: "Generic Models 842:Generic Models 629:5295533" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 843:Generic Models 629" | object type "Generic Models 843:Generic Models 629" | names: "Generic Models 843:Generic Models 629:5295551" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 844:Generic Models 629" | object type "Generic Models 844:Generic Models 629" | names: "Generic Models 844:Generic Models 629:5295570" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 845:Generic Models 629" | object type "Generic Models 845:Generic Models 629" | names: "Generic Models 845:Generic Models 629:5295588" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 846:Generic Models 629" | object type "Generic Models 846:Generic Models 629" | names: "Generic Models 846:Generic Models 629:5295607" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 847:Generic Models 629" | object type "Generic Models 847:Generic Models 629" | names: "Generic Models 847:Generic Models 629:5295625" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 848:Generic Models 629" | object type "Generic Models 848:Generic Models 629" | names: "Generic Models 848:Generic Models 629:5295644" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 849:Generic Models 629" | object type "Generic Models 849:Generic Models 629" | names: "Generic Models 849:Generic Models 629:5295662" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 850:Generic Models 629" | object type "Generic Models 850:Generic Models 629" | names: "Generic Models 850:Generic Models 629:5295681" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 851:Generic Models 629" | object type "Generic Models 851:Generic Models 629" | names: "Generic Models 851:Generic Models 629:5295699" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 852:Generic Models 629" | object type "Generic Models 852:Generic Models 629" | names: "Generic Models 852:Generic Models 629:5295718" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 853:Generic Models 629" | object type "Generic Models 853:Generic Models 629" | names: "Generic Models 853:Generic Models 629:5295736" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 854:Generic Models 629" | object type "Generic Models 854:Generic Models 629" | names: "Generic Models 854:Generic Models 629:5295755" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 855:Generic Models 629" | object type "Generic Models 855:Generic Models 629" | names: "Generic Models 855:Generic Models 629:5295773" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 856:Generic Models 629" | object type "Generic Models 856:Generic Models 629" | names: "Generic Models 856:Generic Models 629:5295792" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 857:Generic Models 629" | object type "Generic Models 857:Generic Models 629" | names: "Generic Models 857:Generic Models 629:5295810" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 858:Generic Models 629" | object type "Generic Models 858:Generic Models 629" | names: "Generic Models 858:Generic Models 629:5295829" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 859:Generic Models 629" | object type "Generic Models 859:Generic Models 629" | names: "Generic Models 859:Generic Models 629:5295847" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 872:Generic Models 629" | object type "Generic Models 872:Generic Models 629" | names: "Generic Models 872:Generic Models 629:5295866" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 873:Generic Models 629" | object type "Generic Models 873:Generic Models 629" | names: "Generic Models 873:Generic Models 629:5295884" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 874:Generic Models 629" | object type "Generic Models 874:Generic Models 629" | names: "Generic Models 874:Generic Models 629:5295903" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 876:Generic Models 629" | object type "Generic Models 876:Generic Models 629" | names: "Generic Models 876:Generic Models 629:5295921" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 877:Generic Models 629" | object type "Generic Models 877:Generic Models 629" | names: "Generic Models 877:Generic Models 629:5295940" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 878:Generic Models 629" | object type "Generic Models 878:Generic Models 629" | names: "Generic Models 878:Generic Models 629:5295958" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 879:Generic Models 629" | object type "Generic Models 879:Generic Models 629" | names: "Generic Models 879:Generic Models 629:5295977" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 880:Generic Models 629" | object type "Generic Models 880:Generic Models 629" | names: "Generic Models 880:Generic Models 629:5295995" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 881:Generic Models 629" | object type "Generic Models 881:Generic Models 629" | names: "Generic Models 881:Generic Models 629:5296014" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 882:Generic Models 629" | object type "Generic Models 882:Generic Models 629" | names: "Generic Models 882:Generic Models 629:5296032" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 883:Generic Models 629" | object type "Generic Models 883:Generic Models 629" | names: "Generic Models 883:Generic Models 629:5296051" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 884:Generic Models 629" | object type "Generic Models 884:Generic Models 629" | names: "Generic Models 884:Generic Models 629:5296069" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 885:Generic Models 629" | object type "Generic Models 885:Generic Models 629" | names: "Generic Models 885:Generic Models 629:5296088" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 886:Generic Models 629" | object type "Generic Models 886:Generic Models 629" | names: "Generic Models 886:Generic Models 629:5296106" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 887:Generic Models 629" | object type "Generic Models 887:Generic Models 629" | names: "Generic Models 887:Generic Models 629:5296125" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 888:Generic Models 629" | object type "Generic Models 888:Generic Models 629" | names: "Generic Models 888:Generic Models 629:5296143" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
      IFCBUILDINGSTOREY "2ND FLOOR" | long name "2ND FLOOR" | object type "Level:Project Base Point" | elevation 10.8020833333333
        contains 145 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 10:Structural Framing 10" | object type "Structural Framing 10:Structural Framing 10" | names: "Structural Framing 10:Structural Framing 10:4058503" | material: "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | object type "C-Channel:C15x33.9, TYP." | BEAM | names: "C-Channel:C15x33.9, TYP.:4152460" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4226601" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4228502" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 30:Structural Framing 10" | object type "Structural Framing 30:Structural Framing 10" | names: "Structural Framing 30:Structural Framing 10:4459006" | material: "TREATED 2X LEDGER - EXT. STAIN" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Timber-Column:(4) 2X6 - BUILT-UP COLUMN" | object type "Timber-Column:(4) 2X6 - BUILT-UP COLUMN" | COLUMN | names: "Timber-Column:(4) 2X6 - BUILT-UP COLUMN:4497736", "Timber-Column:(4) 2X6 - BUILT-UP COLUMN:4498129", "Timber-Column:(4) 2X6 - BUILT-UP COLUMN:4498178" (+1 more) | material: profiles "(4) 2X6 - BUILT-UP COLUMN" ("(4) 2X6 - BUILT-UP COLUMN": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4634364" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4634372" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4635659", "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4635683" | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4635821" | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | object type "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | BEAM | names: "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER:4635882" | material: profiles "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" ("BRAKE METAL FLASHING AT PERIMETER 2X LEDGER": "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4636187", "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4636190" | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4636192" | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | object type "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | BEAM | names: "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER:4636194" | material: profiles "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" ("BRAKE METAL FLASHING AT PERIMETER 2X LEDGER": "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4676443" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 966:Generic Models 629" | object type "Generic Models 966:Generic Models 629" | names: "Generic Models 966:Generic Models 629:4988717" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 967:Generic Models 629" | object type "Generic Models 967:Generic Models 629" | names: "Generic Models 967:Generic Models 629:4989978" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 968:Generic Models 629" | object type "Generic Models 968:Generic Models 629" | names: "Generic Models 968:Generic Models 629:4990045" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 969:Generic Models 629" | object type "Generic Models 969:Generic Models 629" | names: "Generic Models 969:Generic Models 629:4990098" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 970:Generic Models 629" | object type "Generic Models 970:Generic Models 629" | names: "Generic Models 970:Generic Models 629:4990151" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 971:Generic Models 629" | object type "Generic Models 971:Generic Models 629" | names: "Generic Models 971:Generic Models 629:4990204" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 972:Generic Models 629" | object type "Generic Models 972:Generic Models 629" | names: "Generic Models 972:Generic Models 629:4990257" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 973:Generic Models 629" | object type "Generic Models 973:Generic Models 629" | names: "Generic Models 973:Generic Models 629:4990310" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 974:Generic Models 629" | object type "Generic Models 974:Generic Models 629" | names: "Generic Models 974:Generic Models 629:4990363" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 975:Generic Models 629" | object type "Generic Models 975:Generic Models 629" | names: "Generic Models 975:Generic Models 629:4990416" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 976:Generic Models 629" | object type "Generic Models 976:Generic Models 629" | names: "Generic Models 976:Generic Models 629:4990469" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 977:Generic Models 629" | object type "Generic Models 977:Generic Models 629" | names: "Generic Models 977:Generic Models 629:4990522" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 978:Generic Models 629" | object type "Generic Models 978:Generic Models 629" | names: "Generic Models 978:Generic Models 629:4990575" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 979:Generic Models 629" | object type "Generic Models 979:Generic Models 629" | names: "Generic Models 979:Generic Models 629:4990628" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 980:Generic Models 629" | object type "Generic Models 980:Generic Models 629" | names: "Generic Models 980:Generic Models 629:4990681" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 981:Generic Models 629" | object type "Generic Models 981:Generic Models 629" | names: "Generic Models 981:Generic Models 629:4990734" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 982:Generic Models 629" | object type "Generic Models 982:Generic Models 629" | names: "Generic Models 982:Generic Models 629:4990787" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 983:Generic Models 629" | object type "Generic Models 983:Generic Models 629" | names: "Generic Models 983:Generic Models 629:4990840" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 984:Generic Models 629" | object type "Generic Models 984:Generic Models 629" | names: "Generic Models 984:Generic Models 629:4990893" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C.:5172292" | material: profiles "2x12 SYP JOISTS @ 16" O.C." ("2x12 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C.:5172456" | material: profiles "2x12 SYP JOISTS @ 16" O.C." ("2x12 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 889:Generic Models 629" | object type "Generic Models 889:Generic Models 629" | names: "Generic Models 889:Generic Models 629:5215255" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 890:Generic Models 629" | object type "Generic Models 890:Generic Models 629" | names: "Generic Models 890:Generic Models 629:5215289" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 891:Generic Models 629" | object type "Generic Models 891:Generic Models 629" | names: "Generic Models 891:Generic Models 629:5216714" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 892:Generic Models 629" | object type "Generic Models 892:Generic Models 629" | names: "Generic Models 892:Generic Models 629:5216732" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 893:Generic Models 629" | object type "Generic Models 893:Generic Models 629" | names: "Generic Models 893:Generic Models 629:5216788" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 894:Generic Models 629" | object type "Generic Models 894:Generic Models 629" | names: "Generic Models 894:Generic Models 629:5216806" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 895:Generic Models 629" | object type "Generic Models 895:Generic Models 629" | names: "Generic Models 895:Generic Models 629:5216825" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 896:Generic Models 629" | object type "Generic Models 896:Generic Models 629" | names: "Generic Models 896:Generic Models 629:5216843" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 897:Generic Models 629" | object type "Generic Models 897:Generic Models 629" | names: "Generic Models 897:Generic Models 629:5216862" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 898:Generic Models 629" | object type "Generic Models 898:Generic Models 629" | names: "Generic Models 898:Generic Models 629:5216880" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 899:Generic Models 629" | object type "Generic Models 899:Generic Models 629" | names: "Generic Models 899:Generic Models 629:5216899" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 900:Generic Models 629" | object type "Generic Models 900:Generic Models 629" | names: "Generic Models 900:Generic Models 629:5216917" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 901:Generic Models 629" | object type "Generic Models 901:Generic Models 629" | names: "Generic Models 901:Generic Models 629:5216936" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 902:Generic Models 629" | object type "Generic Models 902:Generic Models 629" | names: "Generic Models 902:Generic Models 629:5216954" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 903:Generic Models 629" | object type "Generic Models 903:Generic Models 629" | names: "Generic Models 903:Generic Models 629:5216973" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 904:Generic Models 629" | object type "Generic Models 904:Generic Models 629" | names: "Generic Models 904:Generic Models 629:5216991" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 905:Generic Models 629" | object type "Generic Models 905:Generic Models 629" | names: "Generic Models 905:Generic Models 629:5217010" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 906:Generic Models 629" | object type "Generic Models 906:Generic Models 629" | names: "Generic Models 906:Generic Models 629:5217028" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 907:Generic Models 629" | object type "Generic Models 907:Generic Models 629" | names: "Generic Models 907:Generic Models 629:5217047" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 908:Generic Models 629" | object type "Generic Models 908:Generic Models 629" | names: "Generic Models 908:Generic Models 629:5217065" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 909:Generic Models 629" | object type "Generic Models 909:Generic Models 629" | names: "Generic Models 909:Generic Models 629:5217084" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 910:Generic Models 629" | object type "Generic Models 910:Generic Models 629" | names: "Generic Models 910:Generic Models 629:5217102" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 965:Generic Models 629" | object type "Generic Models 965:Generic Models 629" | names: "Generic Models 965:Generic Models 629:5217121" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1002:Generic Models 629" | object type "Generic Models 1002:Generic Models 629" | names: "Generic Models 1002:Generic Models 629:5217139" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 911:Generic Models 629" | object type "Generic Models 911:Generic Models 629" | names: "Generic Models 911:Generic Models 629:5217158" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 912:Generic Models 629" | object type "Generic Models 912:Generic Models 629" | names: "Generic Models 912:Generic Models 629:5217176" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 913:Generic Models 629" | object type "Generic Models 913:Generic Models 629" | names: "Generic Models 913:Generic Models 629:5217195" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 914:Generic Models 629" | object type "Generic Models 914:Generic Models 629" | names: "Generic Models 914:Generic Models 629:5217213" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 915:Generic Models 629" | object type "Generic Models 915:Generic Models 629" | names: "Generic Models 915:Generic Models 629:5217232" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 916:Generic Models 629" | object type "Generic Models 916:Generic Models 629" | names: "Generic Models 916:Generic Models 629:5217250" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 917:Generic Models 629" | object type "Generic Models 917:Generic Models 629" | names: "Generic Models 917:Generic Models 629:5217269" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 918:Generic Models 629" | object type "Generic Models 918:Generic Models 629" | names: "Generic Models 918:Generic Models 629:5217287" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 919:Generic Models 629" | object type "Generic Models 919:Generic Models 629" | names: "Generic Models 919:Generic Models 629:5217306" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 920:Generic Models 629" | object type "Generic Models 920:Generic Models 629" | names: "Generic Models 920:Generic Models 629:5217324" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 921:Generic Models 629" | object type "Generic Models 921:Generic Models 629" | names: "Generic Models 921:Generic Models 629:5217343" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 922:Generic Models 629" | object type "Generic Models 922:Generic Models 629" | names: "Generic Models 922:Generic Models 629:5217361" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 923:Generic Models 629" | object type "Generic Models 923:Generic Models 629" | names: "Generic Models 923:Generic Models 629:5217380" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 924:Generic Models 629" | object type "Generic Models 924:Generic Models 629" | names: "Generic Models 924:Generic Models 629:5217398" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 763:Generic Models 629" | object type "Generic Models 763:Generic Models 629" | names: "Generic Models 763:Generic Models 629:5293898" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 764:Generic Models 629" | object type "Generic Models 764:Generic Models 629" | names: "Generic Models 764:Generic Models 629:5293916" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 765:Generic Models 629" | object type "Generic Models 765:Generic Models 629" | names: "Generic Models 765:Generic Models 629:5293938" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 766:Generic Models 629" | object type "Generic Models 766:Generic Models 629" | names: "Generic Models 766:Generic Models 629:5293956" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 767:Generic Models 629" | object type "Generic Models 767:Generic Models 629" | names: "Generic Models 767:Generic Models 629:5293974" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 768:Generic Models 629" | object type "Generic Models 768:Generic Models 629" | names: "Generic Models 768:Generic Models 629:5293992" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 769:Generic Models 629" | object type "Generic Models 769:Generic Models 629" | names: "Generic Models 769:Generic Models 629:5294010" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 770:Generic Models 629" | object type "Generic Models 770:Generic Models 629" | names: "Generic Models 770:Generic Models 629:5294028" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 771:Generic Models 629" | object type "Generic Models 771:Generic Models 629" | names: "Generic Models 771:Generic Models 629:5294046" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 772:Generic Models 629" | object type "Generic Models 772:Generic Models 629" | names: "Generic Models 772:Generic Models 629:5294064" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 773:Generic Models 629" | object type "Generic Models 773:Generic Models 629" | names: "Generic Models 773:Generic Models 629:5294082" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 774:Generic Models 629" | object type "Generic Models 774:Generic Models 629" | names: "Generic Models 774:Generic Models 629:5294100" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 775:Generic Models 629" | object type "Generic Models 775:Generic Models 629" | names: "Generic Models 775:Generic Models 629:5294118" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 776:Generic Models 629" | object type "Generic Models 776:Generic Models 629" | names: "Generic Models 776:Generic Models 629:5294136" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 777:Generic Models 629" | object type "Generic Models 777:Generic Models 629" | names: "Generic Models 777:Generic Models 629:5294154" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 778:Generic Models 629" | object type "Generic Models 778:Generic Models 629" | names: "Generic Models 778:Generic Models 629:5294172" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 779:Generic Models 629" | object type "Generic Models 779:Generic Models 629" | names: "Generic Models 779:Generic Models 629:5294190" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 780:Generic Models 629" | object type "Generic Models 780:Generic Models 629" | names: "Generic Models 780:Generic Models 629:5294208" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 781:Generic Models 629" | object type "Generic Models 781:Generic Models 629" | names: "Generic Models 781:Generic Models 629:5294226" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 802:Generic Models 629" | object type "Generic Models 802:Generic Models 629" | names: "Generic Models 802:Generic Models 629:5294793" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 803:Generic Models 629" | object type "Generic Models 803:Generic Models 629" | names: "Generic Models 803:Generic Models 629:5294811" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 804:Generic Models 629" | object type "Generic Models 804:Generic Models 629" | names: "Generic Models 804:Generic Models 629:5294830" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 805:Generic Models 629" | object type "Generic Models 805:Generic Models 629" | names: "Generic Models 805:Generic Models 629:5294848" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 806:Generic Models 629" | object type "Generic Models 806:Generic Models 629" | names: "Generic Models 806:Generic Models 629:5294867" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 807:Generic Models 629" | object type "Generic Models 807:Generic Models 629" | names: "Generic Models 807:Generic Models 629:5294885" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 808:Generic Models 629" | object type "Generic Models 808:Generic Models 629" | names: "Generic Models 808:Generic Models 629:5294904" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 809:Generic Models 629" | object type "Generic Models 809:Generic Models 629" | names: "Generic Models 809:Generic Models 629:5294922" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 810:Generic Models 629" | object type "Generic Models 810:Generic Models 629" | names: "Generic Models 810:Generic Models 629:5294941" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 811:Generic Models 629" | object type "Generic Models 811:Generic Models 629" | names: "Generic Models 811:Generic Models 629:5294959" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 812:Generic Models 629" | object type "Generic Models 812:Generic Models 629" | names: "Generic Models 812:Generic Models 629:5294978" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 813:Generic Models 629" | object type "Generic Models 813:Generic Models 629" | names: "Generic Models 813:Generic Models 629:5294996" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 814:Generic Models 629" | object type "Generic Models 814:Generic Models 629" | names: "Generic Models 814:Generic Models 629:5295015" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 815:Generic Models 629" | object type "Generic Models 815:Generic Models 629" | names: "Generic Models 815:Generic Models 629:5295033" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 816:Generic Models 629" | object type "Generic Models 816:Generic Models 629" | names: "Generic Models 816:Generic Models 629:5295052" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 817:Generic Models 629" | object type "Generic Models 817:Generic Models 629" | names: "Generic Models 817:Generic Models 629:5295070" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 818:Generic Models 629" | object type "Generic Models 818:Generic Models 629" | names: "Generic Models 818:Generic Models 629:5295089" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 819:Generic Models 629" | object type "Generic Models 819:Generic Models 629" | names: "Generic Models 819:Generic Models 629:5295107" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 820:Generic Models 629" | object type "Generic Models 820:Generic Models 629" | names: "Generic Models 820:Generic Models 629:5295126" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 821:Generic Models 629" | object type "Generic Models 821:Generic Models 629" | names: "Generic Models 821:Generic Models 629:5295144" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 822:Generic Models 629" | object type "Generic Models 822:Generic Models 629" | names: "Generic Models 822:Generic Models 629:5295163" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 823:Generic Models 629" | object type "Generic Models 823:Generic Models 629" | names: "Generic Models 823:Generic Models 629:5295181" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 824:Generic Models 629" | object type "Generic Models 824:Generic Models 629" | names: "Generic Models 824:Generic Models 629:5295200" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 825:Generic Models 629" | object type "Generic Models 825:Generic Models 629" | names: "Generic Models 825:Generic Models 629:5295218" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 826:Generic Models 629" | object type "Generic Models 826:Generic Models 629" | names: "Generic Models 826:Generic Models 629:5295237" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 827:Generic Models 629" | object type "Generic Models 827:Generic Models 629" | names: "Generic Models 827:Generic Models 629:5295255" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 828:Generic Models 629" | object type "Generic Models 828:Generic Models 629" | names: "Generic Models 828:Generic Models 629:5295274" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 829:Generic Models 629" | object type "Generic Models 829:Generic Models 629" | names: "Generic Models 829:Generic Models 629:5295292" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 830:Generic Models 629" | object type "Generic Models 830:Generic Models 629" | names: "Generic Models 830:Generic Models 629:5295311" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 831:Generic Models 629" | object type "Generic Models 831:Generic Models 629" | names: "Generic Models 831:Generic Models 629:5295329" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 832:Generic Models 629" | object type "Generic Models 832:Generic Models 629" | names: "Generic Models 832:Generic Models 629:5295348" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 833:Generic Models 629" | object type "Generic Models 833:Generic Models 629" | names: "Generic Models 833:Generic Models 629:5295366" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 834:Generic Models 629" | object type "Generic Models 834:Generic Models 629" | names: "Generic Models 834:Generic Models 629:5295385" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 835:Generic Models 629" | object type "Generic Models 835:Generic Models 629" | names: "Generic Models 835:Generic Models 629:5295403" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 836:Generic Models 629" | object type "Generic Models 836:Generic Models 629" | names: "Generic Models 836:Generic Models 629:5295422" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 837:Generic Models 629" | object type "Generic Models 837:Generic Models 629" | names: "Generic Models 837:Generic Models 629:5295440" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 838:Generic Models 629" | object type "Generic Models 838:Generic Models 629" | names: "Generic Models 838:Generic Models 629:5295459" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Generic Models 839:Generic Models 629" | object type "Generic Models 839:Generic Models 629" | names: "Generic Models 839:Generic Models 629:5295477" | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          9 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Beam System:Structural Framing System:3572614", "Structural Beam System:Structural Framing System:4003764", "Structural Beam System:Structural Framing System:4152940" (+6 more) | parts: 226 IFCBEAM | property sets: Pset_EnvironmentalImpactIndicators
      IFCBUILDINGSTOREY "3RD FLOOR" | long name "3RD FLOOR" | object type "Level:Project Base Point" | elevation 21.46875
        contains 27 elements
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4113135" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4113143" | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          4 x IFCCOLUMN | type IFCCOLUMNTYPE "Timber-Column:(4) 2X6 - BUILT-UP COLUMN" | object type "Timber-Column:(4) 2X6 - BUILT-UP COLUMN" | COLUMN | names: "Timber-Column:(4) 2X6 - BUILT-UP COLUMN:4497964", "Timber-Column:(4) 2X6 - BUILT-UP COLUMN:4498131", "Timber-Column:(4) 2X6 - BUILT-UP COLUMN:4498180" (+1 more) | material: profiles "(4) 2X6 - BUILT-UP COLUMN" ("(4) 2X6 - BUILT-UP COLUMN": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfColumn
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4634355" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | object type "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | names: "C-Channel:C15x33.9, TYP. STRINGER:4634359" | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4636177", "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4636180" | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4636182" | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | object type "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | BEAM | names: "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER:4636184" | material: profiles "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" ("BRAKE METAL FLASHING AT PERIMETER 2X LEDGER": "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          2 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4636197", "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4636200" | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C.:4636202" | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | object type "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | BEAM | names: "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER:4636204" | material: profiles "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" ("BRAKE METAL FLASHING AT PERIMETER 2X LEDGER": "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C.:5030487" | material: profiles "2x12 SYP JOISTS @ 16" O.C." ("2x12 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          1 x IFCBEAM | type IFCBEAMTYPE "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | object type "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | BEAM | names: "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C.:5172554" | material: profiles "2x12 SYP JOISTS @ 16" O.C." ("2x12 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon, Pset_EnvironmentalImpactIndicators, Pset_ReinforcementBarPitchOfBeam
          9 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Beam System:Structural Framing System:4003551", "Structural Beam System:Structural Framing System:4003887", "Structural Beam System:Structural Framing System:4154611" (+6 more) | parts: 224 IFCBEAM | property sets: Pset_EnvironmentalImpactIndicators
      IFCBUILDINGSTOREY "ROOF" | long name "ROOF" | object type "Level:Project Base Point" | elevation 30.4375000000082
        contains 14 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2:Structural Framing 2" | object type "Structural Framing 2:Structural Framing 2" | names: "Structural Framing 2:Structural Framing 2:4355008" | material: "TREATED 2X LEDGER - EXT. STAIN" | property sets: Pset_BuildingElementProxyCommon, Pset_EnvironmentalImpactIndicators
          13 x IFCELEMENTASSEMBLY | object type "Structural Beam System:Structural Framing System" | BEAM_GRID | names: "Structural Beam System:Structural Framing System:4163550", "Structural Beam System:Structural Framing System:4164145", "Structural Beam System:Structural Framing System:4164576" (+10 more) | parts: 397 IFCBEAM | property sets: Pset_EnvironmentalImpactIndicators

Types
  IFCFOOTINGTYPE "Wall Foundation:UNDER LANDSCAPE WALLS" | STRIP_FOOTING | 1 occurrence
  IFCFOOTINGTYPE "Wall Foundation:UNDER LANDSCAPE WALLS" | STRIP_FOOTING | 1 occurrence
  IFCFOOTINGTYPE "Wall Foundation:UNDER LANDSCAPE WALLS" | STRIP_FOOTING | 1 occurrence
  IFCFOOTINGTYPE "Wall Foundation:UNDER LANDSCAPE WALLS" | STRIP_FOOTING | 1 occurrence
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: "STEEL C CHANNEL - HDG - SEE STRUCT DWGS" | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 6X6X3/8" | COLUMN | 1 occurrence | material: profiles "HSS 6X6X3/8" ("HSS 6X6X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8" | COLUMN | 6 occurrences | material: profiles "HSS 5.5X5.5X3/8" ("HSS 5.5X5.5X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 9:Structural Framing 9" | 1 occurrence | material: "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | property sets: Pset_BuildingElementProxyCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8" | COLUMN | 1 occurrence | material: profiles "HSS 5.5X5.5X3/8" ("HSS 5.5X5.5X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 6X6X3/8" | COLUMN | 1 occurrence | material: profiles "HSS 6X6X3/8" ("HSS 6X6X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 2 occurrences | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 1 occurrence | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4"" | BEAM | 3 occurrences | material: profiles "GL - 3 1/2" X 11 1/4"" ("GL - 3 1/2" X 11 1/4"": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 2 occurrences | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 2 occurrences | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 2 occurrences | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X12" | BEAM | 4 occurrences | material: profiles "(3)-2X12" ("(3)-2X12": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 2 occurrences | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 3 occurrences | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 1 occurrence | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)-2X8" | BEAM | 1 occurrence | material: profiles "(3)-2X8" ("(3)-2X8": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 2 occurrences | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X8 - JOIST" | BEAM | 1 occurrence | material: profiles "2X8 - JOIST" ("2X8 - JOIST": "BOTTOM CHORD OF FIELD FRAMED OVERHANG") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 29:Structural Framing 9" | 1 occurrence | material: "TREATED 2X LEDGER - EXT. STAIN" | property sets: Pset_BuildingElementProxyCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X8 - JOIST" | BEAM | 1 occurrence | material: profiles "2X8 - JOIST" ("2X8 - JOIST": "BOTTOM CHORD OF FIELD FRAMED OVERHANG") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X8 - JOIST" | BEAM | 1 occurrence | material: profiles "2X8 - JOIST" ("2X8 - JOIST": "BOTTOM CHORD OF FIELD FRAMED OVERHANG") | property sets: Pset_BeamCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X4 - BLOCKING" | BEAM | 1 occurrence | material: profiles "2X4 - BLOCKING" ("2X4 - BLOCKING": "2X SILL - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x50, TYP." | BEAM | 1 occurrence | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x50, TYP." | BEAM | 1 occurrence | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Dimension Lumber - Truncated:(2) 2X8 @ ROOF EDGE" | BEAM | 2 occurrences | material: profiles "(2) 2X8 @ ROOF EDGE" ("(2) 2X8 @ ROOF EDGE": "TREATED 2X JOISTS - EXT. STAIN") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061713 - Laminated Veneer Lumber:GL - 3 1/2" X 11 1/4"" | BEAM | 1 occurrence | material: profiles "GL - 3 1/2" X 11 1/4"" ("GL - 3 1/2" X 11 1/4"": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(3)2X6" | BEAM | 2 occurrences | material: profiles "(3)2X6" ("(3)2X6": "LVL(s) - SIZE T.B.D.") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X8 - OUTRIGGER" | BEAM | 1 occurrence | material: profiles "2X8 - OUTRIGGER" ("2X8 - OUTRIGGER": "2X8 OUTRIGGER - SISTER TO ROOF TRUSSES") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2X8 - OUTRIGGER" | BEAM | 1 occurrence | material: profiles "2X8 - OUTRIGGER" ("2X8 - OUTRIGGER": "2X8 OUTRIGGER - SISTER TO ROOF TRUSSES") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "Timber-Column:(4) 2X6 - BUILT-UP COLUMN" | COLUMN | 4 occurrences | material: profiles "(4) 2X6 - BUILT-UP COLUMN" ("(4) 2X6 - BUILT-UP COLUMN": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCSLABTYPE "Footing-Rectangular:CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" | BASESLAB | 1 occurrence | material: "CONCRETE FOOTING - SEE STRUCT DWGS" | property sets: Pset_SlabCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 8X8X3/8" | COLUMN | 1 occurrence | material: profiles "HSS 8X8X3/8" ("HSS 8X8X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 8X8X3/8" | COLUMN | 6 occurrences | material: profiles "HSS 8X8X3/8" ("HSS 8X8X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | BEAM | 1 occurrence | material: profiles "2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" ("2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2X8" | BEAM | 2 occurrences | material: profiles "(2) 2X8" ("(2) 2X8": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2X8" | BEAM | 1 occurrence | material: profiles "(2) 2X8" ("(2) 2X8": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2X8" | BEAM | 1 occurrence | material: profiles "(2) 2X8" ("(2) 2X8": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "HSS-Hollow Structural Section-Column:HSS 5.5X5.5X3/8" | COLUMN | 1 occurrence | material: profiles "HSS 5.5X5.5X3/8" ("HSS 5.5X5.5X3/8": "STEEL COLUMN - SEE STRUCT DWGS") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x50, TYP." | BEAM | 1 occurrence | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x50, TYP." | BEAM | 1 occurrence | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x50, TYP." | BEAM | 1 occurrence | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x50, TYP." | BEAM | 1 occurrence | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x50, TYP." | BEAM | 1 occurrence | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x50, TYP." | BEAM | 1 occurrence | material: profiles "C15x50, TYP." ("C15x50, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | BEAM | 1 occurrence | material: profiles "2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" ("2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | BEAM | 1 occurrence | material: profiles "2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" ("2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "Dimension Lumber - Truncated:2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" | BEAM | 1 occurrence | material: profiles "2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)" ("2X8 SYP No.2 JOISTS @ 16" O.C. - (NO TRUNCATE)": "2X ROOF JOISTS - EXT. STAIN-1 - SEE LIFE SAFETY DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 985:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 986:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 987:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 988:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 989:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 990:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 991:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 992:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 993:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 994:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 995:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 996:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 997:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 998:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 734:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 999:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1000:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1001:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:(2) 2x12 - RIM JOIST" | BEAM | 1 occurrence | material: profiles "(2) 2x12 - RIM JOIST" ("(2) 2x12 - RIM JOIST": "(2) SISTERED 2X12'S - BRAKE METAL FLASHING AT TOP/EXTERIOR") | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 925:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 927:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 928:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 929:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 930:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 931:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 932:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 933:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 934:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 935:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 936:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 937:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 938:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 939:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 940:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 941:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 942:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 943:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 944:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 945:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 947:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 948:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 949:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 952:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 953:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 954:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 955:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 956:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 957:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 958:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 959:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 960:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 961:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 962:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 963:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 964:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 782:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 783:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 784:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 785:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 786:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 787:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 788:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 789:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 790:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 791:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 792:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 793:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 794:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 795:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 798:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 799:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 800:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 801:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 840:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 841:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 842:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 843:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 844:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 845:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 846:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 847:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 848:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 849:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 850:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 851:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 852:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 853:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 854:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 855:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 856:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 857:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 858:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 859:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 872:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 873:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 874:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 876:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 877:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 878:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 879:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 880:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 881:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 882:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 883:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 884:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 885:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 886:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 887:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 888:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 10:Structural Framing 10" | 1 occurrence | material: "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | property sets: Pset_BuildingElementProxyCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP." | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP." ("C15x33.9, TYP.": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 30:Structural Framing 10" | 1 occurrence | material: "TREATED 2X LEDGER - EXT. STAIN" | property sets: Pset_BuildingElementProxyCommon
  IFCCOLUMNTYPE "Timber-Column:(4) 2X6 - BUILT-UP COLUMN" | COLUMN | 4 occurrences | material: profiles "(4) 2X6 - BUILT-UP COLUMN" ("(4) 2X6 - BUILT-UP COLUMN": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | 4 occurrences | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | 2 occurrences | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | BEAM | 2 occurrences | material: profiles "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" ("BRAKE METAL FLASHING AT PERIMETER 2X LEDGER": "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | 4 occurrences | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x10 SYP JOISTS @ 16" O.C." | BEAM | 2 occurrences | material: profiles "2x10 SYP JOISTS @ 16" O.C." ("2x10 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" | BEAM | 2 occurrences | material: profiles "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER" ("BRAKE METAL FLASHING AT PERIMETER 2X LEDGER": "BRAKE METAL FLASHING AT PERIMETER 2X LEDGER") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 966:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 967:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 968:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 969:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 970:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 971:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 972:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 973:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 974:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 975:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 976:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 977:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 978:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 979:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 980:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 981:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 982:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 983:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 984:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | BEAM | 1 occurrence | material: profiles "2x12 SYP JOISTS @ 16" O.C." ("2x12 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | BEAM | 1 occurrence | material: profiles "2x12 SYP JOISTS @ 16" O.C." ("2x12 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 889:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 890:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 891:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 892:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 893:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 894:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 895:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 896:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 897:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 898:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 899:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 900:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 901:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 902:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 903:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 904:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 905:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 906:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 907:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 908:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 909:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 910:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 965:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 1002:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 911:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 912:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 913:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 914:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 915:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 916:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 917:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 918:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 919:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 920:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 921:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 922:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 923:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 924:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 763:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 764:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 765:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 766:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 767:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 768:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 769:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 770:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 771:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 772:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 773:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 774:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 775:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 776:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 777:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 778:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 779:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 780:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 781:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 802:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 803:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 804:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 805:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 806:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 807:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 808:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 809:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 810:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 811:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 812:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 813:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 814:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 815:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 816:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 817:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 818:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 819:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 820:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 821:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 822:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 823:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 824:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 825:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 826:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 827:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 828:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 829:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 830:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 831:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 832:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 833:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 834:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 835:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 836:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 837:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 838:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Generic Models 839:Generic Models 629" | 1 occurrence | material: "PREFABRICATED GALV. STEEL TREAD" | property sets: Pset_BuildingElementProxyCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCCOLUMNTYPE "Timber-Column:(4) 2X6 - BUILT-UP COLUMN" | COLUMN | 4 occurrences | material: profiles "(4) 2X6 - BUILT-UP COLUMN" ("(4) 2X6 - BUILT-UP COLUMN": "STRUCTURAL WOOD COLUMN - SIZE TBD") | property sets: Pset_ColumnCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "C-Channel:C15x33.9, TYP. STRINGER" | BEAM | 1 occurrence | material: profiles "C15x33.9, TYP. STRINGER" ("C15x33.9, TYP. STRINGER": "STEEL C CHANNEL - HDG - SEE STRUCT DWGS") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | BEAM | 1 occurrence | material: profiles "2x12 SYP JOISTS @ 16" O.C." ("2x12 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon
  IFCBEAMTYPE "061100 - Wood Framing:2x12 SYP JOISTS @ 16" O.C." | BEAM | 1 occurrence | material: profiles "2x12 SYP JOISTS @ 16" O.C." ("2x12 SYP JOISTS @ 16" O.C.": "2X JOISTS W/ BUTYL TAPE AT TOP EDGE") | property sets: Pset_BeamCommon
  IFCBUILDINGELEMENTPROXYTYPE "Structural Framing 2:Structural Framing 2" | 1 occurrence | material: "TREATED 2X LEDGER - EXT. STAIN" | property sets: Pset_BuildingElementProxyCommon

Property sets
  Pset_SiteCommon | properties | on 1 object (1 IFCSITE)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 64 objects (64 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2x10 SYP JOISTS @ 16" O.C." (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 6.83333333333474 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 64 objects (64 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "TRIMJOIST J18 @ 24" O.C. (TYP)" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 19.3333333333319 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 56 objects (56 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "TRIMJOIST J18 @ 24" O.C. (TYP)" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 24.0000077838585 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 56 objects (56 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "TRIMJOIST J18 @ 24" O.C. (TYP)" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 19.3333333333322 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 30 objects (30 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "PREFABRICATED SLOPED WOOD ROOF TRUSS - SIZE T.B.D" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 19.3333333333319 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 28 objects (28 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "PREFABRICATED SLOPED WOOD ROOF TRUSS - SIZE T.B.D" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 24.0000077838585 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 28 objects (28 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "PREFABRICATED SLOPED WOOD ROOF TRUSS - SIZE T.B.D" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 19.3333333333322 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon | properties | on 23 objects (23 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "2X8 - BOTTOM CHORD" (IFCIDENTIFIER)
    Roll = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Slope = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Span = 1.99999999999909 (IFCPOSITIVELENGTHMEASURE) [FOOT (conversion based)]
  Pset_BeamCommon: 434 more contents on 733 objects not shown
  Pset_EnvironmentalImpactIndicators | properties | on 222 objects (222 IFCBUILDINGELEMENTPROXY)
    Reference = "Generic Models 629" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 208 objects (208 IFCBEAM)
    Reference = "TRIMJOIST J18 @ 24" O.C. (TYP)" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 190 objects (190 IFCBEAM)
    Reference = "2x12 SYP JOISTS @ 16" O.C." (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 104 objects (104 IFCBEAM)
    Reference = "PREFABRICATED SLOPED WOOD ROOF TRUSS - SIZE T.B.D" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 98 objects (98 IFCBEAM)
    Reference = "2X8 TOP CHORD" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 98 objects (98 IFCBEAM)
    Reference = "2X8 SYP No.2 JOISTS @ 16" O.C." (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 80 objects (80 IFCBEAM)
    Reference = "2X8 - BOTTOM CHORD" (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators | properties | on 68 objects (68 IFCBEAM)
    Reference = "2x10 SYP JOISTS @ 16" O.C." (IFCIDENTIFIER)
  Pset_EnvironmentalImpactIndicators: 26 more contents on 321 objects not shown
  Pset_ReinforcementBarPitchOfBeam | properties | on 208 objects (208 IFCBEAM)
    Description = "Joist" (IFCTEXT)
    Reference = "TRIMJOIST J18 @ 24" O.C. (TYP)" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 190 objects (190 IFCBEAM)
    Reference = "2x12 SYP JOISTS @ 16" O.C." (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 104 objects (104 IFCBEAM)
    Description = "Joist" (IFCTEXT)
    Reference = "PREFABRICATED SLOPED WOOD ROOF TRUSS - SIZE T.B.D" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 98 objects (98 IFCBEAM)
    Reference = "2X8 TOP CHORD" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 98 objects (98 IFCBEAM)
    Reference = "2X8 SYP No.2 JOISTS @ 16" O.C." (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 80 objects (80 IFCBEAM)
    Reference = "2X8 - BOTTOM CHORD" (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 68 objects (68 IFCBEAM)
    Reference = "2x10 SYP JOISTS @ 16" O.C." (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam | properties | on 52 objects (52 IFCBEAM)
    Reference = "C15x33.9, TYP." (IFCLABEL)
  Pset_ReinforcementBarPitchOfBeam: 14 more contents on 184 objects not shown
  Pset_ColumnCommon | properties | on 12 objects (12 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "(4) 2X6 - BUILT-UP COLUMN" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 8 objects (8 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HSS 5.5X5.5X3/8" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 7 objects (7 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HSS 8X8X3/8" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "HSS 6X6X3/8" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 10 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ReinforcementBarPitchOfColumn | properties | on 12 objects (12 IFCCOLUMN)
    Reference = "(4) 2X6 - BUILT-UP COLUMN" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 8 objects (8 IFCCOLUMN)
    Reference = "HSS 5.5X5.5X3/8" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 7 objects (7 IFCCOLUMN)
    Reference = "HSS 8X8X3/8" (IFCLABEL)
  Pset_ReinforcementBarPitchOfColumn | properties | on 2 objects (2 IFCCOLUMN)
    Reference = "HSS 6X6X3/8" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 222 objects (222 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Generic Models 629" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Structural Framing 9" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Structural Framing 10" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Structural Framing 2" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDING)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 227 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_ManufacturerTypeInformation | properties | on 312 objects (312 IFCBEAM)
    Manufacturer = "RedBuilt™" (IFCLABEL)
  Pset_FootingCommon | properties | on 4 objects (4 IFCFOOTING)
    Reference = "UNDER LANDSCAPE WALLS" (IFCIDENTIFIER)
  Pset_ReinforcementBarCountOfIndependentFooting | properties | on 4 objects (4 IFCFOOTING)
    Reference = "UNDER LANDSCAPE WALLS" (IFCLABEL)
  Pset_ReinforcementBarPitchOfContinuousFooting | properties | on 4 objects (4 IFCFOOTING)
    Reference = "UNDER LANDSCAPE WALLS" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 9 objects (9 IFCSLAB)
    Reference = "CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" (IFCLABEL)
  Pset_ReinforcementBarPitchOfSlab | properties | on 7 objects (7 IFCSLAB)
    Reference = "CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" (IFCLABEL)
  Pset_SlabCommon | properties | on 9 objects (9 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "CONCRETE STEEL COLUMN FOOTING - 4' X 4' x 2'-6"" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 5 objects (5 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    PitchAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Reference = "CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 2 objects (2 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "CONCRETE STEEL COLUMN FOOTING 5.5' X 5.5' x 2.5'" (IFCIDENTIFIER)
  Pset_SlabCommon | properties | on 16 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 5 objects (5 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Base Point" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDING)
    AboveGround = UNKNOWN (IFCLOGICAL)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 5 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Pset_BuildingSystemCommon | properties | on 1 object (1 IFCBUILDING)
    Reference = "Project Information" (IFCIDENTIFIER)