IFC building model
Schema: "IFC4"
Description: "ViewDefinition[DesignTransferView]"
File name: "Monica_Residence.ifc"
Time stamp: "2024-01-04T14:38:22-06:00"
Preprocessor: "IfcOpenShell v0.7.0-6c9e130ca"
Originating system: "BlenderBIM 0.0.231222-1f3ff0d"
Authorization: "Nobody"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  115 x Person "ryan@openingdesign.com" of Organization (no name given)
  104 x Organization "Autodesk Revit 2020 (ENU)"
  3 x Organization "Autodesk Revit 2022 (ENU)"
  5 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1680878644 (2023-04-07T14:44:04Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1661457979 (2022-08-25T20:06:19Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1682123705 (2023-04-22T00:35:05Z)
  Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1633996150 (2021-10-11T23:49:10Z)
  73 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1682305051 (2023-04-24T02:57:31Z)
  29 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1681941947 (2023-04-19T22:05:47Z)
  3 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2022 (ENU)" version "2022" identifier "Revit" by Organization "Autodesk Revit 2022 (ENU)" | change NOCHANGE | created 1688603340 (2023-07-06T00:29:00Z)
  2 x Owner history of Person "ryan@openingdesign.com" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1691523003 (2023-08-08T19:30:03Z)

Units
  PLANEANGLEUNIT: degree (conversion based)
  AREAUNIT: square foot (conversion based)
  LENGTHUNIT: foot (conversion based)
  VOLUMEUNIT: cubic foot (conversion based)

Spatial structure
IFCPROJECT "My Project"
  IFCSITE "My Site"
    contains 1 element
      1 x IFCANNOTATION | object type "DRAWING" | names: "FLOOR PLAN - 1ST" | property sets: EPset_Drawing, OD_Options
    IFCBUILDING "My Building"
      IFCBUILDINGSTOREY "My Storey"
        contains 928 elements
          424 x IFCBUILDINGELEMENTPROXY | COMPLEX | names: "Continuous Angle1:Continuous Angle:1463390", "Continuous Angle2:Continuous Angle:1578039", "Continuous Angle3:Continuous Angle:1578050" (+421 more) | material: constituents "concrete" (); "TOP METAL STUD TRACK (FASTENER 24" O.C.)"; "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)"; "METAL RUNNER CHANNEL; FASTEN @ 24" O.C."; "CEILING TRACK AS SCHEDULED"; "FIRE RATED SEALANT" | property sets: EPset_Drawing, BBIM_Array, Pset_BuildingElementProxyCommon
          3 x IFCDOOR | type IFCDOORTYPE "30"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: EPset_Status
          2 x IFCDOOR | type IFCDOORTYPE "34"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status, OD_Options
          2 x IFCDOOR | type IFCDOORTYPE "34"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          4 x IFCDOOR | type IFCDOORTYPE "36"80"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status, OD_Options
          5 x IFCDOOR | type IFCDOORTYPE "36"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status, EPset_Drawing
          2 x IFCDOOR | type IFCDOORTYPE "32"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "30"84"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          5 x IFCWALL | type IFCWALLTYPE "W1" | names: "Wall" | material: layers "poche" ("1/2" WOOD SIDING" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "1/2" WOOD SIDING" 0.0520833333333333) | property sets: EPset_Parametric, EPset_Drawing, EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "30"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Drawing, EPset_Status
          3 x IFCDOOR | type IFCDOORTYPE "34"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          2 x IFCDOOR | type IFCDOORTYPE "32"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "34"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          10 x IFCDOOR | type IFCDOORTYPE "36"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status, EPset_Drawing, OD_Options, Qto_DoorBaseQuantities
          4 x IFCDOOR | type IFCDOORTYPE "36"84"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status, EPset_Drawing
          17 x IFCWALL | type IFCWALLTYPE "EXT-VINYL" | names: "Wall" | material: layers "HorzLines6in96scale" ("GENERIC POCHE" 0.583333313465118) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Status, OD_Options, Qto_WallBaseQuantities, EPset_Drawing
          2 x IFCWALL | type IFCWALLTYPE "EXT-BRICK" | names: "Wall" | material: layers "BrickElevation" ("BRICK" 0.583333313465118) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Drawing, EPset_Status
          64 x IFCWALL | type IFCWALLTYPE "W4AØF" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Status, EPset_Drawing, OD_Options, Qto_WallBaseQuantities
          2 x IFCWALL | type IFCWALLTYPE "W4B2D" | names: "Wall" | material: layers "poche" ("1/2" WOOD SIDING" 0.0520830005407333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520830005407333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "1/2" WOOD SIDING" 0.0520830005407333) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "30"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Core_Fill_8in" | names: "BuildingElementProxy" | property sets: BBIM_Array
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Horz Ladder Reinforcing" | names: "BuildingElementProxy" | material: "STANDARD 9-GAUGE (MW11), LADDER-SHAPED WIRE FABRICATED WITH BUTT-WELDED CROSS-RODS SPACED 406-MM (16-IN.) ON CENTER (OC)"
          10 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "8inCMU" | names: "BuildingElementProxy" | property sets: BBIM_Array
          11 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Morter_8inCMU" | names: "BuildingElementProxy" | property sets: BBIM_Array
          9 x IFCFURNITURE | names: "Cube", "CounterTop-Bar", "BaseCabinet-Bar" (+5 more) | property sets: Pset_FurnitureTypeCommon, OD_Options, Pset_WallCommon
          3 x IFCCOLUMN | type IFCCOLUMNTYPE "C1 Copy" | names: "Column" | material: profiles ("Unknown") | property sets: EPset_Parametric, Pset_ColumnCommon
          10 x IFCSLAB | type IFCSLABTYPE "SIDEWALK" | names: "Slab" | material: layers "20Fill" ("8"D X 16"W CONCRETE FOOTING W(2) CONT. #5's" 0.5) | property sets: EPset_Parametric, Pset_SlabCommon, Qto_SlabBaseQuantities, EPset_Status, EPset_Drawing
          1 x IFCSLAB | type IFCSLABTYPE "CONCRETE SLAB" | names: "Slab" | material: layers "5Fill" ("8"D X 16"W CONCRETE FOOTING W(2) CONT. #5's" 0.5) | property sets: EPset_Parametric, Pset_SlabCommon, EPset_Drawing, Qto_SlabBaseQuantities, EPset_Status
          6 x IFCWINDOW | type IFCWINDOWTYPE "WT01 3.6''x5.4'" | names: "Window" | property sets: Pset_WindowCommon, EPset_Status
          15 x IFCCOVERING | type IFCCOVERINGTYPE "COV30" | names: "Covering" | material: layers ("Unknown" 0.0984251968503937) | property sets: EPset_Parametric, Pset_CoveringCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "COV10" | names: "Covering" | material: layers ("Unknown" 0.0328083989501312) | property sets: EPset_Parametric, Pset_CoveringCommon
          1 x IFCWINDOW | type IFCWINDOWTYPE "WT01 4.0'x5.4'" | names: "Window" | property sets: Pset_WindowCommon, EPset_Status
          2 x IFCBEAM | type IFCBEAMTYPE "Curb" | names: "Beam" | material: profiles ("RAMP CURB") | property sets: EPset_Parametric, Pset_BeamCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Curb 1.6'x1.6'" | names: "Beam" | material: profiles ("RAMP CURB") | property sets: EPset_Parametric, Pset_BeamCommon
          2 x IFCWINDOW | type IFCWINDOWTYPE "WT01 6.0'x3.8'" | names: "Window" | property sets: EPset_Status
          3 x IFCWINDOW | type IFCWINDOWTYPE "WT01 2.6'x2.6'" | names: "Window" | property sets: EPset_Status
          2 x IFCSTAIRFLIGHT | STRAIGHT | names: "Cube" | property sets: Pset_StairFlightCommon, BBIM_Stair
          1 x IFCWALL | type IFCWALLTYPE "W6AØF" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.458333343267441, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, OD_Options, Pset_WallCommon, EPset_Status
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Table-Dinning" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Furniture-Stool" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon
          1 x IFCCOVERING | type IFCCOVERINGTYPE "TYPEX" | names: "Covering" | material: layers "10Fill" ("Unknown" 0.020833333954215) | property sets: EPset_Parametric, Qto_CoveringBaseQuantities, Pset_CoveringCommon, EPset_Drawing
          2 x IFCFURNITURE | type IFCFURNITURETYPE "Generic 3-Seater Sofa" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon
          2 x IFCFURNITURE | type IFCFURNITURETYPE "Generic Medium Coffee Table" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon
          6 x IFCFURNITURE | type IFCFURNITURETYPE "Chair-Dining" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | names: "SanitaryTerminal" | property sets: OD_Options, Pset_SanitaryTerminalTypeCommon
          5 x IFCFURNITURE | type IFCFURNITURETYPE "Chair-BarStool" | names: "Furniture" | property sets: OD_Options, Pset_FurnitureTypeCommon
          2 x IFCFURNITURE | type IFCFURNITURETYPE "Bed-King" | names: "Furniture" | material: "bed-king" | property sets: OD_Options, Pset_FurnitureTypeCommon
          3 x IFCDOOR | type IFCDOORTYPE "G36"80"L" | names: "Door" | property sets: EPset_Status, EPset_Drawing
          3 x IFCDOOR | type IFCDOORTYPE "G36"80"R" | names: "Door" | property sets: EPset_Status
          14 x IFCVIRTUALELEMENT | names: "Cad_Import", "Model Text:OD_Very Large:1595839", "Model Text:OD_Very Large:1595840" (+9 more) | property sets: EPset_Drawing
          2 x IFCDOOR | type IFCDOORTYPE "S96"80"" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: EPset_Status
          2 x IFCDOOR | type IFCDOORTYPE "S60"80"" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: EPset_Status
          5 x IFCWALL | type IFCWALLTYPE "M4B2D" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0625, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FO" 0.333333343267441, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0833333358168602) | property sets: Pset_WallCommon, EPset_Parametric, EPset_Status, EPset_Drawing
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "W/D" | names: "ElectricAppliance" | property sets: EPset_Drawing, Pset_ElectricApplianceTypeCommon
          1 x IFCDOOR | type IFCDOORTYPE "S72"80"" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "S90"80"" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: EPset_Drawing, EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "S84"80"" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: EPset_Status
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "Neufert Cooktop 75x51" | names: "ElectricAppliance" | property sets: Pset_ElectricApplianceTypeCommon
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "DW" | names: "ElectricAppliance" | property sets: Pset_ElectricApplianceTypeCommon
          6 x IFCWINDOW | type IFCWINDOWTYPE "W1" | names: "Window" | material: constituents ("DOOR TRIM", "WINDOW", "INSULATED GLAZING") | property sets: Pset_WindowCommon, EPset_Status
          2 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "Generic Medium Sink" | names: "SanitaryTerminal" | property sets: Pset_SanitaryTerminalTypeCommon, EPset_Status
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "TUB:1:2901065" | names: "SanitaryTerminal" | property sets: Pset_SanitaryTerminalTypeCommon
          1 x IFCELECTRICAPPLIANCE | type IFCELECTRICAPPLIANCETYPE "TV" | names: "ElectricAppliance" | material: constituents ("TV") | property sets: Pset_ElectricApplianceTypeCommon
          6 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Cube" | names: "BuildingElementProxy" | property sets: EPset_Drawing
          6 x IFCWALL | type IFCWALLTYPE "EXT-EIFS" | names: "Wall" | material: layers "10Fill" ("EIFS" 0.583333313465118) | property sets: EPset_Parametric, Pset_WallCommon, EPset_Status
          1 x IFCWINDOW | type IFCWINDOWTYPE "4'x5.4'" | names: "Window" | property sets: EPset_Status
          7 x IFCSLAB | type IFCSLABTYPE "GRASS2" | names: "GeographicElement", "Slab" | material: layers "grass" ("GRASS" 0.5) | property sets: EPset_Parametric, Qto_SlabBaseQuantities, EPset_Drawing, Pset_SlabCommon, EPset_Status
          2 x IFCSLAB | type IFCSLABTYPE "ASPHALT DRIVE WAY" | names: "Slab" | material: layers "10Fill" ("ASPHALT DRIVEWAY" 0.5) | property sets: EPset_Parametric, Qto_SlabBaseQuantities, Pset_SlabCommon, EPset_Drawing, EPset_Status
          11 x IFCVIRTUALELEMENT | object type "PROPERTYLINE" | names: "Plane.001", "Plane", "Front Lot Line" (+6 more) | material: "PROPERTY LINE"
          13 x IFCSLAB | type IFCSLABTYPE "ROOF" | names: "Slab" | material: layers "poche" ("GENERIC_FLOOR" 0.300000011920929) | property sets: EPset_Parametric, EPset_Status
          15 x IFCGEOGRAPHICELEMENT | type IFCGEOGRAPHICELEMENTTYPE "PARKING STALL" | names: "GeographicElement" | material: "PARKING STALL" | property sets: BBIM_Array
          8 x IFCELEMENTASSEMBLY | ACCESSORY_ASSEMBLY | names: "WOOD TRUSS FLOOR" | material: "WOOD TRUSS - WEB"; "EXISTING WOOD TRUSS" | property sets: BBIM_Aggregate_Data
          5 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic - SQUARE:Nail - 04d - 12ga- 1.5"" | names: "BuildingElementProxy" | material: "FASTENER AT 24" O.C."
          2 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Nail - 04d - 12ga- .75"" | names: "BuildingElementProxy" | material: "<Unnamed>"
          2 x IFCCOLUMN | type IFCCOLUMNTYPE "4" METAL STUD SHAFT" | names: "Column" | material: profiles ("METAL C-H STUDS 25 GUAGE 24" O.C.") | property sets: EPset_Parametric
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Bathroom-Cabinet-Sink" | names: "Furniture" | property sets: Pset_FurnitureTypeCommon
          1 x IFCDOOR | type IFCDOORTYPE "DT01" | names: "Door" | property sets: EPset_Status
          2 x IFCDOOR | type IFCDOORTYPE "32"80"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          21 x IFCBEAM | type IFCBEAMTYPE "WOOD TRUSS - GENERIC" | names: "EXISTING TRUSSES" | material: profiles ("WOOD TRUSS") | property sets: EPset_Parametric, BBIM_Array, Pset_BeamCommon, EPset_Drawing
          2 x IFCBEAM | type IFCBEAMTYPE "(3) 2x8's (2 JACKS - 1 KING)" | names: "Beam" | material: profiles ("WOOD TRUSS") | property sets: Pset_BeamCommon, EPset_Parametric
          1 x IFCMEMBER | type IFCMEMBERTYPE "W12X35" | names: "Member" | material: profiles ("Unknown") | property sets: EPset_Parametric, Pset_MemberCommon
          3 x IFCSLAB | type IFCSLABTYPE "GENERIC FLOOR" | names: "Slab" | material: layers ("GENERIC_FLOOR" 1.) | property sets: EPset_Parametric, EPset_Drawing, EPset_Status
          1 x IFCSLAB | type IFCSLABTYPE "OVERALL SITE" | names: "Slab" | material: layers ("Unknown" 0.328083989501312) | property sets: EPset_Parametric, Qto_SlabBaseQuantities, EPset_Status
          2 x IFCACTUATOR | ELECTRICACTUATOR | names: "Cube" | material: "1" GYPSUM LINER PANEL"
          1 x IFCGEOGRAPHICELEMENT | type IFCGEOGRAPHICELEMENTTYPE "321723 - Pavement Markings - Aisle Strips" | names: "GeographicElement" | material: "PARKING STALL"
          1 x IFCGEOGRAPHICELEMENT | type IFCGEOGRAPHICELEMENTTYPE "321723 - Pavement Markings - Handicap Symbol" | names: "GeographicElement"
          3 x IFCDOOR | type IFCDOORTYPE "2'-6" X 6'-8"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "2'-4" X 6'-8"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "2'-4" X 6'-8"R" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "2'-6" X 6'-8"L" | names: "Door" | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: EPset_Status
          2 x IFCFURNITURE | type IFCFURNITURETYPE "Neufert Toilet with Cistern" | names: "Furniture" | property sets: EPset_Status
          1 x IFCSANITARYTERMINAL | SHOWER | names: "Plane" | property sets: EPset_Status
          1 x IFCSANITARYTERMINAL | type IFCSANITARYTERMINALTYPE "BathTub" | names: "SanitaryTerminal" | property sets: EPset_Status
          24 x IFCWALL | type IFCWALLTYPE "W6BØF" | names: "Wall" | material: layers "poche" ("SIDING TO MATCH EXISTING\nOVER BUILDING WRAP\nOVER 1/2" CDX/OSB\nOVER 2X6 STUDS 16" O.C. (R-20 BATT INSULATION)\nOVER VAPOR BARRIER\nOVER 1/2" GYP. BD." 0.0520833320915699, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.458332985639572, "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "1/2" WOOD SIDING" 0.0208330005407333) | property sets: EPset_Drawing, EPset_Parametric, EPset_Status
          2 x IFCWALL | type IFCWALLTYPE "W8AØF" | names: "Wall" | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.625, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: EPset_Parametric, EPset_Drawing, EPset_Status
          8 x IFCWALL | type IFCWALLTYPE "8" EXT-CONC. CAST" | names: "Wall" | material: layers ("8" CONCRETE FOUNDATION" 0.583333313465118) | property sets: EPset_Parametric, EPset_Status, EPset_Drawing
          4 x IFCWINDOW | type IFCWINDOWTYPE "DOUBLE HUNG:2'-0" X 4'-0"-XXX" | names: "Window" | property sets: EPset_Status
          2 x IFCWINDOW | type IFCWINDOWTYPE "5'-0" X 4'-4"" | names: "Window" | property sets: EPset_Status
          2 x IFCWINDOW | type IFCWINDOWTYPE "4'-8" X 4'-0"" | names: "Window" | property sets: EPset_Status
          3 x IFCWINDOW | type IFCWINDOWTYPE "5'-0" X 4'-6"" | names: "Window" | property sets: EPset_Status
          2 x IFCWINDOW | type IFCWINDOWTYPE "9'-0" X 4'-6"" | names: "Window" | property sets: EPset_Status
          1 x IFCDOOR | type IFCDOORTYPE "36"80"-P" | names: "Door" | property sets: EPset_Status
          1 x IFCWINDOW | type IFCWINDOWTYPE "DOUBLE HUNG:2'-0" X 4'-0"" | names: "Window" | property sets: EPset_Status
          3 x IFCWALL | type IFCWALLTYPE "16" CONC. FOOTING" | names: "Wall" | material: layers ("8"D X 16"W CONCRETE FOOTING W(2) CONT. #5's" 1.33333301544189) | property sets: EPset_Parametric, EPset_Status, EPset_Drawing
          1 x IFCSLAB | type IFCSLABTYPE "6 MIL VAPOR BARRIER" | names: "Slab" | material: layers ("6MIL VAPOR BARRIER - WITH\nTAPED/SEALED SEAMS AND EDGES\nOVER 6" MIN GRAVEL (FILL TO TOP OF FOOTING - NO FINES)" 0.0500000007450581) | property sets: EPset_Parametric, EPset_Status
          1 x IFCROOF | GABLE_ROOF | names: "Roof" | property sets: EPset_Status
          1 x IFCANNOTATION | type IFCTYPEPRODUCT "Material_Name" | object type "TEXT_LEADER" | names: "Material_Name"
          3 x IFCANNOTATION | type IFCTYPEPRODUCT "Material_Name_First_Item" | object type "TEXT_LEADER" | names: "Material_Name_First_Item"
          5 x IFCBEAM | names: "Beam", "2X4 BLOCKING" | material: "WOOD BLOCKING" | property sets: EPset_Parametric, BBIM_Array, EPset_Status, EPset_Drawing
          3 x IFCBEAM | type IFCBEAMTYPE "2x8 RIM JOIST" | names: "Beam" | material: profiles ("2X8 RIM JOIST") | property sets: EPset_Parametric, EPset_Status
          3 x IFCBEAM | type IFCBEAMTYPE "2x6 JOIST" | names: "Beam" | material: profiles ("2X6 TREATED SILL PLATE ON SILL GASKET -\n1/2" ANCHOR BOLTS @6' O.C. - 7" MIN. EMBED") | property sets: EPset_Parametric, EPset_Status
          8 x IFCELEMENTASSEMBLY | names: "Test Aggregate", "Assembly", "test-assembly" (+5 more) | material: "PREFABRICATED TRUSSES - 24" O.C." | property sets: BBIM_Aggregate_Data, BBIM_Array, EPset_Status
          1 x IFCFURNITURE | type IFCFURNITURETYPE "Closet-Linear" | names: "Furniture" | property sets: EPset_Status
          1 x IFCSLAB | type IFCSLABTYPE "COMPOSITE DECK - HORZ." | names: "Slab" | material: layers ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric, EPset_Status, EPset_Drawing
          2 x IFCSLAB | type IFCSLABTYPE "5/8 GYP CEILING" | names: "Slab" | material: layers "5Fill" ("5/8" GYP. BD @ CEILING" 0.0520830005407333) | property sets: EPset_Parametric, EPset_Status
          1 x IFCSLAB | type IFCSLABTYPE "SHINGLES + SHEATHING" | names: "Slab" | material: layers "5Fill" ("SHINGLES OVER 30 LB FELT - MATCH EXISTING" 0.0208330005407333, "1/2" OSB/CDX" 0.0416669994592667) | property sets: EPset_Parametric, EPset_Drawing
          1 x IFCSLAB | type IFCSLABTYPE "5/8" SUBFLOOR" | names: "Slab" | material: layers "5Fill" ("3/4" SUBFLOOR CDX/OSB SHEATHING" 0.0625) | property sets: EPset_Parametric, EPset_Status
          1 x IFCSANITARYTERMINAL | BATH | names: "BathroomCabinet" | property sets: EPset_Status
          2 x IFCFURNITURE | BED | names: "Mirror", "ClosetShelf" | property sets: EPset_Status
          1 x IFCSLAB | type IFCSLABTYPE "SHINGLES + SHEATHING" | BASESLAB | names: "Slab" | material: layers "5Fill" ("SHINGLES OVER 30 LB FELT - MATCH EXISTING" 0.0208330005407333, "1/2" OSB/CDX" 0.0416669994592667) | property sets: EPset_Parametric
          3 x IFCCOVERING | names: "ROOF-FASCIA" | material: "FASCIA" | property sets: EPset_Status
          1 x IFCROOF | type IFCROOFTYPE "ROOF" | object type "EXISTING-ROOF" | GABLE_ROOF | names: "Roof" | property sets: EPset_Status
          2 x IFCCOVERING | type IFCSLABTYPE "VENTED SOFFIT" | CEILING | names: "Slab" | material: layers "5Fill" ("VENTED SOFFIT TO MATCH EXISTING" 0.0520830005407333) | property sets: EPset_Parametric, EPset_Status
          1 x IFCWINDOW | type IFCWINDOWTYPE "SLIDER: 6'-0" X 2'-6"" | names: "Window" | property sets: EPset_Status
        IFCSPACE "105" | long name "BEDROOM"
        IFCSPACE "108" | long name "KITCHEN"
        IFCSPACE "101" | long name "BEDROOM"
        IFCSPACE "103" | long name "BATHROOM"
        IFCSPACE "102" | long name "CLOSET"
        IFCSPACE "107" | long name "LIVING ROOM"
        IFCSPACE "106" | long name "MECH/LAUNDRY"
        IFCSPACE "104" | long name "CLOSET"

Types
  IFCDOORTYPE "30"80"R" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "34"80"R" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:34" x 80":154791, Door-Single-Panel:34" x 80":154791:1, EPset_Drawing, Qto_DoorBaseQuantities | description "PREHUNG DOOR"
  IFCDOORTYPE "34"84"R" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:34" x 84":154865, Door-Single-Panel:34" x 84":154865:1, EPset_Drawing
  IFCDOORTYPE "36"80"R" | DOOR | SINGLE_SWING_RIGHT | 4 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:36" x 80":154902, Door-Single-Panel:36" x 80":154902:1, EPset_Drawing, Qto_DoorBaseQuantities | description "PREHUNG DOOR"
  IFCDOORTYPE "36"84"R" | DOOR | SINGLE_SWING_RIGHT | 5 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1
  IFCDOORTYPE "32"84"R" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:32" x 84":154765, Door-Single-Panel:32" x 84":154765:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "30"84"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, EPset_Drawing
  IFCWALLTYPE "W1" | STANDARD | 5 occurrences | material: layers "poche" ("1/2" WOOD SIDING" 0.0520833333333333, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.302083333333333, "1/2" WOOD SIDING" 0.0520833333333333) | description "(5/8 GYP - 3 5/8 METAL(BATT) - 5/8 GYP)"
  IFCDOORTYPE "30"84"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "34"80"L" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:34" x 80":154791, Door-Single-Panel:34" x 80":154791:1, EPset_Drawing
  IFCDOORTYPE "32"84"L" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:32" x 84":154765, Door-Single-Panel:32" x 84":154765:1, Pset_DoorCommon
  IFCDOORTYPE "34"84"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:34" x 84":154865, Door-Single-Panel:34" x 84":154865:1, Pset_DoorCommon, EPset_Drawing
  IFCDOORTYPE "36"80"L" | DOOR | SINGLE_SWING_LEFT | 10 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:36" x 80":154902, Door-Single-Panel:36" x 80":154902:1, EPset_Drawing, Qto_DoorBaseQuantities | description "PREHUNG DOOR"
  IFCDOORTYPE "36"84"L" | DOOR | SINGLE_SWING_RIGHT | 4 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, EPset_Drawing
  IFCWALLTYPE "EXT-VINYL" | STANDARD | 17 occurrences | material: layers "HorzLines6in96scale" ("GENERIC POCHE" 0.583333313465118) | property sets: Pset_ElementShading, Pset_ProductRequirements
  IFCWALLTYPE "EXT-BRICK" | STANDARD | 2 occurrences | material: layers "BrickElevation" ("BRICK" 0.583333313465118) | property sets: Pset_ElementShading, Pset_ProductRequirements
  IFCWALLTYPE "W4AØF" | STANDARD | 64 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_ElementShading, Pset_ProductRequirements, EPset_Drawing | description "5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP"
  IFCWALLTYPE "W4B2D" | STANDARD | 2 occurrences | material: layers "poche" ("1/2" WOOD SIDING" 0.0520830005407333, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520830005407333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.291666666666667, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "1/2" WOOD SIDING" 0.0520830005407333) | property sets: Pset_ElementShading, Pset_ProductRequirements, EPset_Drawing | description "5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP"
  IFCDOORTYPE "30"80"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, Pset_DoorCommon, EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "Core_Fill_8in" | COMPLEX | 10 occurrences | property sets: EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "Horz Ladder Reinforcing" | COMPLEX | 1 occurrence
  IFCBUILDINGELEMENTPROXYTYPE "8inCMU" | COMPLEX | 10 occurrences | property sets: EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "Morter_8inCMU" | COMPLEX | 11 occurrences | property sets: EPset_Drawing
  IFCCOLUMNTYPE "C1 Copy" | 3 occurrences | material: profiles ("Unknown")
  IFCSLABTYPE "SIDEWALK" | FLOOR | 10 occurrences | material: layers "20Fill" ("8"D X 16"W CONCRETE FOOTING W(2) CONT. #5's" 0.5) | property sets: EPset_Parametric
  IFCSLABTYPE "CONCRETE SLAB" | FLOOR | 1 occurrence | material: layers "5Fill" ("8"D X 16"W CONCRETE FOOTING W(2) CONT. #5's" 0.5) | property sets: EPset_Parametric
  IFCWINDOWTYPE "WT01 3.6''x5.4'" | 6 occurrences | property sets: EPset_Drawing
  IFCCOVERINGTYPE "COV30" | 15 occurrences | material: layers ("Unknown" 0.0984251968503937) | property sets: EPset_Parametric
  IFCCOVERINGTYPE "COV10" | 1 occurrence | material: layers ("Unknown" 0.0328083989501312)
  IFCWINDOWTYPE "WT01 4.0'x5.4'" | 1 occurrence
  IFCBEAMTYPE "Curb" | BEAM | 2 occurrences | material: profiles ("RAMP CURB")
  IFCBEAMTYPE "Curb 1.6'x1.6'" | BEAM | 1 occurrence | material: profiles ("RAMP CURB")
  IFCWINDOWTYPE "WT01 6.0'x3.8'" | 2 occurrences | property sets: EPset_Drawing
  IFCWINDOWTYPE "WT01 2.6'x2.6'" | 3 occurrences
  IFCWALLTYPE "W6AØF" | STANDARD | 1 occurrence | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.458333343267441, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_ElementShading, Pset_ProductRequirements, EPset_Drawing | description "5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP"
  IFCFURNITURETYPE "Table-Dinning" | TABLE | 1 occurrence | property sets: EPset_Drawing
  IFCFURNITURETYPE "Furniture-Stool" | CHAIR | 1 occurrence | property sets: EPset_Drawing
  IFCCOVERINGTYPE "TYPEX" | FLOORING | 1 occurrence | material: layers "10Fill" ("Unknown" 0.020833333954215) | property sets: EPset_Parametric
  IFCFURNITURETYPE "Generic 3-Seater Sofa" | 2 occurrences
  IFCFURNITURETYPE "Generic Medium Coffee Table" | 2 occurrences | property sets: EPset_Drawing
  IFCFURNITURETYPE "Chair-Dining" | CHAIR | 6 occurrences
  IFCSANITARYTERMINALTYPE "Neufert Toilet with Cistern" | 1 occurrence | property sets: EPset_Drawing
  IFCFURNITURETYPE "Chair-BarStool" | CHAIR | 5 occurrences | property sets: EPset_Drawing
  IFCFURNITURETYPE "Bed-King" | BED | 2 occurrences
  IFCDOORTYPE "G36"80"L" | DOOR | SINGLE_SWING_LEFT | 3 occurrences | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, Qto_DoorBaseQuantities, EPset_Drawing | description "GLASS INSET (TEMPERED GLAZING)"
  IFCDOORTYPE "G36"80"R" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | property sets: Door-Single-Panel:36" x 84":154924, Door-Single-Panel:36" x 84":154924:1, Qto_DoorBaseQuantities
  IFCDOORTYPE "S96"80"" | DOOR | DOUBLE_DOOR_SLIDING | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, EPset_Drawing, Qto_DoorBaseQuantities | description "SLIDING CLOSET DOOR"
  IFCDOORTYPE "S60"80"" | DOOR | DOUBLE_DOOR_SLIDING | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, EPset_Drawing, Qto_DoorBaseQuantities | description "SLIDING CLOSET DOOR"
  IFCWALLTYPE "M4B2D" | STANDARD | 5 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0625, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FO" 0.333333343267441, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0833333358168602) | property sets: Pset_ElementShading, Pset_ProductRequirements, EPset_Drawing, Pset_WallCommon | description "5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP"
  IFCELECTRICAPPLIANCETYPE "W/D" | WASHINGMACHINE | 1 occurrence
  IFCDOORTYPE "S72"80"" | DOOR | DOUBLE_DOOR_SLIDING | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, EPset_Drawing
  IFCDOORTYPE "S90"80"" | DOOR | DOUBLE_DOOR_SLIDING | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1
  IFCDOORTYPE "S84"80"" | DOOR | DOUBLE_DOOR_SLIDING | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "Wood - Birch - Solid Stained Light Low Gloss", "Trim": "Paint - Sienna") | property sets: Door-Single-Panel:30" x 84":154723, Door-Single-Panel:30" x 84":154723:1, EPset_Drawing
  IFCELECTRICAPPLIANCETYPE "Neufert Cooktop 75x51" | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "DW" | 1 occurrence
  IFCWINDOWTYPE "W1" | WINDOW | 6 occurrences | material: constituents ("DOOR TRIM", "WINDOW", "INSULATED GLAZING") | property sets: EPset_Drawing
  IFCSANITARYTERMINALTYPE "Generic Medium Sink" | 2 occurrences
  IFCSANITARYTERMINALTYPE "TUB:1:2901065" | BATH | 1 occurrence
  IFCELECTRICAPPLIANCETYPE "TV" | 1 occurrence | material: constituents ("TV")
  IFCBUILDINGELEMENTPROXYTYPE "Cube" | 6 occurrences | property sets: EPset_Drawing
  IFCWALLTYPE "EXT-EIFS" | STANDARD | 6 occurrences | material: layers "10Fill" ("EIFS" 0.583333313465118) | property sets: Pset_ElementShading, Pset_ProductRequirements
  IFCWINDOWTYPE "4'x5.4'" | 1 occurrence | property sets: EPset_Drawing
  IFCSLABTYPE "GRASS2" | 7 occurrences | material: layers "grass" ("GRASS" 0.5) | property sets: EPset_Parametric
  IFCSLABTYPE "ASPHALT DRIVE WAY" | 2 occurrences | material: layers "10Fill" ("ASPHALT DRIVEWAY" 0.5)
  IFCSLABTYPE "ROOF" | 13 occurrences | material: layers "poche" ("GENERIC_FLOOR" 0.300000011920929)
  IFCGEOGRAPHICELEMENTTYPE "PARKING STALL" | 15 occurrences | material: "PARKING STALL" | property sets: EPset_Drawing
  IFCBUILDINGELEMENTPROXYTYPE "060523 - W_P_C - Fastenings - Generic - SQUARE:Nail - 04d - 12ga- 1.5"" | 5 occurrences | material: "FASTENER AT 24" O.C." | property sets: Pset_BuildingElementProxyCommon
  IFCBUILDINGELEMENTPROXYTYPE "Nail - 04d - 12ga- .75"" | 2 occurrences | material: "<Unnamed>" | property sets: Pset_BuildingElementProxyCommon
  IFCCOLUMNTYPE "4" METAL STUD SHAFT" | COLUMN | 2 occurrences | material: profiles ("METAL C-H STUDS 25 GUAGE 24" O.C.")
  IFCFURNITURETYPE "Bathroom-Cabinet-Sink" | 1 occurrence
  IFCDOORTYPE "DT01" | 1 occurrence
  IFCDOORTYPE "32"80"L" | DOOR | SINGLE_SWING_RIGHT | 2 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:32" x 84":154765, Door-Single-Panel:32" x 84":154765:1, Pset_DoorCommon
  IFCBEAMTYPE "WOOD TRUSS - GENERIC" | BEAM | 21 occurrences | material: profiles ("WOOD TRUSS")
  IFCBEAMTYPE "(3) 2x8's (2 JACKS - 1 KING)" | BEAM | 2 occurrences | material: profiles ("WOOD TRUSS")
  IFCMEMBERTYPE "W12X35" | 1 occurrence | material: profiles ("Unknown")
  IFCSLABTYPE "GENERIC FLOOR" | 3 occurrences | material: layers ("GENERIC_FLOOR" 1.)
  IFCSLABTYPE "OVERALL SITE" | BASESLAB | 1 occurrence | material: layers ("Unknown" 0.328083989501312) | property sets: EPset_Parametric
  IFCGEOGRAPHICELEMENTTYPE "321723 - Pavement Markings - Aisle Strips" | 1 occurrence | material: "PARKING STALL"
  IFCGEOGRAPHICELEMENTTYPE "321723 - Pavement Markings - Handicap Symbol" | 1 occurrence | property sets: EPset_Drawing
  IFCDOORTYPE "2'-6" X 6'-8"R" | DOOR | SINGLE_SWING_RIGHT | 3 occurrences | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, EPset_Drawing
  IFCDOORTYPE "2'-4" X 6'-8"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, EPset_Drawing
  IFCDOORTYPE "2'-4" X 6'-8"R" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM", "Jamb": "DOOR JAMB", "Swing": "DOOR SWING") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, EPset_Drawing
  IFCDOORTYPE "2'-6" X 6'-8"L" | DOOR | SINGLE_SWING_RIGHT | 1 occurrence | material: constituents "MaterialConstituentSet" ("Panel": "DOOR PANEL", "Trim": "DOOR TRIM") | property sets: Door-Single-Panel:30" x 80":154643, Door-Single-Panel:30" x 80":154643:1, EPset_Drawing
  IFCFURNITURETYPE "Neufert Toilet with Cistern" | 2 occurrences | property sets: EPset_Drawing
  IFCSANITARYTERMINALTYPE "BathTub" | BATH | 1 occurrence
  IFCWALLTYPE "W6BØF" | STANDARD | 24 occurrences | material: layers "poche" ("SIDING TO MATCH EXISTING\nOVER BUILDING WRAP\nOVER 1/2" CDX/OSB\nOVER 2X6 STUDS 16" O.C. (R-20 BATT INSULATION)\nOVER VAPOR BARRIER\nOVER 1/2" GYP. BD." 0.0520833320915699, "METAL STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.458332985639572, "3/4" CDX OR OSB PLYWOOD - SEE STRUCT DWGS" 0.0625, "1/2" WOOD SIDING" 0.0208330005407333) | description "5/8 GYP - 6 METAL(BATT) - 5/8 GYP"
  IFCWALLTYPE "W8AØF" | STANDARD | 2 occurrences | material: layers "poche" ("5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333, "2X WOOD STUD - (SEE 'WALL TAG' & 'LAYER MATERIAL SCHEDULE' FOR SIZE, SPACING, & INSULATION)" 0.625, "5/8" GYP. BD OR CEMENT BACKERBOARD ON WET WALL" 0.0520833333333333) | property sets: Pset_ElementShading, Pset_ProductRequirements, EPset_Drawing | description "5/8 GYP - 2X4 WOOD(BATT) - 5/8 GYP"
  IFCWALLTYPE "8" EXT-CONC. CAST" | STANDARD | 8 occurrences | material: layers ("8" CONCRETE FOUNDATION" 0.583333313465118) | property sets: Pset_ElementShading, Pset_ProductRequirements, Pset_WallCommon
  IFCWINDOWTYPE "DOUBLE HUNG:2'-0" X 4'-0"-XXX" | 4 occurrences | property sets: EPset_Drawing
  IFCWINDOWTYPE "5'-0" X 4'-4"" | 2 occurrences | property sets: EPset_Drawing
  IFCWINDOWTYPE "4'-8" X 4'-0"" | 2 occurrences | property sets: EPset_Drawing
  IFCWINDOWTYPE "5'-0" X 4'-6"" | 3 occurrences | property sets: EPset_Drawing
  IFCWINDOWTYPE "9'-0" X 4'-6"" | 2 occurrences | property sets: EPset_Drawing
  IFCDOORTYPE "36"80"-P" | 1 occurrence | property sets: EPset_Drawing
  IFCWINDOWTYPE "DOUBLE HUNG:2'-0" X 4'-0"" | 1 occurrence | property sets: EPset_Drawing
  IFCWALLTYPE "16" CONC. FOOTING" | STANDARD | 3 occurrences | material: layers ("8"D X 16"W CONCRETE FOOTING W(2) CONT. #5's" 1.33333301544189) | property sets: Pset_ElementShading, Pset_ProductRequirements
  IFCSLABTYPE "6 MIL VAPOR BARRIER" | FLOOR | 1 occurrence | material: layers ("6MIL VAPOR BARRIER - WITH\nTAPED/SEALED SEAMS AND EDGES\nOVER 6" MIN GRAVEL (FILL TO TOP OF FOOTING - NO FINES)" 0.0500000007450581) | property sets: EPset_Parametric
  IFCTYPEPRODUCT "Material_Name" | 1 occurrence | property sets: EPset_Drawing
  IFCTYPEPRODUCT "Material_Name_First_Item" | 3 occurrences | property sets: EPset_Drawing
  IFCBEAMTYPE "2x8 RIM JOIST" | BEAM | 3 occurrences | material: profiles ("2X8 RIM JOIST")
  IFCBEAMTYPE "2x6 JOIST" | BEAM | 3 occurrences | material: profiles ("2X6 TREATED SILL PLATE ON SILL GASKET -\n1/2" ANCHOR BOLTS @6' O.C. - 7" MIN. EMBED")
  IFCFURNITURETYPE "Closet-Linear" | SHELF | 1 occurrence
  IFCSLABTYPE "COMPOSITE DECK - HORZ." | FLOOR | 1 occurrence | material: layers ("COMPOSITE DECKING" 0.0719999969005585) | property sets: EPset_Parametric
  IFCSLABTYPE "5/8 GYP CEILING" | FLOOR | 2 occurrences | material: layers "5Fill" ("5/8" GYP. BD @ CEILING" 0.0520830005407333) | property sets: EPset_Parametric
  IFCSLABTYPE "SHINGLES + SHEATHING" | FLOOR | 2 occurrences | material: layers "5Fill" ("SHINGLES OVER 30 LB FELT - MATCH EXISTING" 0.0208330005407333, "1/2" OSB/CDX" 0.0416669994592667) | property sets: EPset_Parametric
  IFCSLABTYPE "5/8" SUBFLOOR" | FLOOR | 1 occurrence | material: layers "5Fill" ("3/4" SUBFLOOR CDX/OSB SHEATHING" 0.0625) | property sets: EPset_Parametric
  IFCROOFTYPE "ROOF" | HIP_ROOF | 1 occurrence | property sets: BBIM_Roof
  IFCSLABTYPE "VENTED SOFFIT" | FLOOR | 2 occurrences | material: layers "5Fill" ("VENTED SOFFIT TO MATCH EXISTING" 0.0520830005407333) | property sets: EPset_Parametric
  IFCWINDOWTYPE "SLIDER: 6'-0" X 2'-6"" | 1 occurrence | property sets: EPset_Drawing

Property sets
  EPset_Drawing | properties | on 152 objects (60 IFCANNOTATION, 55 IFCWALL, 9 IFCSLAB, 8 IFCBUILDINGELEMENTPROXY) | on 49 type objects
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
  EPset_Drawing | properties | on 8 objects (8 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/2"=1'-0"" (IFCLABEL)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/24" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 5 objects (5 IFCANNOTATION)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "3"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCURIREFERENCE)
    Metadata = "material.Category" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCURIREFERENCE)
    Scale = "1/4" (IFCLABEL)
    Stylesheet = "drawings\assets\default.css" (IFCURIREFERENCE)
    Symbols = "drawings\assets\symbols.svg" (IFCURIREFERENCE)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 2 objects (2 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    Exclude = "IfcPipeSegment +IfcDuctSegment + IfcVirtualElement + IfcObject, EPset_Status.Status="DEMOLISH" + IfcFooting, ObjectType = Backfill" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "3/8"=1'-0"" (IFCLABEL)
    ImperialPrecision = "1" (IFCLABEL)
    JoinCriteria = "EPset_Status.Status, mats.Category" (IFCTEXT)
    Markers = "drawings/assets/markers.svg" (IFCTEXT)
    Metadata = "EPset_Status.Status, mats.Category.0, predefined_type" (IFCTEXT)
    Patterns = "drawings/assets/patterns.svg" (IFCTEXT)
    Scale = "1/32" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings/assets/default.css" (IFCTEXT)
    Symbols = "drawings/assets/symbols.svg" (IFCTEXT)
    TargetView = "ELEVATION_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION) | on 2 type objects
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = TRUE (IFCBOOLEAN)
  EPset_Drawing | properties | on 1 object (1 IFCDOOR) | on 1 type object
    HasAnnotation = FALSE (IFCBOOLEAN)
    HasLinework = FALSE (IFCBOOLEAN)
    HasUnderlay = TRUE (IFCBOOLEAN)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    Exclude = "IfcObject , EPset_Status.Status="NEW"" (IFCTEXT)
    GlobalReferencing = TRUE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/4"=1'-0"" (IFCLABEL)
    ImperialPrecision = "1/2" (IFCLABEL)
    JoinCriteria = "EPset_Status.Status" (IFCTEXT)
    Markers = "drawings\assets\markers.svg" (IFCTEXT)
    Metadata = "EPset_Status.Status" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCTEXT)
    Scale = "1/48" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings\assets\default.css" (IFCTEXT)
    Symbols = "drawings\assets\symbols.svg" (IFCTEXT)
    TargetView = "PLAN_VIEW" (IFCLABEL)
  EPset_Drawing | properties | on 1 object (1 IFCANNOTATION)
    CurrentShadingStyle = "Blender Default" (IFCLABEL)
    GlobalReferencing = FALSE (IFCBOOLEAN)
    HasAnnotation = TRUE (IFCBOOLEAN)
    HasLinework = TRUE (IFCBOOLEAN)
    HasUnderlay = FALSE (IFCBOOLEAN)
    HumanScale = "1/8"=1'-0"" (IFCLABEL)
    Markers = "drawings\assets\markers.svg" (IFCTEXT)
    Patterns = "drawings\assets\patterns.svg" (IFCTEXT)
    Scale = "1/96" (IFCLABEL)
    ShadingStyles = "drawings/assets/shading_styles.json" (IFCTEXT)
    Stylesheet = "drawings\assets\default.css" (IFCTEXT)
    Symbols = "drawings\assets\symbols.svg" (IFCTEXT)
    TargetView = "SECTION_VIEW" (IFCLABEL)
  EPset_Drawing: 35 more contents on 35 objects not shown
  EPset_Annotation | properties | on 23 objects (23 IFCANNOTATION)
    Classes = "fill-bg" (IFCLABEL)
  EPset_Annotation | properties | on 21 objects (21 IFCANNOTATION)
    Classes = "fill-bg" (IFCTEXT)
  EPset_Annotation | properties | on 16 objects (16 IFCANNOTATION)
    Classes = "small fill-bg" (IFCLABEL)
  EPset_Annotation | properties | on 8 objects (8 IFCANNOTATION)
    Classes = "oblique, fill-bg" (IFCLABEL)
  EPset_Annotation | properties | on 2 objects (2 IFCANNOTATION)
    Classes = "large" (IFCLABEL)
  EPset_Annotation | properties | on 1 object (1 IFCANNOTATION)
    Classes = "header" (IFCLABEL)
  EPset_Annotation | properties | on 1 object (1 IFCANNOTATION)
    Classes = "oblique fill-bg" (IFCLABEL)
  EPset_Parametric | properties | on 148 objects (145 IFCWALL, 3 IFCCOVERING)
    Engine = "BlenderBIM.DumbLayer2" (IFCLABEL)
  EPset_Parametric | properties | on 118 objects (112 IFCBEAM, 5 IFCCOLUMN, 1 IFCMEMBER)
    Engine = "BlenderBIM.DumbProfile" (IFCLABEL)
  EPset_Parametric | properties | on 62 objects (44 IFCSLAB, 18 IFCCOVERING)
    Engine = "BlenderBIM.DumbLayer3" (IFCLABEL)
  EPset_Parametric | properties | on 12 type objects
    LayerSetDirection = "AXIS3" (IFCLABEL)
  BBIM_Array | properties | on 20 objects (20 IFCBEAM)
    Data (no value)
    Parent = "227zWoiIj96xv8sEFA2$pF" (IFCLABEL)
  BBIM_Array | properties | on 10 objects (10 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "3iGRJZfy51iAd8K3LgiYDq" (IFCLABEL)
  BBIM_Array | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "0zDYnHKt9D9xBQ0J7EbG8P" (IFCLABEL)
  BBIM_Array | properties | on 9 objects (9 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "0QwQTUhPr6EAqfEjNat8se" (IFCLABEL)
  BBIM_Array | properties | on 9 objects (9 IFCGEOGRAPHICELEMENT)
    Data (no value)
    Parent = "1vMyIV3ln5CA9HgV3nDC3Z" (IFCLABEL)
  BBIM_Array | properties | on 6 objects (6 IFCBEAM)
    Data (no value)
    Parent = "1ZpGJbE6L2GulI5Ju5dUNo" (IFCLABEL)
  BBIM_Array | properties | on 6 objects (6 IFCBEAM)
    Data (no value)
    Parent = "328PJNNIH4LwFJM_vVCEhd" (IFCLABEL)
  BBIM_Array | properties | on 4 objects (4 IFCBUILDINGELEMENTPROXY)
    Data (no value)
    Parent = "3QecqJiErB$9TeAgOjclzW" (IFCLABEL)
  BBIM_Array: 13 more contents on 23 objects not shown
  Pset_WallCommon | properties | on 25 objects (25 IFCWALL)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_WallCommon | properties | on 23 objects (23 IFCWALL)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_WallCommon | properties | on 16 objects (16 IFCWALL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_WallCommon | properties | on 16 objects (16 IFCWALL)
    Status in {"NEW"} (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    LoadBearing = TRUE (IFCBOOLEAN)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL) | on 1 type object
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_WallCommon | properties | on 1 object (1 IFCFURNITURE)
    Status in {"NEW"} (IFCTEXT)
  Pset_WallCommon | properties | on 1 type object
    FireRating = "2 HR" (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 25 objects (25 IFCFURNITURE)
    Status in {"NEW"} (IFCLABEL)
  Pset_FurnitureTypeCommon | properties | on 2 objects (2 IFCFURNITURE)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  BBIM_Stair | properties | on 1 object (1 IFCSTAIRFLIGHT)
    Data = "{"stair_type": "CONCRETE", "width": 3.967010021209717, "height": 3.9708399772644043, "number_of_treads": 6, "tread_run": 0.8342519998550415, "base_slab_depth": 0.8202099800109863, "top_slab_depth": 0.8202099800109863, "has_top_nib": true, "tread_depth": 0.8202099800109863}" (IFCLABEL)
  BBIM_Stair | properties | on 1 object (1 IFCSTAIRFLIGHT)
    Data = "{"stair_type": "CONCRETE", "width": 3.967010021209717, "height": 3.8508400917053223, "number_of_treads": 6, "tread_run": 1.179252028465271, "base_slab_depth": 0.8202099800109863, "top_slab_depth": 0.8202099800109863, "has_top_nib": true, "tread_depth": 0.8202099800109863}" (IFCLABEL)
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NumberOfRiser = 7. (IFCCOUNTMEASURE)
    NumberOfTreads = 6. (IFCCOUNTMEASURE)
    RiserHeight = 0.567262828350067 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Status in {"EXISTING"} (IFCLABEL)
    TreadLength = 0.820209980010986 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_StairFlightCommon | properties | on 1 object (1 IFCSTAIRFLIGHT)
    NumberOfRiser = 7. (IFCCOUNTMEASURE)
    NumberOfTreads = 6. (IFCCOUNTMEASURE)
    RiserHeight = 0.550119996070862 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
    Status in {"EXISTING"} (IFCLABEL)
    TreadLength = 0.820209980010986 (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  OD_Options | properties | on 37 objects (23 IFCFURNITURE, 10 IFCWALL, 3 IFCDOOR, 1 IFCSANITARYTERMINAL)
    OD_Option_2 = "N" (IFCTEXT)
  OD_Options | properties | on 8 objects (5 IFCANNOTATION, 2 IFCWALL, 1 IFCFURNITURE)
    OD_Option_1 = "" (IFCTEXT)
    OD_Option_2 = "N" (IFCTEXT)
  Pset_WindowCommon | properties | on 7 objects (7 IFCWINDOW)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_WindowCommon | properties | on 2 objects (2 IFCWINDOW)
    Status in {"NEW"} (IFCLABEL)
  Pset_SlabCommon | properties | on 7 objects (7 IFCSLAB)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    Status in {"NEW"} (IFCLABEL)
  Pset_ColumnCommon | properties | on 3 objects (3 IFCCOLUMN)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_SanitaryTerminalTypeCommon | properties | on 3 objects (3 IFCSANITARYTERMINAL)
    Status in {"NEW"} (IFCLABEL)
  Qto_CoveringBaseQuantities | quantities | on 1 object (1 IFCCOVERING)
    GrossArea = 1222.801 [square foot (conversion based)]
    NetArea = 1222.801 [square foot (conversion based)]
    Width = 0.021 [foot (conversion based)]
  Pset_CoveringCommon | properties | on 15 objects (15 IFCCOVERING)
    Status in {"EXISTING", "DEMOLISH"} (IFCTEXT)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_CoveringCommon | properties | on 1 object (1 IFCCOVERING)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_ElectricApplianceTypeCommon | properties | on 4 objects (4 IFCELECTRICAPPLIANCE)
    Status in {"NEW"} (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 6 objects (6 IFCBUILDINGELEMENTPROXY)
    Status in {"EXISTING"} (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Status in {"NEW"} (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 2 type objects
    IsExternal = FALSE (IFCBOOLEAN)
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossFootprintArea = 22.514 [square foot (conversion based)]
    GrossSideArea = 379.868 [square foot (conversion based)]
    GrossVolume = 221.59 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    Length = 38.595 [foot (conversion based)]
    NetFootprintArea = 22.514 [square foot (conversion based)]
    NetSideArea = 379.868 [square foot (conversion based)]
    NetVolume = 221.59 [cubic foot (conversion based)]
    Width = 0.583 [foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 2 objects (2 IFCWALL)
    GrossFootprintArea = 4.078 [square foot (conversion based)]
    GrossSideArea = 101.398 [square foot (conversion based)]
    GrossVolume = 40.137 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    Length = 10.302 [foot (conversion based)]
    NetFootprintArea = 2.956 [square foot (conversion based)]
    NetSideArea = 82.51 [square foot (conversion based)]
    NetVolume = 32.66 [cubic foot (conversion based)]
    Width = 0.396 [foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 31.639 [square foot (conversion based)]
    GrossSideArea = 533.836 [square foot (conversion based)]
    GrossVolume = 311.404 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    Length = 54.238 [foot (conversion based)]
    NetFootprintArea = 29.889 [square foot (conversion based)]
    NetSideArea = 480.836 [square foot (conversion based)]
    NetVolume = 280.488 [cubic foot (conversion based)]
    Width = 0.583 [foot (conversion based)]
  Qto_WallBaseQuantities | quantities | on 1 object (1 IFCWALL)
    GrossFootprintArea = 6.903 [square foot (conversion based)]
    GrossSideArea = 171.638 [square foot (conversion based)]
    GrossVolume = 67.94 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    Length = 17.438 [foot (conversion based)]
    NetFootprintArea = 6.903 [square foot (conversion based)]
    NetSideArea = 171.638 [square foot (conversion based)]
    NetVolume = 67.94 [cubic foot (conversion based)]
    Width = 0.396 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 8 objects (8 IFCSLAB)
    Depth = 0.5 [foot (conversion based)]
    GrossArea = 289.298 [square foot (conversion based)]
    GrossVolume = 144.649 [cubic foot (conversion based)]
    Length = 42.132 [foot (conversion based)]
    NetArea = 289.298 [square foot (conversion based)]
    NetVolume = 144.649 [cubic foot (conversion based)]
    Perimeter = 138.951 [foot (conversion based)]
    Width = 23.225 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 3 objects (3 IFCSLAB)
    Depth = 0.5 [foot (conversion based)]
    GrossArea = 8410.203 [square foot (conversion based)]
    GrossVolume = 4205.101 [cubic foot (conversion based)]
    Length = 136.89 [foot (conversion based)]
    NetArea = 8410.203 [square foot (conversion based)]
    NetVolume = 4205.101 [cubic foot (conversion based)]
    Perimeter = 619.344 [foot (conversion based)]
    Width = 111.7 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.5 [foot (conversion based)]
    GrossArea = 8410.202 [square foot (conversion based)]
    GrossVolume = 4205.101 [cubic foot (conversion based)]
    Length = 136.89 [foot (conversion based)]
    NetArea = 8410.202 [square foot (conversion based)]
    NetVolume = 4205.101 [cubic foot (conversion based)]
    Perimeter = 619.344 [foot (conversion based)]
    Width = 111.7 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.5 [foot (conversion based)]
    GrossArea = 103.56 [square foot (conversion based)]
    GrossVolume = 51.78 [cubic foot (conversion based)]
    Length = 31.653 [foot (conversion based)]
    NetArea = 103.56 [square foot (conversion based)]
    NetVolume = 51.78 [cubic foot (conversion based)]
    Perimeter = 66.781 [foot (conversion based)]
    Width = 4.327 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.5 [foot (conversion based)]
    GrossArea = 717.516 [square foot (conversion based)]
    GrossVolume = 358.758 [cubic foot (conversion based)]
    Length = 135.008 [foot (conversion based)]
    NetArea = 717.516 [square foot (conversion based)]
    NetVolume = 358.758 [cubic foot (conversion based)]
    Perimeter = 298.373 [foot (conversion based)]
    Width = 15.212 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.5 [foot (conversion based)]
    GrossArea = 1624.966 [square foot (conversion based)]
    GrossVolume = 812.483 [cubic foot (conversion based)]
    Length = 84.5 [foot (conversion based)]
    NetArea = 1624.966 [square foot (conversion based)]
    NetVolume = 812.483 [cubic foot (conversion based)]
    Perimeter = 244.154 [foot (conversion based)]
    Width = 37.956 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.5 [foot (conversion based)]
    GrossArea = 122.867 [square foot (conversion based)]
    GrossVolume = 61.433 [cubic foot (conversion based)]
    Length = 29.52 [foot (conversion based)]
    NetArea = 122.867 [square foot (conversion based)]
    NetVolume = 61.433 [cubic foot (conversion based)]
    Perimeter = 67.364 [foot (conversion based)]
    Width = 4.204 [foot (conversion based)]
  Qto_SlabBaseQuantities | quantities | on 1 object (1 IFCSLAB)
    Depth = 0.5 [foot (conversion based)]
    GrossArea = 123.349 [square foot (conversion based)]
    GrossVolume = 61.675 [cubic foot (conversion based)]
    Length = 25.089 [foot (conversion based)]
    NetArea = 123.349 [square foot (conversion based)]
    NetVolume = 61.675 [cubic foot (conversion based)]
    Perimeter = 64.081 [foot (conversion based)]
    Width = 9.67 [foot (conversion based)]
  Qto_SlabBaseQuantities: 3 more contents on 3 objects not shown
  BBIM_Dimension | properties | on 4 objects (4 IFCANNOTATION)
    ShowDescriptionOnly = TRUE (IFCBOOLEAN)
  BBIM_Aggregate_Data | properties | on 3 objects (3 IFCELEMENTASSEMBLY)
    Data = "[{"children": [], "instance_of": ["3fzeczmmTDzODy5MoOxgsJ"]}]" (IFCLABEL)
    Parent = "0fSC_1z0z88vOeLw0MY65G" (IFCLABEL)
  BBIM_Aggregate_Data | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Data = "[{"children": ["3Dle5DqG1FefxYjQoUGyXK", "0Ux$hg0zX87xUKX5k2fCba", "2UgekhTl15V9PhnLli1APp"], "instance_of": ["1Q$OMoL7f7FQALQ3YyPPRT"]}]" (IFCTEXT)
    Parent = "1wBA4yFC9Ai863jtP5Qykc" (IFCLABEL)
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 179.382 [square foot (conversion based)]
    GrossFloorArea = 179.382 [square foot (conversion based)]
    GrossPerimeter = 57.105 [foot (conversion based)]
    GrossVolume = 1765.575 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 179.382 [square foot (conversion based)]
    NetFloorArea = 179.382 [square foot (conversion based)]
    NetVolume = 1765.575 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 282.46 [square foot (conversion based)]
    GrossFloorArea = 282.46 [square foot (conversion based)]
    GrossPerimeter = 68.917 [foot (conversion based)]
    GrossVolume = 2780.121 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 282.46 [square foot (conversion based)]
    NetFloorArea = 282.46 [square foot (conversion based)]
    NetVolume = 2780.121 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 249.966 [square foot (conversion based)]
    GrossFloorArea = 249.966 [square foot (conversion based)]
    GrossPerimeter = 80.853 [foot (conversion based)]
    GrossVolume = 2460.292 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 0. [square foot (conversion based)]
    NetFloorArea = 249.966 [square foot (conversion based)]
    NetVolume = 2460.292 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 70.842 [square foot (conversion based)]
    GrossFloorArea = 70.842 [square foot (conversion based)]
    GrossPerimeter = 38.048 [foot (conversion based)]
    GrossVolume = 697.268 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 70.842 [square foot (conversion based)]
    NetFloorArea = 70.842 [square foot (conversion based)]
    NetVolume = 697.268 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 50.426 [square foot (conversion based)]
    GrossFloorArea = 50.426 [square foot (conversion based)]
    GrossPerimeter = 29.914 [foot (conversion based)]
    GrossVolume = 496.316 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 50.426 [square foot (conversion based)]
    NetFloorArea = 50.426 [square foot (conversion based)]
    NetVolume = 496.316 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 19.207 [square foot (conversion based)]
    GrossFloorArea = 19.207 [square foot (conversion based)]
    GrossPerimeter = 23.222 [foot (conversion based)]
    GrossVolume = 189.043 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 0. [square foot (conversion based)]
    NetFloorArea = 19.207 [square foot (conversion based)]
    NetVolume = 189.043 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 11.32 [square foot (conversion based)]
    GrossFloorArea = 11.32 [square foot (conversion based)]
    GrossPerimeter = 15.315 [foot (conversion based)]
    GrossVolume = 111.415 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 0. [square foot (conversion based)]
    NetFloorArea = 11.32 [square foot (conversion based)]
    NetVolume = 111.415 [cubic foot (conversion based)]
  Qto_SpaceBaseQuantities | quantities | on 1 object (1 IFCSPACE)
    FinishCeilingHeight = 9.843 [foot (conversion based)]
    FinishFloorHeight = 0. [foot (conversion based)]
    GrossCeilingArea = 222.81 [square foot (conversion based)]
    GrossFloorArea = 222.81 [square foot (conversion based)]
    GrossPerimeter = 69.843 [foot (conversion based)]
    GrossVolume = 2193.01 [cubic foot (conversion based)]
    Height = 9.843 [foot (conversion based)]
    NetCeilingArea = 0. [square foot (conversion based)]
    NetFloorArea = 222.81 [square foot (conversion based)]
    NetVolume = 2193.01 [cubic foot (conversion based)]
  Pset_BeamCommon | properties | on 23 objects (23 IFCBEAM)
    LoadBearing = TRUE (IFCBOOLEAN)
    Status in {"NEW"} (IFCLABEL)
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Pset_MemberCommon | properties | on 1 object (1 IFCMEMBER)
    LoadBearing = TRUE (IFCBOOLEAN)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Qto_DoorBaseQuantities | quantities | on 1 object (1 IFCDOOR) | on 4 type objects
    Height = 6.6667 [foot (conversion based)]
    Width = 3. [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 type object
    Height = 6.6667 [foot (conversion based)]
    Width = 2.8333 [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 type object
    Height = 6.6667 [foot (conversion based)]
    Width = 8. [foot (conversion based)]
  Qto_DoorBaseQuantities | quantities | on 1 type object
    Height = 6.6667 [foot (conversion based)]
    Width = 5. [foot (conversion based)]
  EPset_Status | properties | on 281 objects (125 IFCWALL, 60 IFCDOOR, 36 IFCSLAB, 30 IFCWINDOW)
    Status in {"EXISTING"} (IFCLABEL)
  EPset_Status | properties | on 105 objects (45 IFCBEAM, 17 IFCWALL, 8 IFCSPACE, 6 IFCCOVERING)
    Status in {"NEW"} (IFCLABEL)
  EPset_Status | properties | on 20 objects (14 IFCBEAM, 3 IFCWALL, 2 IFCWINDOW, 1 IFCDOOR)
    Status in {"EXISTING", "DEMOLISH"} (IFCLABEL)
  Door-Single-Panel:30" x 80":154643 | predefined | on 6 type objects
  Door-Single-Panel:30" x 80":154643:1 | predefined | on 6 type objects
  Pset_DoorCommon | properties | on 7 type objects
    IsExternal = FALSE (IFCBOOLEAN)
    ThermalTransmittance = 2.1946486495 (IFCTHERMALTRANSMITTANCEMEASURE)
  Door-Single-Panel:34" x 80":154791 | predefined | on 2 type objects
  Door-Single-Panel:34" x 80":154791:1 | predefined | on 2 type objects
  Door-Single-Panel:34" x 84":154865 | predefined | on 2 type objects
  Door-Single-Panel:34" x 84":154865:1 | predefined | on 2 type objects
  Door-Single-Panel:36" x 80":154902 | predefined | on 2 type objects
  Door-Single-Panel:36" x 80":154902:1 | predefined | on 2 type objects
  Door-Single-Panel:36" x 84":154924 | predefined | on 4 type objects
  Door-Single-Panel:36" x 84":154924:1 | predefined | on 4 type objects
  Door-Single-Panel:32" x 84":154765 | predefined | on 3 type objects
  Door-Single-Panel:32" x 84":154765:1 | predefined | on 3 type objects
  Door-Single-Panel:30" x 84":154723 | predefined | on 7 type objects
  Door-Single-Panel:30" x 84":154723:1 | predefined | on 7 type objects
  Pset_ElementShading | properties | on 10 type objects
    Roughness = 1. (IFCPOSITIVELENGTHMEASURE) [foot (conversion based)]
  Pset_ProductRequirements | properties | on 10 type objects
    Category = "Walls" (IFCLABEL)
  BBIM_Roof | properties | on 1 type object
    Data = "{"roof_type": "HIP/GABLE ROOF", "generation_method": "ANGLE", "roof_thickness": 0.8333329688219886, "rafter_edge_angle": 1.5707963705062866, "angle": 0.3216641843318939, "path_data": {"edges": [[0, 1], [1, 2], [3, 0], [5, 3], [2, 4], [6, 5], [7, 6], [4, 7]], "verts": [[-16.87162208557129, -21.075729370117188, 0.0], [-16.87162208557129, 20.542932510375977, 0.0], [14.815959930419922, 20.542932510375977, 0.0], [14.16038703918457, -21.075729370117188, 0.0], [14.815959930419922, 1.7567006349563599, 0.0], [14.160385131835938, -16.52208137512207, 0.0], [27.410114288330078, -16.52208137512207, 0.0], [27.410114288330078, 1.7336031198501587, 0.0]], "gable_roof_angles": [0.0, 0.0, 0.0, 0.0, 0.0, 0.0, 1.5707963705062866, 0.0], "gable_roof_separate_verts": [0, 0, 0, 0, 0, 0, 0, 0]}}" (IFCTEXT)